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CPCCBC4006B 
Select, procure and store construction materials for low rise projects
ASSESSMENT SUMMARY

The assessment activities for CPCCBC4006B Select, procure and store construction materials for low rise projects cover all aspects of the unit of competency required. To demonstrate competence in this unit, a participant must undertake all tasks and complete them satisfactorily and consistently. For Apprentices and Trainees, this includes employer completion of the Employer Record Book (ERB). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be equitable, fair and flexible. If a participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a participant does not answer some questions or perform some tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. The Trainer/Assessor is able to provide the participant with additional information on interpreting the assessment outcomes and provide guidance on the participant’s options. Should a participant still be deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result. 

By signing the cover page for each assessment item, the participant acknowledges they understand the assessment instructions and requirements and consent to being assessed. The participant also verifies and assures the RTO that the work submitted is their own work. 


	Participant Name
	Emily Conlon




	Task
	Assessment Results 

	Theory Exam
	 Satisfactory 
	 Not Yet Satisfactory

	Practical Assessment
	 Satisfactory 
	 Not Yet Satisfactory

	Outcome for Unit of Competency
	 Competent
	 Not Yet Competent




	Assessor Name
	

	Assessor Signature
	
	Unit Competence Determination Date
	Click here to enter a date.
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	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances, whereby the Participant’s answers will be documented by a party other than the Participant. This must be acknowledged in writing (e.g. FT001 and Assessor Comments)
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· Assessors are to complete marking in pen of a different colour to the Participant.
· If a Participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a Participant changes their response in writing, they must put their initials next to the written change.
· If a Participant changes their response verbally, this must be noted on the exam paper by the assessor.




	Participant name
	Emily Conlon

	
	

	Participant signature
	
	
	

	Date
	23/09/2022



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.




	Number of questions
	Number of questions answered correctly
	Task outcome (Tick)

	44
	
	Satisfactory
	Not Yet Satisfactory

	
	
	
	


	ASSESSOR COMMENTS

	


Q1.  Which of the following documents and/or people would you refer to when selecting materials for a building project? Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
		Australian Standards
	

	
		Contract
	

	
		Drawings
	

	
		Manufacturer
	

	
		National Construction Code
	

	
		Specifications
	

	
		Tolerances
	




Q2.  [bookmark: _Ref427235149]Identify the Volume and Parts of the NCC that relate to suitability of materials for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	NCC 2019 VOL 2, SECTION 1 GOVERNING REQUIREMENTS
	NCC 2019 VOL 1, SECTION A GOVERNING REQUIREMENTS
	




Q3.  [bookmark: _Ref535482367]Identify the assessment methods used to verify a performance solution.

	Answer
	-Evidence of suitability 
- A verification method
- Expert judgement
- Comparison with the deemed to satisfy provisions 
	




Q4.  [bookmark: _Ref496611564][bookmark: _Ref536083431]Which of the following solutions for material selection often references the Australian Standards? Tick your response.

	Answer
	Choice
	Possible Answers
	

	
		Deemed-to-Satisfy solution
	

	
		Performance solution
	




Q5.  [bookmark: _Ref425255684]Identify five (5) materials commonly used for low rise buildings in your region. For each material, identify the following:
· Its name
· Properties of the material

	Answer
	#
	Material name
	Properties
	

	
	1
	Concrete 
	-Composite building material made from combination of aggregate
-Predominant building material in modern age due to longevity, formability and ease of transport
- Concrete has a rather low tensile strength, generally strengthened using steels rods and bars  
	

	
	2
	Metal
	-Steel – strong, flexible and if refined well lasts a long time
-Aluminium alloys and tine are a lower density/corrosive resistant
- Brass was common but it usually restricted today
- Chrome, gold and silver used as decoration  
	

	
	3
	Rock 
	-Longest lasting building material available
- usually readily available 
- very dense material so it provides a lot of protection
- It can be weighty and awkward to use
- energy density is also considered a big draw back; it is hard to keep warm
	

	
	4
	Wood 
	Product of trees, and sometimes other fiberous plants
-Different structures can be built in most climates
- very flexible under loads, keeping strength while bending
- strong when compressed vertically
	

	
	5
	Brick and Block 
	-Made of kiln-fired material, usually clay or shale
-flame retardant 
-cheaper to produce 
	





Q6.  [bookmark: _Ref425323073][bookmark: _Ref425248000]For each of the materials in Q5. identify the following:
· Quality of the material (i.e. durability, serviceability, cost effectiveness)
· Compatibility and non-compatibility of the material (i.e. what it would/would not be suitable for)

	Answer
	#
	Quality
	Compatibility 
	

	
	1
	The quality of concrete is affected by different physical and mechanical properties of aggregate e.g. shaping, grading, durability, specific gravity and water absorption. 
	Houses, driveways, columns. 
	

	
	2
	Strong, flexible and if refined well and or treated lasts a long time. 
	Structural framework for larger buildings such as sky scrapers, or as an external surface covering.  
	

	
	3
	Readily available, dense, weighty and hard to keep warm. 
	Facing work or buildings and retaining walls. 
	

	
	4
	Flexible, can be used in most climates, strong when compressed vertically.
	Used for timber, such as boards and plans and similar materials. 
	

	
	5
	Cheap to produce, flame retardant. 
	Used for exterior of houses. 
	



Q7.  [bookmark: _Ref536083435]Identify five (5) physical characteristics that may be considered when evaluating potential building materials.

	Answer
	-Strength 
-Electrical conductivity 
- Thermal conductivity and capacity 
- Moisture absorption
- Acoustics 
	





Q8.  [bookmark: _Ref536095924]Match the terms and definitions below by writing the appropriate letter next to each number in the centre column.

	Answer
	Term
	Answers
	Definition
	

	
	1
	Carbon footprint
	1 -B
	A
	The amount of energy required to manufacture a product
	

	
	2
	CO2e
	2 -E
	B
	Total GHD emissions produced during manufacture construction and use
	

	
	3
	Embodied energy
	3 -A
	C
	Greenhouse gas emissions
	

	
	4
	Embodied water
	4 -D
	D
	The amount of water required to manufacture a product
	

	
	5
	GHG
	5 -C
	E
	CO2equivalent tonnes emitted into the atmosphere
	




Q9.  [bookmark: _Ref536083463]Which of the following materials would be considered as ‘low energy content’? Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
		Bricks
	

	
		By-products of other industrial processes
	

	
		Cement
	

	
		Glass
	

	
		Metals
	

	
		Plastics
	

	
		Sand
	

	
		Stone
	

	
		Timber
	



Q10.  [bookmark: _Ref536099133]Refer to the table below and identify the wall material type that has the smallest embodied energy and emission impact.

[image: ]

	Answer
	Walls timber frame fibro clad
	





Q11.  [bookmark: _Ref536095926]Identify the Volume and Parts of the NCC that relate to energy efficiency of materials for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	VOL 2, SECTION 2 PERFORMANCE PROVISIONS 2.6 ENERGY EFFICENCY 
	VOL1, SECTION J ENERGY EFFICENCY 
	




Q12.  [bookmark: _Ref536097820]Identify the relevant section of the Standards and Tolerances Guide and the associated Australian Standard that addresses residential slabs and footings.

	Answer
	Standards and Tolerances Guide
	Australian Standard 
	

	
	QBCC, 2.3 Site Drainage 
	AS 2870
	




Q13.  [bookmark: _Ref536097822]Identify the relevant section of the Standards and Tolerances Guide and the associated Australian Standard that addresses roof tiles.

	Answer
	Standards and Tolerances Guide
	Australian Standard 
	

	
	QBCC, 7.4 Roof Tiles
	AS 2050
	




Q14.  [bookmark: _Ref536106144]Identify the Volume and Parts of the NCC that relate to safety barriers for swimming pools for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	VOL 2, PART 3.10.1, SWIMMING POOLS 
	VOL 1, PART 3.10.1 SWIMMING POOLS
	




Q15.  [bookmark: _Ref536106145]In some states, barriers and fences for swimming pools are not entirely regulated by the NCC, as noted in the Ancillary Provisions and State and Territory Variations. Identify the applicable Act and Regulation that regulate safety barriers for swimming pools in your jurisdiction.

	Answer
	BUILDING ACT 1975, SECT 231B 
	



Q16.  [bookmark: _Ref536106146]Identify the Australian Standard that relates to safety barriers for swimming pools.

	Answer
	AS 1926.1 - 2012
	




Q17.  [bookmark: _Ref536107455]True or False (Tick your response): According to the Standard in Q16. all gates must be fitted with a self-closing device that will return the gate to a closed position from any position without the use of manual force.

	Answer
		True 
	
	

	
		False 
	
	




Q18.  [bookmark: _Ref536170034]Identify the Volume and Parts of the NCC that relate to fire-resistance of building elements for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	VOLUME 3, SCHEDULE 5 FIRE-RESISTANCE FOR BUILDING ELEMENTS
	VOLUME 3, SCHEDULE 5 FIRE-RESISTANCE FOR BUILDING ELEMENTS
	




Q19.  [bookmark: _Ref536170036]Identify the Australian Standard that relates to fire-resistance tests for elements of construction.

	Answer
	AS 1530.4 - 2005
	




Q20.  [bookmark: _Ref536169328]For all NCC Classes, where the ground or subfloor space is excessively damp or subject to frequent flooding, which durability class must the subfloor framing must be used where above ground?

	Answer
	Where above ground – above ground durability class 1 or 2 timbers or H3 preservative treated timbers 
Where in ground – in ground durability class 1 or 2 timbers or H5 preservative treated timbers
	





Q21.  [bookmark: _Ref536170040]Identify the Australian Standards that must be observed when meeting the requirements for Q20. 

	Answer
	AS1684.2, AS 1684.3 or AS1684.4
	




Q22.  [bookmark: _Ref536170043]True or False (Tick your response): Where materials are not used as intended (or without considering NCC requirements), this can make a significant difference to the life or serviceability of the structure.

	Answer
		True 
	
	

	
		False 
	
	




Q23.  [bookmark: _Ref536170044]Explain why durability and serviceability impact on the cost effectiveness of chosen materials.

	Answer
	The Building Code sets minimum required levels of durability for different building elements, and this will be a primary driver for materials selection. Beyond this, durability and maintenance requirements should be considered together across the expected service life of the building. Some materials that do not appear to offer high levels of durability may actually perform well over many decades with the right maintenance. Timber weatherboards are a good example – where painted every 8–10 years, they can perform well for 60 years or more.
	




Q24.  [bookmark: _Ref536172033]Provide an example of short term degradation of materials and describe its effects on a building on structure.

	Answer
	Timber is often prone to short term degradation. When exposed to the weather it may suffer from weathering, causing splitting and crumbling or if it is unprotected and remains damp for long periods, it will rot. Some timbers are naturally resistant to rot, for example western red cedar. These timbers form a protective skin on the surface that keeps them relatively intact. 
	





Q25.  [bookmark: _Ref536172034]Provide an example of long term degradation of materials and describe its effects on a building on structure.

	Answer
	Stone usually forms a surface skin when exposed to the atmosphere. This can act to protect the stone or in some cases it may cause failure. The failure is usually associated with acid rain, a result of sulphur dioxide pollution in the atmosphere. 
	




Q26.  [bookmark: _Ref425327163][bookmark: _Ref425327708]You have spoken to a supplier who has indicated that some of the client’s desired materials are unavailable. When considering alternative building materials what must be taken into consideration (i.e. other than the client’s requirements)?

	Answer
	-Availability
- Transportation
- Handling 
- Testing
- Waste Reduction 
-Reuse/recycling
- Renewable non- renewable 
- Environmental impact 
-Embedded energy 
- Fire resistance rating 
- Compatibility 
- Acoustic properties 
- Life cycle cost 
- Short and long term degradation 

	




Q27.  [bookmark: _Ref536177031]Identify two (2) things that you should look for when receiving a delivery of materials.

	Answer
	1.Before the delivery person leaves and before you sign anything confirm the quantity is correct and confirm condition of the delivery.

	




Q28.  [bookmark: _Ref536177032]If you encounter issues with delivery, what two (2) options do you have?

	Answer
	1.Accept the shipment with ‘conditions’ or 
2. Reject the entire shipment 
	




Q29.  [bookmark: _Ref409518704][bookmark: _Ref408838393]Which of the following should be assessed before shifting materials? Tick all that apply. 

	Answer
	Choice
	Possible Answers
	

	
		What needs to be relocated (e.g. size, weight)
	

	
		The relocation area, site layout and obstacles
	

	
		Distance and time to relocate load
	

	
		Whether a team is available and/or appropriate
	

	
		Whether PPE must be worn (e.g. for hazardous materials)
	




Q30.  [bookmark: _Ref536178585]What document should you refer to for guidance on how to handle and store hazardous chemicals? 

	Answer
	Safety Data Sheet 
	




Q31.  [bookmark: _Ref408838395][bookmark: _Ref409519364]Name three (3) ways you can reduce the risk of injury if a load is too heavy for one person to carry, push or pull. 

	Answer
	-Ensure pathway is clear and no trip hazards are in the way
- take breaks from repetitious tasks
- ensure no jerky movements when lifting, carrying, pulling or pushing an object 
	





Q32.  [bookmark: _Ref401922320]In the diagram below a person is lifting a tool box.
Filling in the table, indicate how each body part should be used/placed. 
[image: lifting]F. Hands
E. Knees
D. Shoulders
C. Feet
B. Back
A. Neck

	Answer
	Area of body (Letter)
	How it should be placed
	

	
	D
	Level
	

	
	A
	Upright
	

	
	F
	Good grip
	

	
	B
	Natural curve
	

	
	E
	Bent
	

	
	C
	Flat, facing load
	




Q33.  [bookmark: _Ref404158235]How should construction materials and components be handled? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
		Sorted to suit material type and size, separating hazardous material
	

	
		Stacked or stockpiled for ease of identification and retrieval
	

	
		Stored in access ways for ease of retrieval
	

	
		Stored clear of access ways
	

	
		Handled and positioned ready for installation
	




Q34.  [bookmark: _Ref536180244]Identify the Australian Standard that relates to the storage and handling of LP gas.

	Answer
	AS / NZS 1596
	



Q35.  [bookmark: _Ref536194481]List one (1) testing method for each of the building materials listed below.

	Answer
	Material name
	Properties
	

	
	Concrete
	Hydraulic Press 
	

	
	Metals
	Ductility is tested by bending a bar around a pin over a wide angle. 
	

	
	Timber
	When timber is used in domestic construction where it is not highly stressed, a visual grading may be a sufficient means of testing the material.
	




Q36.  [bookmark: _Ref536181364]What Code gives detailed tables which state the required grade of timber for specific sizes and uses?

	Answer
	The Australian Timber Framing Code 
	




Q37.  [bookmark: _Ref536181366]Name two (2) ways that defects may be seen in timber.

	Answer
	Knots, splits, gum veins, pockets or resin and insect damage. 
	




Q38.  [bookmark: _Ref536181368]Identify two (2) tests that may be performed to determine the durability of stone.

	Answer
	Standard tests include acid immersion 
	



Q39.  [bookmark: _Ref536181370]Name two (2) ways that defects may be seen in stone.

	Answer
	Cracks and fissures in the rock surface. 
	




Q40.  [bookmark: _Ref536187863]True or False (Tick your response): Under a contract, builders and other specialist tradespersons are the ones most likely to rectify or remedy problems that arise from incorrect installation, application or placement of materials.

	Answer
		True 
	
	

	
		False 
	
	




Q41.  [bookmark: _Ref536187427]Name two (2) established methods that may be used to preserve timber.

	Answer
	Mechanical protection and soil poisoning. 
	




Q42.  [bookmark: _Ref536187429]Identify two (2) established methods that may be used to protect ferrous metals.

	Answer
	Cathodic protection and corrosion inhibitors. 
	





Q43.  [bookmark: _Ref536187430]Explain why the corrosion resistance of non-ferrous metals is superior to that of ordinary steel.

	Answer
	This is a result of the production of a ceramic coating of oxide or salt on the metal which protects it from further corrosion. 
	




Q44.  [bookmark: _Ref536187432]When should aluminium be coated with bituminous paint? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
		At all times
	

	
		When it is buried in soil
	

	
		When it comes in contact with chemical materials
	

	
		When it is immersed in water
	

	
		When it is used on bitumen
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	PRACTICAL ASSESSMENT INSTRUCTIONS

· The following practical assessment will require the Participant to complete work related activities.
· The Assessor will conduct observations of the Participant’s work to determine whether they display sufficient practical skills and knowledge. 
· Please fill in the details below – providing your name, signature and date of assessment.
· The Participant’s signature acknowledges that the Assessor provided clear instructions and the Participant understood what was required to complete this assessment.
· The Assessor may substitute a Practical Task with an alternate task of equal value.
· Alternate tasks must be fully documented by the assessor in the Assessor Comments area.





	Participant name
	Emily Conlon

	
	

	Participant signature
	
	
	

	Date
	23/09/2022



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.





	Task
	Task outcome (Tick)

	
	Satisfactory
	Not Yet Satisfactory

	Task 1 (Occasion 1)
		
	Task 1 (Occasion 2)
		



	ASSESSOR COMMENTS

	


CPCCBC4006B
Select, procure and store construction materials for low rise projects

	Practical Task 1 (2X)

	Description of task:
On two (2) occasions, a suitable observer is to verify the participant’s ability to supervise systems through which materials are selected, acquired and stored on site for the following projects:
· Occasion 1: Construction classified as Class 1 and 10 construction
· Occasion 2: Construction classified in Classes 2 to 9 with a gross floor area not exceeding 2000 square metres, not including Type A or Type B construction

The participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. Evidence to be submitted may include: 
· Copy of PO sent to site team for materials.
· Email correspondence sighting need for materials, delivery of materials and storage of materials (if relevant).

The observer is to provide detailed comments on the tasks completed by the participant. The assessor is to verify the observer’s comments in the Assessor Comments section, and provide the Practical Assessment outcome on the front cover of this document.

	Resources required: 
Computer, Building Contract, Drawings, Specifications, Building materials (including timber, and ferrous and non-ferrous metal).

	Assessment of task

	Name of participant:
	Emily Conlon

	Name of observer:
	Amy Cowling 

	Role of observer 
(Confirm suitability to sign)
	Project Administrator Team Manager 

	Email address of observer
	Amy.cowling@seecivil.com.au

	Signature of observer:
	
	Date:
	23/09/2022

	When completing the task, did the participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	
	1st
Occasion
	2nd
Occasion

	1 Evaluate building materials

	1.1A.  [bookmark: _Ref535842396]Identify suitability of materials commonly used in the region for low rise buildings. 
	
	

	1.1B.  [bookmark: _Ref535842402][bookmark: _Ref536020766]Through research and testing, identify properties of different materials, their quality and compatibility and non-compatibility and maintain effective sampling and organisational record-keeping processes.
	
	

	1.1C.  [bookmark: _Ref535842408]Identify the environmental impacts of different materials. 
	
	

	1.1D.  [bookmark: _Ref535842411]Identify the impact of allowable tolerances on the conversion of naturally occurring materials. 
	
	

	1.1E.  [bookmark: _Ref535842424]Identify and check tolerances for installing and assembling materials with regard to the nature of the work being performed and the requirements of relevant construction industry Australian standards. 
	
	

	2 Material selection 

	1.2A.  [bookmark: _Ref535842432]Select materials structurally adequate and appropriate for the building system specified in the contract, drawings and specifications. 
	
	

	1.2B.  [bookmark: _Ref535842436]Select materials after considering:
· Safety
· Required fire resistance rating
· Suitability to the application
· Durability
· Serviceability and cost effectiveness
· Compliance with NCC, legislation, regulations and Australian Standards
	
	

	1.2C.  [bookmark: _Ref535842439]Consider short and long-term degradation of materials in relation to the building’s proposed life cycle. 
	
	

	1.2D.  [bookmark: _Ref535842441][bookmark: _Ref536188601]Select and evaluate alternative materials, if specified materials were unavailable or unsuitable – justifying decisions to regulatory authorities, as necessary
	
	

	1.2E.  [bookmark: _Ref535842446]Finalise selection of materials in accordance with contractual requirements and in consultation with relevant professionals and the client, compiling results in a report.
	
	

	1.2F.  [bookmark: _Ref535842459]Effectively communicate using the following methods:
· Language/concepts appropriate to cultural differences
· Non-verbal communication
	
	

	3 Supervising materials on site 

	1.3A.  [bookmark: _Ref535842490]Determine limitations and effects of transportation on material and components, taking action in potentially damaging circumstances. 
	
	

	1.3B.  [bookmark: _Ref535842494]Ensure materials were correctly and safely handled on site using appropriate equipment and safe work practices. 
	
	

	1.3C.  [bookmark: _Ref535842471]Communicate with manufacturers and suppliers to ensure materials are stored in accordance with specifications and Australian standards. 
	
	

	1.3D.  [bookmark: _Ref535842501]Implement processes for inspecting all materials delivered on site for naturally occurring and/or manufactured defects before installation. 
	
	

	1.3E.  [bookmark: _Ref535842506]Ensure personnel were aware of actions to be taken in the case of defects caused by incorrect installation, application or placement. 
	
	

	1.3F.  [bookmark: _Ref535842510]Preserve and protect timber and ferrous and non-ferrous metal used in the construction process.
	
	

	The Participant’s performance was:  Satisfactory     Not Satisfactory





	OBSERVER COMMENTS

	Emily was competent in all tasks observed. 
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