
CONTRACT SUPPORTING DOCUMENTS - STRICTLY CONFIDENTIAL AND USED STRICTLY FOR THIS COURSE STUDY ONLY 


RESIDENTIAL PROJECT - 123 ABC Residential street, QLD
There are various supporting documents that are attached to and form part and parcel of the Contract for RESIDENTIAL BUILD/RENOVATE – KITCHEN, PANTRY AND LAUNDRY


EQUIPMENT INFORMATION

	MAKE/MODEL
	DESCRIPTION
	OWNED/LEASED

	Jack Hammer
	For demolition
	Leased



Contractor and Subcontractor tools brought in their own.

SITE ACCOMODATION INFORMATION

Contractors establishment and office workshop facility, as required - The Contractor shall provide and maintain an established office workshop facility. The facility shall include the following: 
· An approved workshop with equipment and capabilities sufficient to carry out work as requested under the Contract. 
· An approved office space with sufficient personnel necessary to take, record or pass on any emergency message that may be received, provide day to day information with regard to prices availability and delivery. Be sufficiently qualified to process and forward invoices for work carried out. 
· Storage facilities
· Parking areas

SERVICES INFORMATION

Facilities such as water, lighting, communication, toilet and security will be supplied on site.
Site temporary works - Temporary works: Provide and maintain required barricades, guards, fencing, shoring, temporary roadways, footpaths, signs, lighting, watching and traffic flagging. 
Site Accessways, services: Do not obstruct or damage roadways and footpaths, drains and watercourses and other existing services in use on or adjacent to the site. Determine the location of such services. 
Site and Property: Do not interfere with or damage property which is to remain on or adjacent to the site, including adjoining property encroaching onto the site, and trees. 
OCCUPATIONAL HEALTH AND SAFETY
The Contractor shall: 
(a)  Comply with all requirements of the contract and all statutory requirements for Occupational Health and Safety. 
(b)  Ensure that each of its Subcontractors and Workers comply in like manner. 
(c)  Demonstrate to the Client whenever requested that requirements of the contract and statutory requirements for Occupational Health and Safety are being met. 

Safety requirements of the works undertaken in the contract and statutory requirements for Occupational Health and Safety are capable of being met. 
Where inappropriate or inadequate provision of Occupational Health and Safety Management by the Contractor or Contractor’s subcontractor results in costs, losses or damages incurred by the clients or claims by third parties against the client for either direct or consequential costs, losses or damages, the Contractor shall be liable for costs, losses or damages associated with any claim including but not limited to administration and legal costs incurred by the Client in resolving such claim. 
PROTECTION OF THE ENVIRONMENT
The Contractor shall; 
a)  Comply with all statutory requirements and accepted current practices for 
Environmental management. 
b)  Comply in every respect with the Erosion and Sedimentation Plan pertaining 
to this contract. 
c)  Ensure that each of its subcontractors and Workers comply in like manner. 
All work shall be carried out in such a manner as to avoid nuisance and/or damage to the environment. The Contractor shall comply with the requirements of the conditions of approval imposed by the Local Government Act, Environmental Offences and Penalties Act and the Water Act. No variation in costs or extensions of time will be considered due to these requirements. 

The Contractor shall plan and carry out the Works to avoid erosion, contamination and sedimentation of the site and its surroundings. 

Herbicides and other toxic chemicals shall not be used on the site without the prior written approval of the Client. 

No noise or smoke or other nuisance, which in the opinion of the Client is unnecessary or excessive shall be permitted by the Contractor in the performance of the works under this Contract. Should work outside customary working hours be approved, the Contractor shall not use, during such period, any plant, machinery or equipment which in the opinion of the Client is causing or is likely to cause a nuisance to the public. No noisy works and/or works likely to disturb nearby residents shall be undertaken during the hours precluding such activity as specified by Council in accordance with the requirements for development consent and building approval made under the Local Government Act and appropriate Noise Legislation. 

The Contractor shall ensure that fugitive dust from disturbed areas is minimised by a method approved by the Client. 
PUBLIC SAFETY AND TRAFFIC CONTROL
The Contractor shall provide Traffic Management Plans and erect all necessary fences, barricades, warning lights as may be necessary for the protection of the works and the safety of the public and vehicles all to conform to Australian Standard AS 1742.3 - 1996. Road notices, speed restriction signs, flagman etc., shall be provided and maintained to the satisfaction of the relevant Traffic Authority. 

If the Contractor fails after notification in writing to carry out the requirements of this clause, the Superintendent shall have the power to have the work carried out at the Contractor's expense. The cost thereof will be deducted from any moneys owing to the Contractor under this Contract. 

HUMAN RESOURCE PROJECTIONS
· Human resource projection helps the company plan and find the people they need and measure its working capacity to meet its goals. Human resource projections allow parties involved to know the essential human resource required for the project and anticipate the needed manpower for projects tasks. Human resources projection assists the company to know the problems, solutions, and plans for the shifting phases of its human resources
· The Contractor shall be suitably qualification to carry out the work as detailed in the Specification. The Contractors and sub-contractors must have a suitable qualification and license if required, to carry out the sub- contracted work. 
· CONTRACTOR’S RESPONSIBILITY - It shall be the responsibility of the Contractor to ascertain all information relating to the services, the works and site conditions that may affect the progress or method of performing all services and works as specified within the scope of this contract and to prepare for every contingency that may arise. It is further understood that just provision for these contingencies have been accounted for, implicitly or explicitly within the Residential contract lump sum price submitted. 
· The contractor shall employ Sufficient qualified personnel employed to carry out the work as detailed elsewhere in this Specification. Due to the nature and anticipated workload of this Contract, it is envisaged that the successful Contractor shall be operating a business which employs at the least, a staff of two (2) tradesmen working from a fully equipped workshop and vehicles. 
· Contractors for the work covered by this Specification must be experienced in the type of work specified.
· All repairs, maintenance and new work shall be carried out by personnel having relative trade qualifications and experience. 
· It is the Contractors responsibility to ensure that all work performed under this Contract is adequately supervised by a qualified and experienced member of the Contractor’s staff and to the approval of the Superintendent. 
· All work shall be completed in accordance with all the latest editions of relevant or listed Australian Standards (defined hereafter as Standards) and Codes of Practice and conforming to all requirements of the Building Code of Australia (BCA). 
· The contractor shall clean the site to its original condition including reinstatements of all surfaces on completion of works. 
· Program of work - Sequence of work to include:
· Allowance for holidays. 
· Activity inter-relationships. 
· External dependencies including provision of access, document approvals and work by others. 
· Periods within which various stages or parts of the work are to be executed. 
· Time scale: Working days. 
· Updated program: Identify changes since the previous version and show the estimated percentage of completion for each item of work. 
· Completion of the works includes:
· Final cleaning and before practical completion, clean throughout, including interior and exterior surfaces exposed to view. Vacuum carpeted and soft surfaces. Clean debris from the site, roofs, gutters, downpipes and drainage systems. Remove waste and surplus materials
· Reinstatement - Before practical completion, clean and repair damage caused by installation or use of temporary work and restore existing facilities used during construction to original condition. 
· Removal of plant - Within 10 working days after practical completion, remove temporary works and construction plant no longer required. Remove the balance before the end of the defects liability period. 
· The personnel are:
· CONTRACTOR – FAO 
Qualifications – Diploma in Building and Construction and Building Licence
· KEY PERSONNEL 
· Name FA
Company role Site supervisor
Years of experience 10
Qualifications Dip in Bldg
· Name SB
Company role Leading Hand
Years of experience 8
Qualifications Dip in Bldg


	Relevant construction works/services
	Description/scope
	Hrs
	Unit price
	Total price

	Demolition labour
	Demolish existing kitchen and make good
Dismantling the existing storage, slab platform including supporting walls, wall tiles, flooring, sink etc. at all levels as required carefully and disposing off and clearing away the debris
Slabs to be chased to allow for new plumbing


	16
	$425
	$6800

	Kitchen Labour
	Installation of supply mentioned above
	138.4
	$60
	$8305

	Butlers Pantry Labour
	Installation of supply mentioned above
	35
	$50
	$1745

	Laundry Labour
	Installation of supply mentioned above
	40
	$50
	$2000

	Plumbing
	Installation of supply mentioned above
Slabs to be chased to allow for new plumbing
Plumbing cap off and reconnections
Plumbing dis-connections to existing serviceable connection points and connections
Water dis-connection and connections from pre-tapped water main

	33.3
	$75
	$2500

	Electrical
	Installation of supply mentioned above
Electricity cap off and reconnections
Electricity dis-connections to existing serviceable connection points and connections
Duct work for bench mount exhaust to run through back of drawers and wall to external wall and motor
Cooktop downdraft ventilation system
	29
	$110
	$3200

	Building / Carpentry Labour
	Labour for scopes of work described excluding the installation of above fixtures
New stud plasterboard wall to be build
New fixed glass window to existing opening
Enclose wall above and below to match existing 
Window tint to be discussed with client
New doors to match switch opening with screens
New doors to match triple slider with screens
New Laundry door location cavity slider to match existing
Tambour door in kitchen
New Laundry window to suit existing opening width over dishwasher

	230
	$65
	$15000

	Tiling Labour
	Installation of supply mentioned above
	122
	$65
	$7930

	Butlers Pantry - Fixed Glass Window Labour
	Installation of supply mentioned above
	2
	$80
	$160

	French Doors - Triple Slider Labour
	Installation of supply mentioned above
	3
	$80
	$240

	Dining Room Slider - Reverse Opening Labour
	Installation of supply mentioned above
	5
	$80
	$400

	Removal of Debris
	Labour and clean-up
	8
	$75
	$600

	TOTAL ESTIMATED COST OF CONSTRUCTION WORKS/SERVICES
	$48880




	CONTRACTOR/SUPPLIER
	CONTACT DETAILS
	DESCRIPTION OF WORKS/MATERIALS

	Builder
	0123
	As per contract

	Carpenter
	1456
	As per contract

	Electrician
	0789
	As per contract

	Plumber
	0456
	As per contract

	Tiler
	1234
	As per contract



MATERIALS LISTS
· The Contractor shall provide all general and specialised equipment, tools and materials to carry out and test the Work. It shall be the responsibility of the Contractor to be fully equipped on each attendance call. 
· The Contractor is expected to locate his own source of supply of the materials required to carry out any work under this Contract and should make satisfactory arrangements for such to be available. 
· All materials, unless otherwise specified by the Superintendent, are to be new and of the highest quality and installed in accordance with the manufacturer’s specifications and industry best practice. 



	Material
	Description
	Measurement of material 
	Unit price
	Total price

	Demolition – Jack Hammer
	Demolish the 17 sqm of existing storage, supporting walls, wall tiles, flooring, sink etc. at all levels as required carefully and disposing off and clearing away the debris 
	sqm
	$310
	$5270

	Kitchen 
Elevation
Bench
Drawers
Spice rack
Brushed stainless steel laminate
Ducting
Overheads
Shelves
Caesarstone bench top
Island
Sink cupboard
Paint
Cabinetry - Blum Tandembox antaro h. Fronted pull-out C - DQC5JY, D - DQC69A, DQCB6M
Urbane Castella 192mmCTC handle

	Kitchen elevation 2730x2550Hx600mm diameter or expressed as 2.7mx2.55mx0.6m
Bench height 1000mm with 3 sets of 3 blum tip drawers with 1 of orga line spice rack insert
Brushed stainless steel laminate kick face
Ducting for downdraft cooktop to run behind draws
Overheads 650mm Height with 1 of adjustable shelf with doors hanging below as finger pull and LED strip lighting to underside
Internal 16mm HMR with 1mm ABS PVC match edge
Fronts in 18mm white sating with 2 pac satin finish
40mm Caesarstone bianco drift bench top with cutout for drop in cooktop
Kitchen island 3000x1000Wx1000 D – LH side with pull out drawer with 2x35L bin inserts
Sink cupboard with 1 door housing undermount single bowl sink with 3 sets of 4 blum tip on drawers with 1 of cutlery insert and 2 of utensil insert. Internals 16mmwh HMR with 1mm ABS PVC matching edge. All fronts in 18mm wh sat with 2pac satin finish

	mm, m
L
W, H, D, thickness, pieces
	


$4500
$2500
$500
$2600

$9850
$3345
$1000

$12400
	$36695

	Butlers Pantry
Door sink cupbard
Bins
Dishwasher
Drawers
Shelves
Overheads
Paint
	4480x2550 Hx620mm D pantry or expressed as 4.48m x 2.550m x 0.620m with door sink cupboard and 2x20L bins
Dishwasher opening 600mm
3 sets of 3 blum tip on drawers with 885mm pantyr to RH side
2 door pantry unit with 5 blum soft close internal drawers and 4 adj shelves
Overheads 3595x650 Hx400mm D with 1 adj shelf with doors hanging below as finger pull
	Mm, m
L
W, H, D, thickness, pieces

	$4500

$2320
$2500

$2430

$4505
	$‎16255

	Laundry
Laundry tub unit
Shelves
Bench
Caesartone top 6131 Bianco Drift, 4600 Organic white
Shute cupboard
Overheads
Drawers
Tall cupboard
Brushed SS laminate
Single door cupboard
Paint
	L shaped laundry 2450x2520x2550mm or expressed as 2.45m x 2.52m x 2.55m with 4 door laundry tub unit with 1 adj shelf with bench at 1000mm H
40mm Caesarstone organic white top running wall to wall below laundry shute cupboard and 20mm thick splashback 150mm height
4 door overhead cupboard with 2 adj shelves and dorrs hanging down as finger pull above dryer and washing machine openings with flat pull out shelves and 1 of blum soft close drawer below
2 door Tall broom storage cupboard to right side with 1 of blum soft close drawer below 1 0f internal adj shelf
Brushed stainless steel laminate kick face
Single door cupboard 600x600mm on opposite wall 1000mm height bench top.
All internals 16mm white HMR with 1mm ABS PVCedge.  All fronts in 18mm white sating with 2 pac satin finish
Dryer and washing machine panels, bottoms in 32mm MDF with 2pac finish
	mm, L, m
W, H, D, thickness, pieces
	$1000


$2950



$3200



$1900


$990


$2960
	$‎13000

	Plumbing
Franke Ancona single bowl undermount sink
Double bowl undermount sink
Mizu drift sink mixer
Mizu smothe sq sink mixer
	Island & laundry - franke ancona single bowl undermount sink – anx 110-48
Pantry - franke ancona double bowl undermount sink - anx 120
Island & pantry - mizu drift mk2 gooseneck sink mixer pull-out
Laundry - mizu soothe square gooseneck sink mixer

	 4 pcs
	$900


$1650

$1400

$2300
	$6250

	Electrical
Light
LED tape
	Beacon Herman 1 light pendant
14 watt led tape and recess led profile under overhead cupboards
Single phase underground power connection from existing supply point. 
Led light strip under island bench
Cooktop isolation switch

	2 pcs
	$1900

$1150
	$3050

	Tiling
Timber look tile flooring
Ceramic tile splashback – kitchen and laundry
Kitchen timber look tile to match floors
Brushed stainless steel laminate

	New timber look tile flooring 
Kitchen – timber look tiles to match floors 1200x x230mm
Laundry and kitchen - ceramic tile splashback - Snow Brillo Tile Sc19 A7615, Amber Tiles To Match Cabinets. 130mmx130mm
Brushed stainless steel laminate kick face
130 sqm 
	Sqm, mm
	$69
	$8970

	Butlers Pantry - Fixed Glass Window
	New fixed glass window to suit existing opening width frame
1800x600mm
Colour to match exiting and tinted to client requirement (customized)

	1 pcs, mm
	$1790
	$1790

	French Doors - Triple Slider
	New Triple Slider With Screens To Match Existing Profile & Colour
2710x2100mm

	1 pc, mm
	$4800
	$4800

	Dining Room Slider - Reverse Opening
	Slider with reversed opening with screen to match existing profile and colour
1810mmx2100mm
	1 pc, mm
	$2850
	$2850

	Removal of Debris
Cleaning material
Skip bin

	Cleaning materials

Skip bins
	1 pc

2 pcs
	$500

$1400
	$1900

	TOTAL  ESTIMATED COST OF MATERIAL /SUPPLY
	$100830



CONSTRUCTION DRAWINGS
As attached in the folder ‘Residential plans’
CONSTRUCTION SPECIFICATIONS

FINISHES
	2P01
	SATIN 2Pac MDF DULUX ROTTNEST ISLAND SW1B6

	CT01
	SPLASHBACK - SNOW BRILLO TILE SC19 A7615, AMBER TILES OR COLOUR BACK GLASS TO MATCH CABINETS.

	ST01
	STONE TOP - CAESARSTONE 6131 BIANCO DRIFT

	ST02
	STONE TOP - CAESARSTONE 4600 ORGANIC WHITE

	BS01
	BRUSHED STAINLESS STEEL LAMINATE

	T01
	TBA TO MATCH FLOORS - CLIENT TO SELECT




APPLIANCES
	FRIDGE
	CLIENT TO SUPPLY

	OVEN
	CLIENT TO SUPPLY

	MICROWAVE / OVEN
	CLIENT TO SUPPLY

	COOKTOP
	CLIENT TO SUPPLY

	DISHWASHER
	CLIENT TO SUPPLY

	DRYER
	CLIENT TO SUPPLY

	WASHING MACHINE
	CLIENT TO SUPPLY




CABINETRY
	TYPE 1
	BLUM TANDEMBOX ANTARO DRAWER M - DQC2QM

	TYPE 2
	BLUM TANDEMBOX ANTARO H. FRONTED PULL-OUT C - DQC5JY

	TYPE 3
	BLUM TANDEMBOX ANTARO H. FRONTED PULL-OUT D - DQC69A

	TYPE 4
	BLUM TANDEMBOX ANTARO INNER PULL-OUT C - DQCAHA

	TYPE 5
	BLUM TANDEMBOX ANTARO INNER PULL-OUT D - DQCB6M

	BIN KIT.
	TOP MOUNTED CR235D HIDEAWAY BIN, 2x35L

	BIN PAN.
	BASE MOUNTED KCF220SCH HIDEAWAY BIN, 2x20L

	HANDLE
	URBANE CASTELLA 192mmCTC

	
	WHERE POSSIBLE DRAWERS AND DOORS TO BE HANDLESS OR PLUM TIP-ON FUNCTION



PLUMBING
ISLAND & LAUNDRY - FRANKE ANCONA SINGLE BOWL UNDERMOUNT SINK – ANX 110-48
PANTRY - FRANKE ANCONA DOUBLE BOWL UNDERMOUNT SINK - ANX 120
ISLAND & PANTRY - MIZU DRIFT MK2 GOOSENECK SINK MIXER PULL-OUT
LAUNDRY - MIZU SOOTHE SQUARE GOOSENECK SINK MIXER

ELECTRICAL
	D1
	CONTRACTOR TO SELECT WITH CLIENT

	P1
	BEACON HERMAN 1 LIGHT PENDANT

	LED
	14 WATT LED TAPE + RECESS LED PROFILE




DO0RS AND WINDOWS
	D1
	NEW TRIPLE SLIDER WITH SCREENS TO MATCH EXISTING PROFILE & COLOUR

	D2
	NEW SLIDER WITH REVERSED OPENING WITH SCREEN TO MATCH EXISTING PROFILE & COLOUR

	D3
	NEW CAVITY SLIDER TO MATCH EXISTING DOORS AND HARDWARE

	W1
	NEW FIXED GLASS WINDOW TO SUIT EXISTING OPENING WIDTH FRAME
COLOUR TO MATCH EXITING
TINTING TO BE DISCUSSED WITH CLIENT




PROJECT TIMELINES
1. Kick-off meeting for Residential Project 1/3/23
2. Possession of site date 5/3/23 
3. Start date 5/3/23
4. Plumbing Rough In 7/3/23
5. Electrical Rough In 7/3/23
6. Building works – wet areas, walls, ceiling, doors/windows 10/3/23
7. Plaster works  and finish 17/3/23
8. Water proofing 19/3/23
9. Cabinets installation, skirting/architraves installation, benchtop , kitchen, laundry, pantry installation 28/3/23
10. Tiling 28/4/23
11. Electrical Fit-Off 1/5/23
12. Plumbing Fit-Off 1/5/23
13. Accessories Fit-Off 3/5/23
14. Caulking 3/5/23
15. Screen installation 4/5/23
16. Practical completion date 5/5/23
17. Completion: Prior to Practical Completion, submit a detailed schedule of defects and incomplete work to the Superintendent indicating that each item has been corrected or completed to the satisfaction of the Contractor. 
18. Collect the section 40 Certificates of Compliance from the subcontractors and the Final Inspection Certificate from the Building Certifier. Submit these with the Builder’s Declaration prior to Practical Completion. Practical Completion is contingent upon receipt of the Building Certifier’s Occupancy Permit. 


SCHEDULES

SCHEDULE – refer to contract as attached - This will consist of the following details:
1. Owner Name/details
2. Contractor Name/details
3. Architect Name/details
4. Any special conditions
5. Will the owner remain in occupation
6. Contract price
7. Scope of works
8. Site of works
9. Any security required
10. Any % of contract price indications
11. Period of payment of certificates
12. Public Liability Insurance and amounts and excess
13. Contract works insurance and amounts and excess
14. Any cover fees (%) for architect or other consultants
15. Profit margin
16. Allowance for delay due to disruptive weather conditions
17. Date of practical completion
18. Commissioning tests for practical completion
19. Defects liability period for the works
20. Date of submitting progress claims
21. Interest rate on overdue amounts
22. Any official documents to be obtained by the contractor
23. Any official documents to be obtained by the Owner/Client

INSURANCE

WORKERS COMPENSATION
POLICY NUMBER - 456
NAME OF INSURER - DEF
DATE OF EXPIRY – 1/1/2025

PUBLIC LIABILITY AND WARRANTY INSURANCE – 10M
POLICY NUMBER - 789
NAME OF INSURER -GHI
DATE OF EXPIRY – 1/1/2025
PREMIUM PAYABLE: $6000

Signed: NAO
Date:15/1/2023
For: Knights CBI
Position Held: Estimator/Contract administrator/Project Manager


