Quality Assurance required throughout the project build 
Pre-pour checklists
· Engineer inspected including any adjustments
· Plumber signed off
· Electrician signed off
· Mechanical signed off (if required for tundishes etc.)
· Current drawings issued
· Formwork signed off
· Formwork/falsework checked
· RPEQ formwork inspection
· Penetrations formed and meshed
· Edge protection in place (if required for suspended slabs)
· Deck cleaned down (if required for suspended slabs)
· REO signed off by contractor
· Check segregation of services (if required in risers etc.)
· Check construction joints
· Test ordered (compaction cylinders)
· Access for concrete and labour
· Confirm slab RL
· Curing complete using approved method
· Surface inspection at completion of pour
· Instructions issued for non-compliance (if required)
Pre-sheet
· Trades roughed in
· Electrical
· Mechanical
· Fire
· Plumber
· Plumbing inspection complete
· Variations captured
· Noggins captured
· Tv
· Dryer
· Towel rails
· Toilet roll holder
· Mirror
· Shower screen
· Acoustic zones complete (if required)
· Fire party walls correct (if installed)
· Check access hatches
· Correct location
· Correct hatch for sound/fire rating
· Check any ductwork and ventilation installed correctly
· All tundish and AC wastes lines installed correctly with appropriate fall
· Visual check of frames
· Button head screws behind gyprock
· Straight and plumb
· Screws through services
· Ceiling correct height for downlights
· Previous trades cleaned up
· Windows fitted and sealed
· Fire collars and penetrations sticker certified (if required)
Engineers Inspections
· Slabs
· Compaction tests checked and correct compaction achieved after 28 days
· Slab thickness correct as per drawings
· Garage and wet area set downs achieved as per the NCC
· Frame & tie down
· Frames installed as per structural drawings
· Tie downs achieved as per NCC
Occupation certificate of classification inspection by certifier
· [bookmark: _GoBack]Final check and signoff by certifier to ensure all items installed to NCC standards
