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CPCCBC4006B 
Select, procure and store construction materials for low rise projects
ASSESSMENT SUMMARY

The assessment activities for CPCCBC4006B Select, procure and store construction materials for low rise projects cover all aspects of the unit of competency required. To demonstrate competence in this unit, a participant must undertake all tasks and complete them satisfactorily and consistently. For Apprentices and Trainees, this includes employer completion of the Employer Record Book (ERB). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be equitable, fair and flexible. If a participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a participant does not answer some questions or perform some tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. The Trainer/Assessor is able to provide the participant with additional information on interpreting the assessment outcomes and provide guidance on the participant’s options. Should a participant still be deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result. 

By signing the cover page for each assessment item, the participant acknowledges they understand the assessment instructions and requirements and consent to being assessed. The participant also verifies and assures the RTO that the work submitted is their own work. 


	Participant Name
	Rachel Redpath




	Task
	Assessment Results 

	Theory Exam
	 Satisfactory 
	 Not Yet Satisfactory

	Practical Assessment
	 Satisfactory 
	 Not Yet Satisfactory

	Outcome for Unit of Competency
	 Competent
	 Not Yet Competent




	Assessor Name
	

	Assessor Signature
	
	Unit Competence Determination Date
	Click here to enter a date.
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	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances, whereby the Participant’s answers will be documented by a party other than the Participant. This must be acknowledged in writing (e.g. FT001 and Assessor Comments)
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· Assessors are to complete marking in pen of a different colour to the Participant.
· If a Participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a Participant changes their response in writing, they must put their initials next to the written change.
· If a Participant changes their response verbally, this must be noted on the exam paper by the assessor.




	Participant name
	Rachel Redpath

	
	

	Participant signature
	
	
	

	Date
	18/03/2021



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.




	Number of questions
	Number of questions answered correctly
	Task outcome (Tick)

	44
	
	Satisfactory
	Not Yet Satisfactory

	
	
	
	


	ASSESSOR COMMENTS

	


Q1.  Which of the following documents and/or people would you refer to when selecting materials for a building project? Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
		Australian Standards
	

	
		Contract
	

	
		Drawings
	

	
		Manufacturer
	

	
		National Construction Code
	

	
		Specifications
	

	
		Tolerances
	




Q2.  [bookmark: _Ref427235149]Identify the Volume and Parts of the NCC that relate to suitability of materials for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	Volume 2 - Section 1 Part A5 1 - 3
	Volume 1 - Section B Park B1
	




Q3.  [bookmark: _Ref535482367]Identify the assessment methods used to verify a performance solution.

	Answer
	· Evidence of suitability
· A verification method
· Expert judgement
· Comparison with the Deemed-to-Satisfy provisions

	




Q4.  [bookmark: _Ref496611564][bookmark: _Ref536083431]Which of the following solutions for material selection often references the Australian Standards? Tick your response.

	Answer
	Choice
	Possible Answers
	

	
		Deemed-to-Satisfy solution
	

	
		Performance solution
	




Q5.  [bookmark: _Ref425255684]Identify five (5) materials commonly used for low rise buildings in your region. For each material, identify the following:
· Its name
· Properties of the material

	Answer
	#
	Material name
	Properties
	

	
	1
	Timber
	· Colour.
· Appearance.
· Hardness.
· Specific Gravity.
· Moisture Content.
· Shrinkage and Swelling.
· Strength

	

	
	2
	Rock/Stone
	Hardness
colour 
specific gravity 
cleavage 
fracture 
tenacity
	

	
	3
	Steel
	· Weldability. 
· Hardenability
· Machinability
· Workability (Bending / Forming) 
· Wear Resistance
· Corrosion Resistance.

	

	
	4
	Concrete
	· Strength
· Durability. ...
· Porosity and density. ...
· Fire resistance.
· Thermal and acoustic insulation properties.
· Impact resistance

	

	
	5
	Glass
	· Hardness and Brittleness.
· Weather Resistance
· Insulation
· Chemical Resistance
· Colour and Shape Varieties
· Transparency
· Fire Resistant Glazing

	





Q6.  [bookmark: _Ref425323073][bookmark: _Ref425248000]For each of the materials in Q5. identify the following:
· Quality of the material (i.e. durability, serviceability, cost effectiveness)
· Compatibility and non-compatibility of the material (i.e. what it would/would not be suitable for)

	Answer
	#
	Quality
	Compatibility 
	

	
	1
	Timber
	Cost Effective
Visually Appealing
Suitable for framing on houses
Not suitable for direct ground contact & termite prone areas. 
	

	
	2
	Rock/Stone
	Not Cost Effective, can be very expensive, especially granite. 
Great durability
Disadvantage is the weight of the product, can be very heavy
Rock/Stone is good for retaining walls and outside of buildings. 

	

	
	3
	Steel
	Durability is great, lasts, doesn’t expand or shrink. 
Cost effective to an extent, dearer then timber. 
Suitable for framing of homes which means no termites.
Steel posts on concrete is another good use. 
	

	
	4
	Concrete
	Durability and life span is enormous.  
Suitable for foundations and driveways. 
Block walls using concrete sleepers. 
Disadvantage is the toughness with load on concrete.
	

	
	5
	Glass
	Minimal environmental impact. 
Strong with glazed and provides good thermal insulation. 
Great for windows and facades.  Also can be used for tiling purposes, splashbacks etc
Not cost effective due to workload to produce.
	



Q7.  [bookmark: _Ref536083435]Identify five (5) physical characteristics that may be considered when evaluating potential building materials.

	Answer
	Purchase and installation cost
Cost to repair
Maintenance
Quality
Interaction & Compatability

	




Q8.  [bookmark: _Ref536095924]Match the terms and definitions below by writing the appropriate letter next to each number in the centre column.

	Answer
	Term
	Answers
	Definition
	

	
	1
	Carbon footprint
	1 -B
	A
	The amount of energy required to manufacture a product
	

	
	2
	CO2e
	2 -E
	B
	Total GHD emissions produced during manufacture construction and use
	

	
	3
	Embodied energy
	3 -A
	C
	Greenhouse gas emissions
	

	
	4
	Embodied water
	4 -D
	D
	The amount of water required to manufacture a product
	

	
	5
	GHG
	5 -C
	E
	CO2equivalent tonnes emitted into the atmosphere
	




Q9.  [bookmark: _Ref536083463]Which of the following materials would be considered as ‘low energy content’? Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
		Bricks
	

	
		By-products of other industrial processes
	

	
		Cement
	

	
		Glass
	

	
		Metals
	

	
		Plastics
	

	
		Sand
	

	
		Stone
	

	
		Timber
	



Q10.  [bookmark: _Ref536099133]Refer to the table below and identify the wall material type that has the smallest embodied energy and emission impact.

[image: ]

	Answer
	Walls Timber Frame, Fibro Cladding 
	





Q11.  [bookmark: _Ref536095926]Identify the Volume and Parts of the NCC that relate to energy efficiency of materials for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	Volume Two
Part 3.12
	Volume One
Part J
J1.1 
	




Q12.  [bookmark: _Ref536097820]Identify the relevant section of the Standards and Tolerances Guide and the associated Australian Standard that addresses residential slabs and footings.

	Answer
	Standards and Tolerances Guide
	Australian Standard 
	

	
	Section 2.0 
QBCC Standards & Tolerances Guide
	AS2870-2011
	




Q13.  [bookmark: _Ref536097822]Identify the relevant section of the Standards and Tolerances Guide and the associated Australian Standard that addresses roof tiles.

	Answer
	Standards and Tolerances Guide
	Australian Standard 
	

	
	Section 6.4
QBCC Standards & Tolerances Guide
	AS 2049 & AS2050
	




Q14.  [bookmark: _Ref536106144]Identify the Volume and Parts of the NCC that relate to safety barriers for swimming pools for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	Volume 2
Part 3.10.1
		Volume 2
Part 3.10.1



	




Q15.  [bookmark: _Ref536106145]In some states, barriers and fences for swimming pools are not entirely regulated by the NCC, as noted in the Ancillary Provisions and State and Territory Variations. Identify the applicable Act and Regulation that regulate safety barriers for swimming pools in your jurisdiction.

	Answer
	Building Act 1975
Building Regulation 2006
AS 1926
	



Q16.  [bookmark: _Ref536106146]Identify the Australian Standard that relates to safety barriers for swimming pools.

	Answer
	AS 1926.1
	




Q17.  [bookmark: _Ref536107455]True or False (Tick your response): According to the Standard in Q16. all gates must be fitted with a self-closing device that will return the gate to a closed position from any position without the use of manual force.

	Answer
		True 
	
	

	
		False 
	
	




Q18.  [bookmark: _Ref536170034]Identify the Volume and Parts of the NCC that relate to fire-resistance of building elements for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	Volume Two
Part 3.7.1
	Volume One 
Section C
	




Q19.  [bookmark: _Ref536170036]Identify the Australian Standard that relates to fire-resistance tests for elements of construction.

	Answer
	AS 1530.4-2005
	




Q20.  [bookmark: _Ref536169328]For all NCC Classes, where the ground or subfloor space is excessively damp or subject to frequent flooding, which durability class must the subfloor framing must be used where above ground?

	Answer
	Class 1 or 2 durability timbers or Class H3 preservative treated timbers

	





Q21.  [bookmark: _Ref536170040]Identify the Australian Standards that must be observed when meeting the requirements for Q20. 

	Answer
	AS 1684 Residential timber framed construction series of Australian Standards
	




Q22.  [bookmark: _Ref536170043]True or False (Tick your response): Where materials are not used as intended (or without considering NCC requirements), this can make a significant difference to the life or serviceability of the structure.

	Answer
		True 
	
	

	
		False 
	
	




Q23.  [bookmark: _Ref536170044]Explain why durability and serviceability impact on the cost effectiveness of chosen materials.

	Answer
	The durability & Serviceability impact the cost of chosen materials as cheaper materials may not last long for your particular building project but spending abit more money on a more durable product may last longer therefore will not be required to be replaced earlier or more often. This also relates to serviceability.  Is the product going to withstand the project for a more reliable period. 
Sometimes being cost effective on materials may not be the best option in the long run. 

	




Q24.  [bookmark: _Ref536172033]Provide an example of short term degradation of materials and describe its effects on a building on structure.

	Answer
	Short Term degradation on timber which is exposed to weather and water will rot and weather at a more rapid rate. This in turn will require the materials to be replaced in a short term basis.  Good idea to use a more durable product that can withstand the weather and water. 
	





Q25.  [bookmark: _Ref536172034]Provide an example of long term degradation of materials and describe its effects on a building on structure.

	Answer
	Certain metals used in building projects can overtime corrode due to the oxygen levels in the air. This will happen in long term basis and slowly.  If corroding occurs it can damage the metals can cause them to break down and disintegrate. They will need to be replaced when the structure is at risk due to the corrosion. 
	




Q26.  [bookmark: _Ref425327163][bookmark: _Ref425327708]You have spoken to a supplier who has indicated that some of the client’s desired materials are unavailable. When considering alternative building materials what must be taken into consideration (i.e. other than the client’s requirements)?

	Answer
	Availability and non-availability
Environmental Issues
Life Cycle Assessment Mythology
Compatibility
Testing Evidence
Short or long term degradation
Fire Resistant (If Required)

When choosing an alternative product, you also need to look at if the product is tested and efficeient for what you are using it for. Also what impacts it has on the environment and if it is cost effective for the client. 

	




Q27.  [bookmark: _Ref536177031]Identify two (2) things that you should look for when receiving a delivery of materials.

	Answer
	Make sure all materials ordered have been delivered. 
Make sure all materials are in good condition and not damaged. 
	




Q28.  [bookmark: _Ref536177032]If you encounter issues with delivery, what two (2) options do you have?

	Answer
	Accept the delivery with ‘conditions’ or reject the delivery and ask the supplier to re-send.

	




Q29.  [bookmark: _Ref409518704][bookmark: _Ref408838393]Which of the following should be assessed before shifting materials? Tick all that apply. 

	Answer
	Choice
	Possible Answers
	

	
		What needs to be relocated (e.g. size, weight)
	

	
		The relocation area, site layout and obstacles
	

	
		Distance and time to relocate load
	

	
		Whether a team is available and/or appropriate
	

	
		Whether PPE must be worn (e.g. for hazardous materials)
	




Q30.  [bookmark: _Ref536178585]What document should you refer to for guidance on how to handle and store hazardous chemicals? 

	Answer
	SDS – Safety Data Sheet
	




Q31.  [bookmark: _Ref408838395][bookmark: _Ref409519364]Name three (3) ways you can reduce the risk of injury if a load is too heavy for one person to carry, push or pull. 

	Answer
	Use a mechanical aid
Lighten the load
Ask for assistance to help move it with another person
	





Q32.  [bookmark: _Ref401922320]In the diagram below a person is lifting a tool box.
Filling in the table, indicate how each body part should be used/placed. 
[image: lifting]F. Hands
E. Knees
D. Shoulders
C. Feet
B. Back
A. Neck

	Answer
	Area of body (Letter)
	How it should be placed
	

	
	D
	Level
	

	
	A
	Upright
	

	
	F
	Good grip
	

	
	B
	Natural curve
	

	
	E
	Bent
	

	
	C
	Flat, facing load
	




Q33.  [bookmark: _Ref404158235]How should construction materials and components be handled? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
		Sorted to suit material type and size, separating hazardous material
	

	
		Stacked or stockpiled for ease of identification and retrieval
	

	
		Stored in access ways for ease of retrieval
	

	
		Stored clear of access ways
	

	
		Handled and positioned ready for installation
	




Q34.  [bookmark: _Ref536180244]Identify the Australian Standard that relates to the storage and handling of LP gas.

	Answer
	AS1596:2002
	



Q35.  [bookmark: _Ref536194481]List one (1) testing method for each of the building materials listed below.

	Answer
	Material name
	Properties
	

	
	Concrete
	Tested in Hydraulic Press
	

	
	Metals
	Repeated Loading
	

	
	Timber
	Stress Grading Machine Test
	




Q36.  [bookmark: _Ref536181364]What Code gives detailed tables which state the required grade of timber for specific sizes and uses?

	Answer
	Australian Timber Framing Code
	




Q37.  [bookmark: _Ref536181366]Name two (2) ways that defects may be seen in timber.

	Answer
	Knots, Splits, Veins, Insect Damage, Pockets of Resin
	




Q38.  [bookmark: _Ref536181368]Identify two (2) tests that may be performed to determine the durability of stone.

	Answer
	Acid Immersion
Or
Visually to check colour and grain size uniformity
Or
Water retention test
	



Q39.  [bookmark: _Ref536181370]Name two (2) ways that defects may be seen in stone.

	Answer
	Cracks and Fissures and how porous it is 
	




Q40.  [bookmark: _Ref536187863]True or False (Tick your response): Under a contract, builders and other specialist tradespersons are the ones most likely to rectify or remedy problems that arise from incorrect installation, application or placement of materials.

	Answer
		True 
	
	

	
		False 
	
	




Q41.  [bookmark: _Ref536187427]Name two (2) established methods that may be used to preserve timber.

	Answer
	Chemically treating timber to preserve timber from insects
Mechanical protection to prevent termites (Termite protection barrier) 
	




Q42.  [bookmark: _Ref536187429]Identify two (2) established methods that may be used to protect ferrous metals.

	Answer
	Galvanising the steel
Painting the metal using a special protection barrier. 
	





Q43.  [bookmark: _Ref536187430]Explain why the corrosion resistance of non-ferrous metals is superior to that of ordinary steel.

	Answer
	A layer of ceramic oxide or salt is applied to the non-ferrous metals such as aluminium, stainless steel or zinc to produce a barrier that protects it from corrosion. 
	




Q44.  [bookmark: _Ref536187432]When should aluminium be coated with bituminous paint? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
		At all times
	

	
		When it is buried in soil
	

	
		When it comes in contact with chemical materials
	

	
		When it is immersed in water
	

	
		When it is used on bitumen
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	PRACTICAL ASSESSMENT INSTRUCTIONS

· The following practical assessment will require the Participant to complete work related activities.
· The Assessor will conduct observations of the Participant’s work to determine whether they display sufficient practical skills and knowledge. 
· Please fill in the details below – providing your name, signature and date of assessment.
· The Participant’s signature acknowledges that the Assessor provided clear instructions and the Participant understood what was required to complete this assessment.
· The Assessor may substitute a Practical Task with an alternate task of equal value.
· Alternate tasks must be fully documented by the assessor in the Assessor Comments area.





	Participant name
	Rachel Redpath

	
	

	Participant signature
	
	
	

	Date
	7/04/2021



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.





	Task
	Task outcome (Tick)

	
	Satisfactory
	Not Yet Satisfactory

	Task 1 (Occasion 1)
		
	Task 1 (Occasion 2)
		



	ASSESSOR COMMENTS

	


CPCCBC4006B
Select, procure and store construction materials for low rise projects

	Practical Task 1 (2X)

	Description of task:
On two (2) occasions, a suitable observer is to verify the participant’s ability to supervise systems through which materials are selected, acquired and stored on site for the following projects:
· Occasion 1: Construction classified as Class 1 and 10 construction
· Occasion 2: Construction classified in Classes 2 to 9 with a gross floor area not exceeding 2000 square metres, not including Type A or Type B construction

The participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. Evidence to be submitted may include: 
· Copy of PO sent to site team for materials.
· Email correspondence sighting need for materials, delivery of materials and storage of materials (if relevant).

The observer is to provide detailed comments on the tasks completed by the participant. The assessor is to verify the observer’s comments in the Assessor Comments section, and provide the Practical Assessment outcome on the front cover of this document.

	Resources required: 
Computer, Building Contract, Drawings, Specifications, Building materials (including timber, and ferrous and non-ferrous metal).

	Assessment of task

	Name of participant:
	Rachel Redpath

	Name of observer:
	Matt Boxall 

	Role of observer 
(Confirm suitability to sign)
	Director

	Email address of observer
	admin@corporateplumbing.com.au

	Signature of observer:
	


	Date:
	8/04/2021

	When completing the task, did the participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	
	1st
Occasion
	2nd
Occasion

	1 Evaluate building materials

	1.1A.  [bookmark: _Ref535842396]Identify suitability of materials commonly used in the region for low rise buildings. 
	
	

	1.1B.  [bookmark: _Ref535842402][bookmark: _Ref536020766]Through research and testing, identify properties of different materials, their quality and compatibility and non-compatibility and maintain effective sampling and organisational record-keeping processes.
	
	

	1.1C.  [bookmark: _Ref535842408]Identify the environmental impacts of different materials. 
	
	

	1.1D.  [bookmark: _Ref535842411]Identify the impact of allowable tolerances on the conversion of naturally occurring materials. 
	
	

	1.1E.  [bookmark: _Ref535842424]Identify and check tolerances for installing and assembling materials with regard to the nature of the work being performed and the requirements of relevant construction industry Australian standards. 
	
	

	2 Material selection 

	1.2A.  [bookmark: _Ref535842432]Select materials structurally adequate and appropriate for the building system specified in the contract, drawings and specifications. 
	
	

	1.2B.  [bookmark: _Ref535842436]Select materials after considering:
· Safety
· Required fire resistance rating
· Suitability to the application
· Durability
· Serviceability and cost effectiveness
· Compliance with NCC, legislation, regulations and Australian Standards
	
	

	1.2C.  [bookmark: _Ref535842439]Consider short and long-term degradation of materials in relation to the building’s proposed life cycle. 
	
	

	1.2D.  [bookmark: _Ref535842441][bookmark: _Ref536188601]Select and evaluate alternative materials, if specified materials were unavailable or unsuitable – justifying decisions to regulatory authorities, as necessary
	
	

	1.2E.  [bookmark: _Ref535842446]Finalise selection of materials in accordance with contractual requirements and in consultation with relevant professionals and the client, compiling results in a report.
	
	

	1.2F.  [bookmark: _Ref535842459]Effectively communicate using the following methods:
· Language/concepts appropriate to cultural differences
· Non-verbal communication
	
	

	3 Supervising materials on site 

	1.3A.  [bookmark: _Ref535842490]Determine limitations and effects of transportation on material and components, taking action in potentially damaging circumstances. 
	
	

	1.3B.  [bookmark: _Ref535842494]Ensure materials were correctly and safely handled on site using appropriate equipment and safe work practices. 
	
	

	1.3C.  [bookmark: _Ref535842471]Communicate with manufacturers and suppliers to ensure materials are stored in accordance with specifications and Australian standards. 
	
	

	1.3D.  [bookmark: _Ref535842501]Implement processes for inspecting all materials delivered on site for naturally occurring and/or manufactured defects before installation. 
	
	

	1.3E.  [bookmark: _Ref535842506]Ensure personnel were aware of actions to be taken in the case of defects caused by incorrect installation, application or placement. 
	
	

	1.3F.  [bookmark: _Ref535842510]Preserve and protect timber and ferrous and non-ferrous metal used in the construction process.
	
	

	The Participant’s performance was:  Satisfactory     Not Satisfactory





	OBSERVER COMMENTS

	[bookmark: _GoBack]
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