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CHECKLIST for building fire protection compliance in Queensland 
	Passive Fire Protection
	Assessment

	Fire-Resistance Levels (FRL)
	✓ Compliant

	Fire-Rated Materials
	✓ Compliant

	Compartmentation
	✓ Compliant

	Fire Stopping
	✓ Compliant



	Active Fire Protection
	Assessment

	Fire Sprinkler Systems
	✓ Compliant

	Fire Detection and Alarm Systems
	✓ Compliant

	Emergency Lighting and Exit Signs
	✓ Compliant

	Occupant Warning Systems
	✗ Not Observed



	Overall Assessment

	Wynnum demonstrates satisfactory compliance with passive and active fire protection requirements for a Class 2 Commercial Building as outlined in the National Construction Code (NCC). The building's fire-resisting elements, fire-rated materials, and active fire protection systems are in good condition and meet the necessary standards.


Passive Fire Protection:
· The building's walls, floors, and ceilings have appropriate fire-resistance levels (FRL) as specified in the NCC.
· Fire-rated materials have been used for doors and walls separating different fire compartments.
· The building is divided into fire-resisting compartments with suitable fire-rated walls and doors to limit the spread of fire.
· Fire stopping is appropriately installed around service penetrations and openings in fire-rated elements.
Active Fire Protection:
· The building is equipped with an automatic fire sprinkler system, which appears to be operational and in good condition.
· Functional smoke detectors, heat detectors, and manual call points are installed at appropriate locations.
· Emergency lighting and illuminated exit signs were observed throughout the building.
· An occupant warning system was not observed to be present in the building.
Recommendations:
1. Conduct regular maintenance and testing of all fire protection systems in accordance with the manufacturer's guidelines and AS 1851.
2. Consider installing an occupant warning system for enhanced emergency communication during fire events.
3. Provide regular fire safety training for building occupants, emphasizing evacuation procedures and the proper use of fire-fighting equipment.
4. Ensure that all fire exits and accessways are unobstructed and clearly marked.
5. Review the building's fire safety management plan and update it as necessary.


