 (
Practical
 
Assessment
 
-
 
CPCCBC4001A
 
Apply
 
building
 
codes
 
and
 
standards
 
to
 
the
 
construction
 
process
 
for
 
low
 
rise
 
building
 
projects
)
Assessment Summary - CPCCBC4001A Apply building codes and standards to the construction process for low rise building projects
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The assessment activities for CPCCBC4001A Apply building codes and standards to the construction process for low rise building projects cover all aspects of the unit of competency required. To demonstrate competence in this unit, a participant must undertake all tasks and complete them satisfactorily and consistently. For Apprentices and Trainees, this includes employer completion of the Employer Record Book (ERB).

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be equitable, fair and flexible. If a participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor.

To satisfactorily complete the assessment, the participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a participant does not answer some questions or perform some tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. The Trainer/Assessor is able to provide the participant with additional information on interpreting the assessment outcomes and provide guidance on the participant’s options. Should a participant still be deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result.

By signing the cover page for each assessment item, the participant acknowledges they understand the assessment instructions and requirements and consent to being assessed. The participant also verifies and assures the RTO that the work submitted is their own work.

 (
UAA
 
Darshika
Participant
 
Name
)


	
	

	Theory Exam
	◻ Satisfactory
	◻ Not Yet Satisfactory

	Practical Assessment
	◻ Satisfactory
	◻ Not Yet Satisfactory

	
	◻ Competent
	◻ Not Yet Competent




	Assessor Name
	Myles Walder

	
Assessor Signature
	[image: ]
Click here to enter a date.

	Unit Competence Determination Date
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 (
THEORY
 
EXAM
 
INSTRUCTIONS
This
 
exam
 
will
 
occur
 
under
 
standard
 
assessment
 
conditions.
An oral examination may be allowed under certain circumstances,
 
whereby
 
the
 
Participant’s
 
answers
 
will
 
be
 
documented
 
by
 
a
 
party
 
other
 
than
 
the
 
Participant.
 
This
 
must
 
be
 
acknowledged
 
in
 
writing
 
(e.g.
 
FT001
 
and
 
Assessor
 
Comments)
Participants
 
must
 
provide
 
enough
 
detail
 
in
 
their
 
responses
 
to
 
demonstrate
 
their
 
knowledge
 
and
 
skills.
Please
 
fill
 
in
 
the
 
details
 
below,
 
providing
 
your
 
name,
 
signature
 
and
 
date
 
of
 
assessment.
Your
 
signature
 
acknowledges
 
that
 
this
 
is
 
your
 
own
 
work.
Assessors
 
are
 
to
 
complete
 
marking
 
in
 
pen
 
of
 
a
 
different
 
colour
 
to
 
the
 
Participant.
If
 
a
 
Participant
 
initially
 
answers
 
a
 
question
 
incorrectly
 
but
 
modifies
 
their
 
response,
 
they
 
must
 
follow
 
the
 
instructions
 
below:
If
 
a
 
Participant
 
changes
 
their
 
response
 
in
 
writing,
 
they
 
must
 
put
 
their
 
initials
 
next
 
to
 
the
 
written
 
change.
If
 
a
 
Participant
 
changes
 
their
 
response
 
verbally,
 
this
 
must
 
be
 
noted
 
on
the
 
exam
 
paper
 
by
 
the
 
assessor.
)

Participant name	UAA Darshika	 Participant signature	Dars³ika	
Date	18/04/2021	


Assessor name	Myles Walder	 Assessor signature


Date	Click here to enter a date.	


	Number of questions
	Number of questions answered correctly
	Task outcome (Tick)

	
38
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	Not Yet Satisfactor
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	◻
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the
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Q1.	A Performance Solution must abide by which of the following?
Tick all that apply.

 (
Choice
Possible
 
Answers
x
Be
 
assessed
 
according
 
to
 
one
 
or
 
more
 
of
 
the
 
Assessment
 
Methods
◻
Go
 
beyond
 
the
 
requirements
 
of
 
Deemed-to-Satisfy
 
Provisions
x
Comply
 
with
 
the
 
Performance
 
Requirements
)Answer	◻








Q2.	True or False (Tick your response): The Performance Requirements of the National Construction Code can be achieved by using a Performance Solution, a Deemed-to-Satisfy Solution, or a combination of both.

 (
x
True
◻
False
)Answer	◻




Q3.	True or False (Tick your response): The term ‘Performance Solution’ in the NCC was formerly known as ‘Alternative Solution’.

 (
x
True
◻
False
)Answer	◻


Q4.	Where a Performance Solution has been proposed, which of the following documentation should be prepared and retained?
Tick all that apply.

 (
Choice
Possible
 
Answers
x
Details
 
of
 
the
 
relevant
 
Performance
 
Requirements
x
Assessment
 
Methods
 
used
 
to
 
establish
 
compliance
 
with
 
the
 
relevant
Performance
 
requirements
x
Details
 
of
 
any
 
Expert
 
Judgement
 
relied
 
upon
x
Details
 
of
 
any
 
tests
 
of
 
calculations
 
used
 
to
 
determine
 
compliance
 
with
the
 
Performance
 
Requirements
x
Details
 
of
 
any
 
Standards
 
or
 
other
 
information
 
which
 
were
 
relied
 
upon
)Answer	◻
 (
Theory
 
Exam
 
-
 
CPCCBC4001A
 
Apply
 
building
 
codes
 
and
 
standards
 
to
 
the
 
construction
 
process
 
for
 
low
 
rise
 
building
 
projects
)
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Q5.	True or False (Tick your response): Where a Deemed-to-Satisfy solution has been proposed, all relevant plans/specifications should be retained.

 (
x
True
◻
False
)Answer	◻




Q6.	Identify the Volume and Parts of the NCC that outline the Assessment Methods used to determine whether a Performance Solution or a
Deemed-to-Satisfy Solution complies with the Performance Requirements for Classes 1 and 10, and Classes 2 to 9.

 (
Classes
 
1
 
and
 
10
Classes
 
2
 
to
 
9
Volume
2
-
Section
2
-
 
Performance
 
provisions
Volume
 
1-
 
Part
 
A0/A2.2
)Answer	◻





Q7.	Identify the Australian Standard that relates to artificial lighting needed for safe movement, as noted in the NCC.

 (
AS/NZS
 
1680.0
) (
◻
)Answe r


Q8.	Identify the Volume and Parts of the NCC that outline the requirements for artificial lighting needed for safe movement for Classes 1 and 10, and Classes 2 to 9.

 (
Classes
 
1
 
and
 
10
Classes
 
2
 
to
 
9
Volume
 
2
 
-
 
part
 
3.8.4.3
 
Artificial
 
lighting,
 
3.12.5.5
 
Artificial
 
lighting
volume
 
one
 
-
 
part
 
J6
-
 
Artificial
 
lighting
 
and
 
power
)Answer	◻
 (
Theory
 
Exam
 
-
 
CPCCBC4001A
 
Apply
 
building
 
codes
 
and
 
standards
 
to
 
the
 
construction
 
process
 
for
 
low
 
rise
 
building
 
projects
)
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Q9.	Fill in the blanks for the statement below, referring to Volume 1 of the NCC with regards to lighting:
Where a Deemed-to-Satisfy Solution is proposed, Performance Requirements
_BP1.1	to	BP1.4	are satisfied by complying with
(i)	_B1.1	to	B1.6	; and
(ii) For a building containing an occupiable outdoor area,	; and
(iii) for farm buildings and farm sheds,	.


Where a Performance Solution is proposed, the relevant Performance
Requirements must be determined in accordance with	and
 	as applicable.

 (
◻
)Answe r

Q10. Fill in the blanks for the statement below, referring to Volume 2 of the NCC with regards to light:
Where an alternative light system is proposed as a Performance Requirement to that described in _Part 3.8.4	, that proposal must comply with
–
(a) Performance Requirement	P2.4.4	; and
(b) the relevant Performance Requirements determined in accordance with
 	1.0.7	and	1.0.4	as applicable.

 (
◻
)Answe r

Q11.	Identify the Australian Standard that relates to each of the listed types of fire fighting equipment, as noted in the NCC.

 (
Equipment
Australian
 
Standard
Fire
 
hydrants
AS
 
2419.1
Fire
 
hose
 
reels
AS
 
2441
Portable
 
fire
 
extinguishers
AS
 
2444
)Answer	◻
 (
Theory
 
Exam
 
-
 
CPCCBC4001A
 
Apply
 
building
 
codes
 
and
 
standards
 
to
 
the
 
construction
 
process
 
for
 
low
 
rise
 
building
 
projects
)
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	Smoke alarms
	AS 3786



Q12. For each of the listed types of fire fighting equipment, identify whether they are required by the NCC (if so, identify the relevant Part).

 (
Equipment
Volume
 
1
Volume
 
2
Fire
 
hydrants
E1.3
Tas
 
3.7.4.2
 
Water
 
Supply
Fire
 
hose
 
reels
E1.4
Portable
 
fire
 
extinguishers
E1.6
Smoke
 
alarms
EP2.1
3.7.2
)Answer	◻







Q13. Identify the applicable Act in your jurisdiction that outlines the
requirements for smoke alarm installation in domestic dwellings. Briefly identify the requirements.

 (
Act
 
name
 
and
section(s)
Requirements
Fire and
 
Emergency
 
Services
 
(Domestic
 
Smoke
 
Alarms)
 
Amendment Act
 
2016
 
-
Section 7 -
 
104RBA
Owner must
 
install
 
smoke
alarm
The
 
owner
 
of
 
a
 
domestic
 
dwelling
 
must install
 
smoke alarms in the dwelling in compliance with this
 
section.
Maximum
 
penalty—5
 
penalty
 
units.
A
 
smoke
 
alarm
 
must
 
be
 
installed
 
in
 
each
 
place
 
in
 
the domestic dwelling required by a regulation.
 
(5)Each
 
smoke
 
alarm
 
must—
be
 
powered
 
in
 
a
 
way
 
prescribed
 
by
 
regulation;
 
and
comply
 
with
 
other
 
requirements
 
prescribed
 
by
 
regulation;
 
and
have
 
been
 
manufactured
 
less
 
than
 
10
 
years
 
before
 
the
 
smoke
 
alarm
 
is
 
installed;
 
and
operate
 
when
 
tested;
 
and
be
 
interconnected
 
to
 
every
 
other
 
smoke
 
alarm
 
installed
 
in
 
the
 
domestic
 
dwelling.
)Answer	◻
 (
Theory
 
Exam
 
-
 
CPCCBC4001A
 
Apply
 
building
 
codes
 
and
 
standards
 
to
 
the
 
construction
 
process
 
for
 
low
 
rise
 
building
 
projects
)
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Q14. Identify the applicable Act in your jurisdiction that outlines the requirements for testing smoke alarms in domestic dwellings. Briefly identify the requirements.

 (
Act
 
name
 
and
section(s)
Requirements
(3)A
 
smoke
 
alarm
 
installed
 
in
 
a
 
domestic
 
dwelling
 
must
 
be
 
tested
 
as
 
follows—
Fire and
 
Emergency
 
Services
 
(Domestic
 
Smoke
 
Alarms)
 
Amendment Act
 
2016
 
-
 
5
Insertion
 
of
 
news
 
104RAA
for
 
an
 
alarm
 
that
 
can
 
be tested by pressing a
 
button or other device to indicate whether the alarm
 
is
 
capable
 
of
 
detecting
 
smoke—by
 
pressing
 
the
 
button
 
or
 
other
 
device;
otherwise—
by
 
being
 
tested
 
by
 
the
 
owner
 
of
 
the
 
dwelling
 
in
 
the
 
way
 
stated
 
in
 
the
 
manufacturer’s
 
instructions;
 
or
by
 
being
 
tested
 
by
 
a
 
tenant
 
of
 
the
 
dwelling
 
in
 
the
 
way
 
stated
 
in
 
the
 
information
 
statement.
(2)Also,
 
if
 
a
 
smoke
 
alarm
 
in
 
a
 
domestic dwelling
 
does
 
not
 
operate
 
when
 
tested,
 
the
 
owner
 
of
 
the
 
dwelling must immediately replace the smoke alarm
 
under
 
this
 
section.
Maximum
 
penalty—5
 
penalty
 
units.
)Answer	◻


























Q15. Identify the applicable Act in your jurisdiction that outlines what must occur if smoke alarm in a domestic dwelling does not operate upon testing and when any rectification must occur. Briefly identify the
requirements.

 (
Act
 
name
 
and
section(s)
Requirements
Fire
and
Emergency
Services
(Domestic
 
Smoke
Alarms)
(2)Also,
 
if
 
a
 
smoke
 
alarm
 
in
 
a
 
domestic
 
dwelling
 
does
 
not
 
operate
 
when
 
tested,
 
the
 
owner
 
of
 
the
Amendment
Act
dwelling
 
must
 
immediately
 
replace
 
the
 
smoke
 
alarm
2016
 
-
under
 
this
 
section.
8
Maximum
 
penalty—5
 
penalty
 
units.
Replacement
 
of
 
s
104RC
(Lessor
must
replace
smoke
 
alarm)
)Answer	◻
 (
Theory
 
Exam
 
-
 
CPCCBC4001A
 
Apply
 
building
 
codes
 
and
 
standards
 
to
 
the
 
construction
 
process
 
for
 
low
 
rise
 
building
 
projects
)
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Q16. In observation of NCC Volume 2, identify three (3) aspects which should be checked with regards to smoke alarms.

 (
(a)
comply
 
with
 
AS
 
3786,
 
except
 
that
 
in
 
a
 
Class
 
10a
 
private
 
garage
where
 
the
 
use
 
of
 
the area is likely to result in smoke alarms causing
 
spurious signals, any other alarm deemed suitable in accordance with AS
 
1670.1 may be installed provided that smoke alarms complying AS 3786
 
are
 
installed
 
elsewhere
 
in
 
the
 
Class
 
1
 
building;
 
and
be connected to the consumer mains power where consumer
 
power
 
is
 
supplied
 
to
 
the
 
building;
 
and
be
 
interconnected
 
where
 
there
 
is
 
more
 
than
 
one
 
alarm.
) (
◻
)Answe r
 (
Theory
 
Exam
 
-
 
CPCCBC4001A
 
Apply
 
building
 
codes
 
and
 
standards
 
to
 
the
 
construction
 
process
 
for
 
low
 
rise
 
building
 
projects
)
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Q17. Must all smoke alarms be interconnected in domestic dwellings?
Explain your response with reference to legislation.

 (
Fire and Emergency Services (Domestic Smoke Alarms) Amendment Act
 
2016
 
-
Section
 
7
 
-
 
(5)
 
&
 
(6)
A
 
smoke
 
alarm (the 
first smoke alarm
) is interconnected to another
 
smoke
 
alarm
 
if—
the first smoke alarm sounds an alert if the other smoke
 
alarm is activated because its sensor detects smoke;
 
and
the other smoke alarm sounds an alert if the first smoke
 
alarm
 
is
 
activated
 
because
 
its
 
sensor
 
detects
 
smoke.
) (
◻
)Answe r
















Q18. Fill in the blanks for the definition of fire compartments, referring to Volume 1 of the NCC:
Fire compartment means –
(a) The total space of a building; or
(b) When referred to in –
(i) The Performance Requirements – any part of a building separated from the remainder by			to fire such as  	 and/or	having an appropriate resistance to the spread of fire with any		adequately protected; or
(ii) The Deemed-to-Satisfy Provisions – any part of a building separated from the remainder by		and/or	each having an	not less than that required for a fire
 	for that type of construction and where all
 	in the	construction are protected in accordance with the DtS Provisions of the relevant Part.
 (
◻
)Answe r


Q19. Identify the Volume and Parts of the NCC that outline the requirements for fire compartmentation and separation for Classes 1 and 10, and
Classes 2 to 9.
 (
Theory
 
Exam
 
-
 
CPCCBC4001A
 
Apply
 
building
 
codes
 
and
 
standards
 
to
 
the
 
construction
 
process
 
for
 
low
 
rise
 
building
 
projects
)
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 (
Classes
 
1
 
and
 
10
Classes
 
2
 
to
 
9
Volume
 
1
 
-
 
Part
 
C2
)Answer	◻




Q20. Fill in the blanks for the statement below, referring to Volume 1 of the NCC with regards to fire compartmentation and separation:

Where a Deemed-to-Satisfy Solution is proposed, Performance Requirements
 	to	are satisfied by complying with
(i)  	to	,	to  	
and	to	; and
(ii) in a building containing an atrium,	; and
(iii) for additional requirements for Class 9b buildings,	; and
(iv) for farm sheds,	.
Where a Performance Solution is proposed, the relevant Performance
Requirements must be determined in accordance with	A2.2(3)	 and	A2.4(3)	as applicable.

 (
◻
)Answe r


Q21. Fill in the blanks for the statement below, referring to Volume 2 of the NCC with regards to fire separation:

Where an alternative fire separation design is proposed as a Performance Solution to that described in Part	3.7.1		that proposal must comply with Performance Requirement	P2.3.1		; and the relevant Performance Requirements determined in accordance with
 	1.0.7	and	as applicable.

 (
◻
)Answe r


Q22. Identify the Australian Standard referenced in NCC Volume 1 with regards to compartmentation and separation for electricity supply systems.

 (
◻
)Answe r
 (
Theory
 
Exam
 
-
 
CPCCBC4001A
 
Apply
 
building
 
codes
 
and
 
standards
 
to
 
the
 
construction
 
process
 
for
 
low
 
rise
 
building
 
projects
)
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Q23. Identify the Volume and Parts of the NCC that outline the level of fire resistance required for Classes 1 and 10, and Classes 2 to 9.

 (
Classes
 
1
 
and
 
10
Classes
 
2
 
to
 
9
Volume
 
1
 
-
Schedule
 
5
Volume
 
2
 
-
3.7.1.5
 
Construction
 
of
 
walls
3.7.1.8
 
Separating
 
walls
3.7.1.11
 
Separating
 
floors
external
C3.5
 
C1.3
Specification
 
C1.8
4.1
Fire-resistance
of
building
 
elements
5
 
Type
 
C
 
fire-resisting
 
construction
)Answer	◻















Q24. In a building’s specifications, an FRL is stated as being 90 / 60 / -.
If exposed to a standard fire test, how many minutes can you expect this building element to last for the criteria listed below?

 (
Minutes
Criteria
-
Insulation
60
Integrity
90
Structural
 
adequacy
)Answer	◻







Q25. Fill in the blanks:
According to NCC Volume 1, an electricity substation located within a building must be separated from any other part of the building by construction having an FRL of no less than _120	/ _120	/	120	and have any doorway in that construction protected with a self-closing fire door having an FRL of not less than	-	/	120	/ _30		.

 (
◻
)Answe r


Q26. Fill in the blanks: According to NCC Volume 2, if an electrical wire or cable penetrates a separating wall, the service and building element at the penetration must be identical with a prototype assembly which has been tested and achieve an FRL of not less than	-	/	60	/	60	.
 (
Theory
 
Exam
 
-
 
CPCCBC4001A
 
Apply
 
building
 
codes
 
and
 
standards
 
to
 
the
 
construction
 
process
 
for
 
low
 
rise
 
building
 
projects
)
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 (
◻
)Answe r
 (
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Exam
 
-
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building
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and
 
standards
 
to
 
the
 
construction
 
process
 
for
 
low
 
rise
 
building
 
projects
)
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Q27. Identify the applicable Act in your jurisdiction that outlines the occupier’s requirements for maintaining prescribed fire safety installations (e.g. fire doors). Briefly identify the requirements.

 (
Act
 
name
 
and
section(s)
Requirements
Building
 
Fire
 
Safety Regulation
 
2008
 
(Qld)-
Part
5
Maintenance
of
 
prescribed
fire
 
safety
 
installations
Fire safety installations and protection are required
 
to be ready to operate at all times, or a substantial
 
threat
 
to occupants and property may exist. They
 
may
 
only
 
be
 
required
 
to
 
operate
 
infrequently
 
over
 
the life of a building and therefore their reliability in a
 
building
 
is
 
critical.
 
Regular
 
maintenance
 
of
 
fire
 
protection
 
systems
 
and
 
equipment
 
for
 
continuing
 
operational
 
efficiency
 
is
 
an
 
important
 
part
 
of
 
every
building
 
occupier's
 
responsibility.
)Answer	◻














Q28. Identify the applicable Regulation in your jurisdiction that outlines the timeframes in which repair or corrective action must be taken when maintaining prescribed fire safety installations. Briefly identify the
requirements.

 (
Regulation
 
name
 
and
 
section(s)
Requirements
Building
 
Fire
Safety
 
Regulation
2008
 
-
Division 3 -
 
Obligations
 
of
 
occupiers
54
 
-
 
Maintenance
 
of
 
prescribed
 
fire
(4)
 
The
 
occupier
 
of
 
the
 
building must ensure the
 
repair is carried out or the corrective action is taken
 
no later than 1 month after the maintenance of the
 
installation was carried out, unless the occupier has
 
a
 
reasonable
 
excuse.
safety
installations
)Answer	◻














Q29. NCC Volume 1 outlines that fire doors must be fitted with smoke seals and the assembly must be tested in accordance with Australian
Standards. To which classes of building does this specification apply?

 (
Class
 
2
 
and
 
3
 
buildings:
 
Concession
) (
◻
)Answe r

Q30. Do all fire doors require tags? Explain your response with reference to legislation.
 (
Theory
 
Exam
 
-
 
CPCCBC4001A
 
Apply
 
building
 
codes
 
and
 
standards
 
to
 
the
 
construction
 
process
 
for
 
low
 
rise
 
building
 
projects
)
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 (
No.
Buildings approved after 1 April 1976 under the Building Act 1975 (Qld) all
 
require
 
tags
 
to
 
be
 
fitted
 
to
 
the
 
fire
 
doors.
 
Fire
 
doors
 
that
 
have been
 
replaced
 
after
 
the
 
1
 
April
 
1976
 
all
 
require
 
tags
 
to
 
be
 
fitted.
Buildings approved before this date are not required to have tags fitted to
 
the
 
fire
 
doors
 
unless
 
required
 
by
 
the
 
local
 
authority
 
at
 
the
 
time
 
of
 
approval.
) (
◻
)Answe r





Q31. Match the building classifications and their descriptions by writing the appropriate letter next to each number in the centre column.

 (
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and
 
standards
 
to
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construction
 
process
 
for
 
low
 
rise
 
building
 
projects
)
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Answer	◻
1  (
Classification
1
Class
 
1
2
Class
 
2
3
Class
 
3
4
Class
 
4
5
Class
 
5
6
Class
 
6
7
Class
 
7
8
Class
 
8
9
Class
 
9
1
0
Class
 
10
) (
Description
A
A
 
non-habitable
 
building
 
or
 
structure.
B
A
 
laboratory
 
or
 
a
 
building
 
in
 
which
 
a
handicraft
 
or
 
process
 
for
 
the
 
production,
 
assembling,
 
altering,
 
repairing,
 
packing,
 
finishing
 
or
 
cleaning
 
of
 
goods
 
or
 
produce
 
is
carried
 
on
 
for
 
trade,
 
sale
 
or
 
gain.
C
A
 
residential
 
building
 
other
 
than
 
Class
 
1
 
or
 
2
 
which
 
is
 
a
 
common
 
place
 
of
 
long
 
term
 
transient
 
living
 
for
 
a
 
number
 
of
 
unrelated
persons.
D
A
 
dwelling
 
in
 
a
 
building
 
that
 
is
 
Class
 
5,
 
6,
 
7,
 
8
or
 
9
 
if
 
it
 
is
 
the
 
only
 
dwelling
 
in
 
the
 
building.
E
May
 
be
 
a
 
single
 
dwelling
 
or
 
a
 
boarding
house,
 
guest
 
hose
 
or
 
hostel
 
with
 
a
 
floor
 
area
 
less
 
than
 
300m
2
.
F
An
 
office
 
building
 
used
 
for
 
professional
 
or
 
commercial
 
purposes,
 
excluding
 
buildings
 
of
 
Class
 
6,
 
7,
 
8
 
or
 
9.
G
A
 
shop
 
or
 
other
 
building
 
for
 
the
 
sale
 
of
 
goods
 
by
 
retail
 
or
 
the
 
supply
 
of
 
services
 
direct
 
to
 
the
public.
H
A
 
building
 
containing
 
2
 
or
 
more
sole-occupancy
 
units,
 
each
 
being
 
a
 
separate
dwelling.
I
A
 
building
 
which
 
is
 
a
 
carpark
 
or
 
fore
 
storage/display
 
of
 
goods
 
or
 
produce
 
for
 
sale
by
 
wholesale.
J
A
 
building
 
of
 
a
 
public
 
nature.
)- E


2 - H



3 - C

4 - D

5 - F

6 - G

7 - I

8 - B

9 - J

10 - A



Q32. What class of building would shops, restaurants and cafes belong to?

 (
Class
 
6
) (
◻
)Answe r

Q33. What class of building would a general medical practitioner’s office belong to?

 (
Class
 
5
) (
◻
)Answe r



Q34. True or False (Tick your response): At the design stage, it may not be clear who the final tenant will be (or how they will be using their tenancy), so as long as the design meets the minimum requirements of all the classifications, it could be used for any of the purposes.

 (
X
True
◻
False
)Answer	◻




Q35. Where parts of a building have different purposes, the classification of Class 1 may apply to the whole building if not more than what percentage of the floor area is used for a purpose which is a different classification? Tick your response.

 (
Choice
Possible
 
Answers
◻
5%
x
10%
◻
25%
◻
50%
)Answer	◻










Q36. The NCC aims to ensure structures appropriately withstand normal forces. Match the terms and definitions below by writing the appropriate letter next to each number in the centre column.

 (
Theory
 
Exam
 
-
 
CPCCBC4001A
 
Apply
 
building
 
codes
 
and
 
standards
 
to
 
the
 
construction
 
process
 
for
 
low
 
rise
 
building
 
projects
)
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Answe

Answer	◻
1  (
Term
1
Bending
2
Compressio
 
n
3
Shear
4
Strain
5
Stress
) (
Definitions
A
A
 
force
 
which
 
shortens
 
or
 
crushes.
B
A
 
fore
 
which
 
stretches
 
and
 
squashes
 
at
 
the
 
same
 
time.
C
A
 
force
 
which
 
tries
 
to
 
pull
 
something
 
apart.
D
Intensity
 
of
 
the
 
internally
 
distributed
 
forces
 
that
 
resist
 
a
 
change
 
in
 
the
 
form
 
of
 
a
 
body.
E
Physical
 
change
 
in
 
the
 
dimensions
 
of
 
a
structure
 
that
 
results
 
from
 
applying
 
a
 
load.
)- B

2 - A
3 - F
4 - E

5 - D


6  (
Tension
6
) (
F
Created
 
where
 
two
 
opposite
 
forces
 
try
 
to
cut,
 
tear
 
or
 
rip
 
something
 
in
 
two.
)- C
 (
Theory
 
Exam
 
-
 
CPCCBC4001A
 
Apply
 
building
 
codes
 
and
 
standards
 
to
 
the
 
construction
 
process
 
for
 
low
 
rise
 
building
 
projects
)
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Q37. True or False (Tick your response): When a beam is loaded, the top is compressed and the bottom is in tension.

 (
x
True
◻
False
)Answer	◻




Q38. True or False (Tick your response): When a cantilever is loaded, the top surface is in tension and the bottom is in compression.

 (
x
True
◻
False
)Answer	◻
 (
Theory
 
Exam
 
-
 
CPCCBC4001A
 
Apply
 
building
 
codes
 
and
 
standards
 
to
 
the
 
construction
 
process
 
for
 
low
 
rise
 
building
 
projects
)
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 (
A
PPLY
) (
BUILDING
)[image: ][image: ] (
STANDARDS
)[image: ] (
CONSTRUCTION
) (
AND
 
LOW
)

 (
CPCCBC4001A
)
CODES	TO THE
 (
PROCESS
)  (
FOR
)	 (
RISE
)  (
BUILDING
)  (
PROJECTS
)

 (
PRACTICAL
 
ASSESSMENT
 
INSTRUCTIONS
The
 
following
 
practical
 
assessment
 
will
 
require
 
the
 
Participant
 
to
 
complete
 
work
 
related
 
activities.
The
 
Assessor
 
will
 
conduct
 
observations
 
of
 
the
 
Participant’s
 
work
 
to
 
determine
 
whether
 
they
 
display
 
sufficient
 
practical
 
skills
 
and
 
knowledge.
Please
 
fill
 
in
 
the
 
details
 
below
 
–
 
providing
 
your
 
name,
 
signature
 
and
 
date
 
of
 
assessment.
The Participant’s signature acknowledges that the Assessor provided
 
clear
 
instructions
 
and
 
the
 
Participant
 
understood
 
what
 
was
 
required
 
to
 
complete
 
this
 
assessment.
The
 
Assessor
 
may
 
substitute
 
a
 
Practical
 
Task
 
with
 
an
 
alternate
 
task
 
of
 
equal
 
value.
Alternate
 
tasks
 
must
 
be
 
fully
 
documented
 
by
 
the
 
assessor
 
in
 
the
 
Assessor
 
Comments
 
area.
)


Participant name	UAA Darshika	

Participant signature	Dars³ika
Date	18/04/2021	


Assessor name	Myles Walder	 Assessor signature


Date	Click here to enter a date.	



	Task
	Task outcome (Tick)

	
	Satisfactory
	Not Yet Satisfactory

	Task 1 (Occasion 1)
	◻
	◻

	Task 1 (Occasion 2)
	◻
	◻
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ASSESSOR COMMENTS
 (
Practical
 
Assessment
 
-
 
CPCCBC4001A
 
Apply
 
building
 
codes
 
and
 
standards
 
to
 
the
 
construction
 
process
 
for
 
low
 
rise
 
building
 
projects
)
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 (
FOR
 
LOW
) (
RISE
) (
BUILDING
) (
PROJECTS
) (
CPCCBC4001A
) (
A
PPLY
 
BUILDING
) (
CODES
 
AND
) (
STANDARDS
 TO
) (
CONSTRUCTION
) (
PROCESS
)THE

	Practical Task 1 (2X)

	Description of task:
On two (2) occasions, a suitable observer is to verify the participant’s ability to access, interpret and apply relevant building codes and standards.
· Occasion 1: Construction classified as Class 1 and 10 construction
· Occasion 2: Construction classified in Classes 2 to 9 with a gross floor area not exceeding 2000 square metres, not including Type A or Type B construction
The participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet.
Evidence to be submitted may include:
· Documented evidence of determining a compliant solution on a project including:
· Correspondence such as letters, emails, and records of other communications
· Certifier reports, instructions
· Other compliance documentation for a project including:
· Council or private certifier inspection reports
· Structural inspection certificates
· Occupation certificates
The observer is to provide detailed comments on the tasks completed by the participant. The assessor is to verify the
observer’s comments in the Assessor Comments section, and provide the Practical Assessment outcome on the front cover of this document.

	Resources required:
Drawings and specifications, National Construction Code, Australian Standards, Relevant legislation.

	Assessment of task

	Name of participant:
	UAA Darshika

	Name of observer:
	Myles Walder

	Role of observer
(Confirm suitability to sign)
	

	Email address of observer
	

	
Signature of observer:
	
[image: ]

	Date:
	Click here to enter a date.

	
When completing the task, did the participant:
	Tick if satisfactorily completed.
Provide comments if left unticked.

	
	1st
Occasion
	2nd
Occasion

	1 Access and interpret codes and standards

	1.A. Identify relevant performance requirements from the National Construction
Code that apply to individual projects described as low rise.
	◻
	◻

	1.B. Determine requirements of relevant National Construction Code
deemed-to-satisfy (DTS) provisions.
	◻
	◻

	1.C. Access and interpret requirements of relevant Australian standards
referenced in the National Construction Code.
	◻
	◻


 (
Practical
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-
 
CPCCBC4001A
 
Apply
 
building
 
codes
 
and
 
standards
 
to
 
the
 
construction
 
process
 
for
 
low
 
rise
 
building
 
projects
)
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	2 Classify buildings

	1.2A. Determine the nature of building according to its use and arrangement.
	◻
	◻

	1.2B. Apply National Construction Code criteria to determine the defined
classification.
	◻
	◻

	1.2C. Identify and interpret National Construction Code requirements for
multiple classification.
	◻
	◻

	3 Solutions for compliance

	1.3A. Determine range of criteria to ensure that construction methods comply with National Construction Code performance requirements.
	◻
	◻

	1.3B. In accordance with company policy and procedures, discuss and propose alternative solutions to a design or construction problem that complied with National Construction Code requirements, considering basic design principles and the behaviour of materials and structures under stress, strain, compression, bending or combined actions.
	◻
	◻

	1.3C. Identify and document performance-based solutions in accordance with
National Construction Code requirements.
	◻
	◻

	1.3D. Analyse and apply assessment methods referenced in the National Construction Code to determine whether a building solution complied with performance requirements or DTS provision.
	◻
	◻

	1.3E. Identify and complete relevant documentation in accordance with National Construction Code requirements.
	◻
	◻

	1.3 F. Effectively communicate using the following methods:
· Language/concepts appropriate to cultural differences
· Non-verbal communication
	◻
	◻

	4 Fire protection requirements

	1.4A. Identify and apply passive and active fire control elements for low rise
buildings, as required by the National Construction Code and other legislation (including WHS requirements).
	◻
	◻

	1.4B. Determine level of fire resistance required for the construction of various
low rise buildings.
	◻
	◻

	1.4C. Check existing buildings for compliance with passive and active fire
protection requirements, in accordance with National Construction Code
requirements.
	◻
	◻

	The Participant’s performance was: ◻ Satisfactory	◻ Not Satisfactory
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