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Hazard Identification Form Template
	Project name
	Maroochydore Private Hospital

	Prepared by
	Ric

	Date completed
	19/02/2024


Table Format
	
	
	
	Control measure

	Hazard
	Affected personnel
	Associated risks
	Control measure for implementation
	Personnel who will implement
	Deadline for implementation

	Mobile Plant 
	All Workers
	Crush/struck by
	Pos coms/exclusion zones
	Plant operator and Spotter
	Prior to commencement of task- 9:am 19/02/2024

	Vehicle access to site
	All workers
	Plant interaction Public/pedestrian interaction, vehicle roll ways
	  Construction traffic to follow designated route via controlled site access points    
	Traffic management
	Prior to commencement of task- 9:am 19/02/2024

	House keeping
	All workers
	    Poor Housekeeping (Slips, trips, falls)  
	    Is adequate to allow persons who are not employees to move safely within the place of work and facilitates safe access to and egress from the place of work, including emergency exits  Daily weekly cleans bins provided
	All workers
	During and After completed works

	PPE selection, supply and use
	All workers
	   Not meeting Australian standards    
	[bookmark: _GoBack]   Work activities to be employed that eliminate the requirement for extra PPE other than site mandatory PPE where possible    Employer to provide compliant PPE as per SWMS 
	All workers
	Prior to work commencing each day

	
	
	
	Control measure

	Hazard
	Affected personnel
	Associated risks
	Control measure for implementation
	Personnel who will implement
	Deadline for implementation

	    Fire protection / detection 
operation during works   
	All workers
	Unarmed 
Set off due to work activity
	All fire sensors to be identified before work commences and protected during works
During hot works a Fire blanket is to be placed  between work area and sensor
Complete Hot Works Permit and identify all fire heads and sensors for protection
	   McNab
Subcontractor (PCBU)    
	     Prior to work commencing each day  

	     Workplace Violence  
	All workers
	Intimidation, Bullying 

	Provide counselling for those involved
During Site Induction, identify that bullying and harassment is unacceptable on site
	   McNab
Subcontractor (PCBU)    
	At all times

	    Mobile phone use  
	All workers
	    Personal injury  
	No mobile phones are to be used when operating plant
Persons at the workplace should never make or receive calls when working in the vicinity of operating plant
If phone needs to be answered or calls need to be made, check surroundings or move to a safe area. 
Persons using phone on site are to isolate themselves from moving plant
Persons using phone are not to walk  around the site whilst using the mobile phone
	   McNab
Subcontractor (PCBU)  
	At all times

	   Workplace Stress  
	All workers
	   Work hours, work environment  
	Where possible, employees not to be exposed to excessive heat or cold, irritant noise, poor lighting or physical hazards 
Ensure regular consultation with employees through tool box talks 
Working hours not to exceed those stipulated in award.
Welfare and trauma counselling made available to all staff in the event of a serious incident on site
	  McNab   Subcontractor (PCBU)
	At all times

	Dust
	All workers
	Dust
	  Offsite cutting and prefabrication should be used as much as possible 
Erect cutting rooms or designated cutting areas to capture dust and with adequate ventilation 
Use methods to suppress dust i.e. water spray, dust barriers
Regular clean ups to be completed on site
Equipment to be regularly cleaned   
	   McNab
Subcontractor (PCBU)  
	At all times

	Noise / vibration
	All workers     
	   Noise / vibration  
	  Works to be completed within DA conditional hours.  
Where there is a potential for Noise and vibration exposure limited to noise in excess of: 85 dB(A) continuously for eight hours or a daily noise dose equivalent to or above 85dB(A) in a shorter time frame, silencers on plant to be considered and implemented where possible. Hearing Protection to be worn at all times.
Vibration exposure to arms/ hands from tools for greater than 4 hours in a 24 hour period to be used to manufacturers specification and duration. Anti vibration gloves to be worn. Rotation schedule to be established.
Exposure to whole body vibration must not exceed the exposure levels nominated for machinery or plant by the manufacturer. Use tools and methods that create less noise and vibration where possible 
Noise producing activities to be isolated where ever possible, Subcontractor to address the control of noise during their activities
Wear appropriate ear protection and take note of signage and restricted areas 
Plant and equipment to be maintained i.e. exhausts ; Community complaints register to be maintained by McNab   
	    McNab
Subcontractor (PCBU) 
	At all times



End of Hazard Identification Form Template


Page 8 of 9		CSTC Pty Ltd (RTO #0699)

CSTC Pty Ltd (RTO #0699)		Page 9 of 9
