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	Handout 5 - CPCCBC4012 Read and interpret plans and specifications

Cost Estimation Sheet

	Participant name
	Lucy Muston 

	Date
	08/04/2025 



Details of Building and Construction Project
	Name of project
	Calvary Christian College – New Prep Building 

	Type of project
	 Residential building
 Commercial building

	State/Territory
	Queensland 

	Plans accessed for material estimates
	Yes 




Identify internal linings, external cladding and roof materials from plans and specification
	Item
	Description 

	Internal linings
	ACP
Item: Acoustic Ceiling Panel
Product Name: Quiet Space Panel
Brand: Autex
Material: Thermally Bonded Polyester
Thickness: 25mm
Colour: Nude White
Sheet Size: 2400 x 1200 (cut into 1200 x 1200 panels)
Description: The Acoustic Ceiling Panels will be directly fixed to the ceiling lining in accordance with the manufacturer’s recommendations. This product helps in sound absorption, contributing to a quieter indoor environment.

CLT-01
Item: Ceiling Lining – Type 01
Product Name: Plasterboard – Flush Set
Brand: Gyprock or Equivalent
Material: Standard Grade Commercial Plasterboard
Thickness: 13mm
Finish: Painted
Sheet Size: To suit application
Description: The plasterboard will be installed with a Level 5 finish. Junctions between plasterboard surfaces will be square set, and Rondo P50 shadow line junctions will be used for connections to non-plasterboard surfaces.

CLT-02
Item: Ceiling Lining – Type 02 Wet Areas
Product Name: Aquachek
Brand: Gyprock or Equivalent
Material: Moisture Resistant Plasterboard
Thickness: 13mm
Finish: Painted
Sheet Size: To suit application
Description: The ceiling lining in wet areas will have a Level 5 finish with square set junctions to other plasterboard surfaces and Rondo P50 shadow line junctions to non-plasterboard surfaces for a smooth transition.

PBL
Item: Plasterboard Wall Lining
Product Name: Plasterboard – Flush Set
Brand: Gyprock or Equivalent
Material: Standard Grade Plasterboard
Thickness: 10mm
Colour: Painted
Sheet Size: To suit application
Description: The plasterboard will be finished to a Level 5 finish, with square set junctions to other plasterboard surfaces and Rondo P50 shadow line junctions to non-plasterboard surfaces for seamless integration.

VBL
Item: Villaboard Wall Lining – Wet Areas
Product Name: Villaboard – Flush Set
Brand: James Hardie
Material: Fibre Cement
Thickness: 9mm
Colour: Painted
Sheet Size: To suit application
Description: The Villaboard will be installed with square set junctions to other plasterboard surfaces, providing a durable and water-resistant wall lining in wet areas.

	External cladding
	
9mm FC cladding to external walls on and including battening system. 

External cladding / battens and flashing to external bulkheads. 


	Roofing materials
	
Main Roof 
0.48mm Colorbond Ultra Spandeck roof sheeting 
Safety wire under roof sheeting 
Metal CL4 Colour coded fasteners 
Anticon 60mm R1.3 Insulation HD 
Thermoseal 733 Sarking 
Topspan 40 .75 Battens to Steel Framed Trusses 
0.55mm Colorbond Ultra Expansion Flashing 
0.55mm Colorbond Ultra Flashings to the roof 
250mm Half Round Colorbond Ultra Eaves Gutter, brackets, stop ends and droppers 
150mm dia PVC downpipe offsets to Eaves gutter 
dia Galvanised CHS downpipe Shoes to Eaves gutter 
Freespan Danpalon 16mm Polycarbonate roof sheeting system 
Access equipment and Cranage for roofing installation 
0.48mm Colorbond Ultra Spandeck Vertical Wall Cladding 
0.55mm Colorbond Ultra Flashings to wall cladding 
Topspan 40 .75 Battens to wall cladding 
Thermoseal 733 Medium Duty Sarking behind wall cladding 
Freespan Danpalon 16mm Multicell Polycarbonate wall cladding system 









Lower Roof 
0.48mm Colorbond Ultra Spandeck roof sheeting 
Safety wire under roof sheeting 
Metal CL4 Colour coded fasteners 
Anticon 60mm R1.3 Insulation HD 
Thermoseal 733 Sarking 
0.55mm Colorbond Ultra Flashings to the roof 
150mm Half Round Colorbond Ultra Eaves Gutter, brackets, stop ends and droppers 
100mm dia PVC downpipe offsets to Eaves gutter 
100mm dia Galvanised CHS downpipe Shoes to Eaves gutter 
Freespan Danpalon 16mm Polycarbonate roof sheeting system 
Access equipment for roofing installation 


Walkway Roof 
.48mm Colorbond Ultra Spandeck roof sheeting 
Safety wire under roof sheeting 
Metal CL4 Colour coded fasteners 
Thermoseal 733 Sarking 
.55mm Colorbond Ultra Flashings to the roof 
150mm Half Round Colorbond Ultra Eaves Gutter, brackets, stop ends and droppers 
100mm dia PVC downpipe offsets to Eaves gutter 
100mm dia Galvanised CHS downpipe Shoes to Eaves gutter 
Access equipment for roofing installation 

















Opinion of costs - for one (1) room identify costs of three (3) materials needed.
	Item
	Description (including size, thickness)
	Cost per Unit
	Quantity
	Total cost
	Construction method

	1
	Classroom 1- Flooring - vinyl sheet VIN-01 Tarkett Acczent Excellence 80 – colour Oak Tree Beige, thickness – Height: 10.71 metres. 
	$35.00 per m2
	110.4m2
	$3,864.00
	The construction method for Tarkett Acczent Excellence 80 vinyl sheet flooring involves a glue-down installation technique. This method ensures the vinyl sheets are securely adhered to the prepared subfloor using a high-performance adhesive, offering enhanced durability and stability. The seams are typically heat-welded, providing a seamless, watertight finish that improves the flooring’s resistance to moisture and wear. 

	2
	Classroom 1- Painting - 
Painting – Type 31, Colour: Winter Orange S11H8 

	$30.00 per litre
	212m2
	$6360.00
	The construction method for applying Type 31 Winter Orange S11H8 paint involves surface preparation, including cleaning and repairing any imperfections. A primer is applied, if necessary, followed by two coats of paint using a brush, roller, or spray system. The paint is left to dry between coats to achieve a smooth, durable finish.

	3
	Basin – type 03 - Brand Caroma 
	$507.32
	1
	$507.32
	The construction method for the installation of the Caroma Type 03 Basin begins with preparing the area by ensuring it is clean and verifying that all required plumbing connections, including water supply and drainage, are correctly positioned. The basin is then mounted using either a wall bracket or pedestal base, ensuring it is securely fixed and level with proper alignment. Following the mounting, the water supply lines are connected to the basin’s inlet valves, and the drain is sealed to prevent any leaks. Once the basin is installed, a thorough leak test is conducted to ensure proper functioning of all connections. Finally, the installation area is cleaned, and the basin is left ready for use.














Identify two (2) Prime Cost (PC) items and two Provisional Sum items
	Prime Cost items
	Provisional Sum items

	Nil
	Building Signage - $20,000.00

	
	Fixed playground equipment and soft fall base layer - $ 100,000.00 

	
	Irrigation - $ 32,000.00
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