Interim Test Report - Footing and Slab 
Site address:									
Date:										
Site Supervisor:									
Signature:									
The purpose of this report is to ensure critical aspects of the construction points are adhered to in accordance with AS2850 Slab and Footings and the National Construction Code Volume 2 – Part 3.2.5 Footing and Slab Construction

	Item
	Checkpoint
	Notes

	Boundary clearances
	☐ Setbacks to all relevant allotment boundaries and other buildings and structures
☐ Distances from easements and local government infrastructure
	

	Excavation of foundation material
	☐ Dimensions of excavations
☐ profile of soil excavated 
☐ Bearing surfaces of excavations.
	

	Compaction of fill material (if necessary)
	☐ Level of compaction
☐ Retention of compacted fill.
	

	Cut and fill batters
	☐ Location of cut and fill batters (required as part of the footing and slab system) 
☐ Construction and location of retaining walls (required as part of the footing and slab system) 
☐ Provisions for drainage of cut and fill batters and retaining walls
      falls to external finished areas.
	

	Piers through fill
	☐ Location of piers through compacted fill 
☐ Depth and bedding of piers through compacted fill to natural ground or in accordance with approved design requirements.
	


	Piers through fill
	☐ Location of piers through compacted fill 
☐ Depth and bedding of piers through compacted fill to natural ground or in accordance with approved design requirements.
	

	Reinforcement of slab and footing system
	☐ Type and placement of steel reinforcing 
☐ Size and gauge of reinforcing steel 
☐ Location and dimension of laps to    reinforcement steel.
☐ Type of connections to reinforcement steel
	

	Vapour barrier
	☐ Type and location of vapour barrier
☐ Type and location of joint overlaps to vapour barrier
☐ Treatment to penetrations through vapour barrier
	

	Termite management system
	☐ Location and type of physical and chemical barriers 
☐ Protection of penetrations through footing or slab elements
	

	Floor levels
	☐ Finished slab levels to establish heights above flood levels, building height or to accommodate drainage requirements.
	

	Slab inspection booked
	☐ Yes                                                                 ☐ No
	Booking date:

	Supporting photos/ documentation attached
	☐ Yes                                                                 ☐ No
	



