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BSBOHS201A 
Participate in OHS processes


	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances. 
Answers will be documented and FT003 (Oral examination declaration form) must be completed.
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· If a participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a participant changes their response in writing, they must put their initials next to the written change.
· If a participant changes their response verbally, this must be noted on the exam paper by the assessor.




	[bookmark: _Ref396827952]Participant name
	Sarah Durrant

	

	

	Participant signature
	



	Assessor name
	

	

	

	Assessor signature
	



	Date
	Click here to enter a date.



	Number of questions
	Number of questions answered correctly
	Satisfactory?

	24
	
	Yes
	No

	
	
		

	ASSESSOR COMMENTS

	


Match the terms and definitions by writing the appropriate letter next to each number in the centre column.

	Answer
	Terms
	Answers
	Definition
	
	
	1
	PRA
	1 - F
	A
	Outline the requirements of the work to be undertaken.
	

	
	2
	JSA
	2 - E
	B
	Outline what to do in the event of fires and other accidents
	

	
	3
	Plans and specifications
	3 - A
	C
	Contains important information about hazardous materials or chemicals.
	

	
	4
	Manufacturer specifications
	4 - D
	D
	Outlines how tools and equipment should be used (e.g. lubricant levels, maintenance requirements).
	

	
	5
	SDS
	5 - C
	E
	Identifies hazards and potential hazards that may be encountered while working.
	

	
	6
	Emergency procedures
	6 - B
	F
	A personal assessment of risk
	




[bookmark: _Ref424210309][bookmark: _Ref412796746]For each of the hazards identified below, describe the injuries/damage they may cause (i.e. to fellow workers, other people and/or animals) and suggest a suitable control measure.

	Answer
	Hazard
	Injuries or damage
	Control measure
	
	
	Hazardous chemical
	Respiratory damage, skin rashes and chemical burns
	Handle chemicals as per SDS guidelines, use PPE and store chemicals in a safe location
	

	
	Noise
	Hearing damage, headaches and fatigue
	Ensure adequate PPE is used or illuminate the object making the noise if possible
	

	
	Manual handling
	Strains and Sprains
	Follow correct manual handling procedures and use equipment to assist where possible
	




[bookmark: _Ref415045277]Who should you speak to if you find problems (e.g. hazards, accidents and emergencies)?

	Answer
	Supervisor, site/project manager
	


[bookmark: _Ref406591713]What should you do if you discover a fault with plant, tools or equipment?

	Answer
	Stop using the equipment 
Tag it out of service
Report it to your supervisor
Record the details of the fault 

	



[bookmark: _Ref424211517]Which legislation relates to safety in the workplace? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
	☐	Occupational Health and Safety Act 2015 
	

	
	☒	Work Health and Safety Act 2011 
	

	
	☐	Safety Act 1900 
	

	
	☐	Safety and Health Act 2011 
	




[bookmark: _Ref424211632]True or False (Tick your response): Employers are required by legislation to implement safety measures which are reasonably practicable.

	Answer
	☒	True 
	
	
	
	☐	False 
	
	




[bookmark: _Ref424211634]True or False (Tick your response): Workers are required by legislation to follow reasonable employer directives (e.g. to undertake first aid and/or fire safety training).

	Answer
	☒	True 
	
	
	
	☐	False 
	
	





[bookmark: _Ref424213216]The following symbols appear under the heading ‘Required PPE’ on an SDS. What do the symbols represent?

	Answer
	Symbol
	Meaning
	
	
	
[image: ]

	Protective clothing
	

	
	
[image: ]

	Gloves
	

	
	
[image: ]

	Eye Protection i.e safety glasses
	

	
	
[image: ]

	Respiratory Mask
	




[bookmark: _Ref408209094]Describe the meaning and use of the signs displayed below.

	Answer
	Sign
	Meaning
	
	[bookmark: _GoBack]
	[image: First aid.jpg]
	Location of First Aid Kit
	

	
	[image: Do Not Enter Saftety Sign]
	Warns off unauthorised persons from entering area

	

	
	[image: https://encrypted-tbn3.gstatic.com/images?q=tbn:ANd9GcRfZQGVU3BvP46nBERPIeqexiKuKX8OHW4dEmTYE6j-oAKUgPPkHw]
	Location of a Fire Fighting Facilities 
	





Refer to the Risk Matrix below when responding to Q10. to Q12. 

	Matrix
	A:
Death or permanent disability
	B:
Serious injury
	C:
Lost time injury
	D:
Casualty Treatment
	E:
First Aid

	1: Very Likely
	E
	E
	H
	H
	M

	2: Likely
	E
	H
	H
	M
	M

	3: Possible
	H
	H
	M
	M
	L

	4: Unlikely
	H
	M
	M
	L
	L

	5: Very Unlikely
	M
	M
	L
	L
	L



	E: Extreme
	H: High
	M: Medium
	L: Low




[bookmark: _Ref408921283]Which rating is designated for the highest risk and which rating is used for the lowest risk?

	Answer
	Highest Risk:  1:A
Lowest Risk:   5:E

	



[bookmark: _Ref408921265]What is the risk rating for the following circumstances: An event which is possible and would require low-level hospital treatment.

	Answer
	3:D
	



[bookmark: _Ref408921287][bookmark: _Ref412797660]What are the factors that would lead to a risk rating of E: Extreme?

	Answer
	A risk that is Very Likely resulting in Serious Injury, Death or Permanent Disability. A risk that is Likely resulting in Death or Permanent Disability
	



[bookmark: _Ref424212548]When should safety checks be undertaken on machinery and equipment? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
	☐	Before operation
	

	
	☐	After operation
	

	
	☒	Both before and after operation
	



[bookmark: _Ref408921427]Order the elements of the hierarchy of control, from 1 to 6 (i.e. most effective to least effective).


	Answer
	Label (1 – 6)
	Element
	
	
	3
	Isolate the hazard
	

	
	6
	Provide and use Personal Protective Equipment (PPE)
	

	
	1
	Eliminate the hazard
	

	
	4
	Control the hazard by engineering means
	

	
	5
	Control the hazard by administrative means
	

	
	2
	Substitute the hazard
	




[bookmark: _Ref408921430]Why is elimination the best method of hazard control and PPE considered the least effective?

	Answer
	Eliminating the hazard removes the risk entirely and the use of PPE allows the hazard to continue but uses safety equipment to minimilise the risk.
	



[bookmark: _Ref408921432]If you were to replace a flammable solvent with a water-based solvent, what category of control measure would that be under the hierarchy of control?

	Answer
	Substituting the Hazard
	


[bookmark: _Ref401921251][bookmark: _Ref401900343]

[bookmark: _Ref401922320]In the diagram below a person is lifting a tool box.
Filling in the table, indicate how each body part should be used/placed. 
[image: lifting]F. Hands
E. Knees
D. Shoulders
C. Feet
B. Back
A. Neck

	Answer
	Area of body (Letter)
	How it should be placed
	
	
	D
	Level
	

	
	B
	Upright
	

	
	F
	Good grip
	

	
	A
	Natural curve
	

	
	E
	Bent
	

	
	F
	Flat, facing load
	




[bookmark: _Ref415049799][bookmark: _Ref421093133]In a medical emergency, what is the first step in the DRSABCD action plan that you need to follow?

	Answer
	Danger Checked
	



[bookmark: _Ref421092991]In the event of a fire emergency, what should you do? 
Fill in the table below to explain the acronym R.A.C.E.

	Answer
	Letter
	Meaning
	
	
	R
	Remove people from immediate danger
	

	
	A
	Alert people of emergency
	

	
	C
	Confine Fire and Smoke
	

	
	E
	Evacuate to the assembly area
	



[bookmark: _Ref414952615]What should you do as part of the clean up process? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
	☐	Store all plant, tools and equipment without cleaning
	

	
	☒	Maintain plant, tools and equipment
	

	
	☒	Dispose of materials that cannot be reused or recycled
	

	
	☒	Report faults in logbook and/or site records
	

	
	☒	Clean all plant, tools and equipment before storage
	




[bookmark: _Ref408921186]Read the scenario below and complete the Hazard Report Form.

SCENARIO
Today at 10:45am a delivery truck reversed into a car park (located at 54 Standish Street, Salisbury) to deliver gardening materials. There was nobody in the car park to guide the driver and he backed into a number of drums of diesel located to the left of the photograph (below).  One drum was pierced and its contents erupted from the container. 

The marked area on the photo represents the diesel spill, measuring 3m x 4m.











HAZARD REPORT FORM

	GENERAL

	Date
	7th January 2018

	Submitted by
	Sarah Durrant

	HAZARD DETAILS

	Location
	54 Standish Street, Salisbury

	Description of issue
	Truck ran into Drums of 205 Diesel located at the carpark location listed above and pierced one of the drums resulting in a 3x4m spill.

	Risk class
	☐  Extreme
	☒  High
	☐  Medium
	☐  Low

	CONTROL MEASURES

	Corrective action required 
	Notify the Supervisor as soon as possible. Spill required to be contained, soaker bunded, cordoned off from the public and cleaned up. Signs to direct delivery drivers should be installed for times that the carpark is left unattended by workers. The 205 drums should be actioned to be stored on a bunded pallet

	Person to action
	Personnel on Hand and Supervisor to be Notified
	When
	☒  Immediately
☐  Within 24 hours
☐  Within 7 days



	Answer
	
	


[bookmark: _Ref412803069]Who would you submit a hazard report form to?

	Answer
	Supervisor, site/project manager
	



[bookmark: _Ref412803089]Who would approve proposed risk controls and organise the required resources for implementation of the risk control?

	Answer
	Supervisor, site/project manager
	



[bookmark: _Ref424215038]Identify one (1) way you can assess if risk controls have been effective.

	Answer
	The hazard has been illuminated and there has been no further instances occur
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