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CPCCBC4006B 
Select, procure and store construction materials for low rise projects
ASSESSMENT SUMMARY

The assessment activities for CPCCBC4006B Select, procure and store construction materials for low rise projects cover all aspects of the unit of competency required. To demonstrate competence in this unit, a participant must undertake all tasks and complete them satisfactorily and consistently. For Apprentices and Trainees, this includes employer completion of the Employer Record Book (ERB). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be equitable, fair and flexible. If a participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a participant does not answer some questions or perform some tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. The Trainer/Assessor is able to provide the participant with additional information on interpreting the assessment outcomes and provide guidance on the participant’s options. Should a participant still be deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result. 

By signing the cover page for each assessment item, the participant acknowledges they understand the assessment instructions and requirements and consent to being assessed. The participant also verifies and assures the RTO that the work submitted is their own work. 


	Participant Name
	Christine Muter




	Task
	Assessment Results 

	Theory Exam
	 Satisfactory 
	 Not Yet Satisfactory

	Practical Assessment
	 Satisfactory 
	 Not Yet Satisfactory

	Outcome for Unit of Competency
	 Competent
	 Not Yet Competent




	Assessor Name
	

	Assessor Signature
	
	Unit Competence Determination Date
	Click here to enter a date.
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	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances, whereby the Participant’s answers will be documented by a party other than the Participant. This must be acknowledged in writing (e.g. FT001 and Assessor Comments)
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· Assessors are to complete marking in pen of a different colour to the Participant.
· If a Participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a Participant changes their response in writing, they must put their initials next to the written change.
· If a Participant changes their response verbally, this must be noted on the exam paper by the assessor.




	Participant name
	Christine Muter

	
	

	Participant signature
	
	
	

	Date
	21/12/2021



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.




	Number of questions
	Number of questions answered correctly
	Task outcome (Tick)

	44
	
	Satisfactory
	Not Yet Satisfactory

	
	
	
	


	ASSESSOR COMMENTS

	


Q1.  Which of the following documents and/or people would you refer to when selecting materials for a building project? Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
		Australian Standards
	

	
		Contract
	

	
		Drawings
	

	
		Manufacturer
	

	
		National Construction Code
	

	
		Specifications
	

	
		Tolerances
	




Q2.  [bookmark: _Ref427235149]Identify the Volume and Parts of the NCC that relate to suitability of materials for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	Volume1 Part A5
	Volume 2 Part A5.
	




Q3.  [bookmark: _Ref535482367]Identify the assessment methods used to verify a performance solution.

	Answer
	The “Deemed to Satisfy” method showing Evidence of suitability and Expert judgement
 The “Performance solution” method showing , evidence of suitability, A verification method and expert judgement
 And  a comparison with the Deemed-to-Satisfy provisions 
 
	




Q4.  [bookmark: _Ref496611564][bookmark: _Ref536083431]Which of the following solutions for material selection often references the Australian Standards? Tick your response.

	Answer
	Choice
	Possible Answers
	

	
		Deemed-to-Satisfy solution
	

	
		Performance solution
	




Q5.  [bookmark: _Ref425255684]Identify five (5) materials commonly used for low rise buildings in your region. For each material, identify the following:
· Its name
· Properties of the material

	Answer
	#
	Material name
	Properties
	

	
	1
	Timber
	It is a generic building material and is used in building because:
-Different structures can be built in most climates
- Timber is very flexible under loads, keeping strength while bending
- It is incredibly strong when compressed vertically
There are many types so specific species are better for various uses than others 

	

	
	2
	Ceramic
	Ceramics are such things as tiles and fixtures which are used as floor and walls coverings in buildings, including ceramic floors and walls, counter-tops and ceilings.
Ceramics used to be a specialized form of clay-pottery firing in kilns, but it has evolved into more technical areas and its application to more modern day designs
	

	
	3
	Concrete
	Concrete is a composite building materials made from the combination of aggregate (composite) and a binder, i.e. Cement and it has been the predominant building material in today’s modern age due to its longevity, formability, and ease of transport and is extremely cost effective
	

	
	4
	Brick
	Bricks are blocks made of kiln-fired material, usually clay or shale, but also may be of lower quality mud, etc. And is considered to be a durable material. 

	

	
	5
	Glass
	A natural material - Clear windows have been used since the invention of glass to cover small openings in a building. 
They provided people with the ability to both let light into rooms while keeping inclement weather outside. Glass is generally made from mixtures of sand and silicates, and is very brittle.
	





Q6.  [bookmark: _Ref425323073][bookmark: _Ref425248000]For each of the materials in Q5. identify the following:
· Quality of the material (i.e. durability, serviceability, cost effectiveness)
· Compatibility and non-compatibility of the material (i.e. what it would/would not be suitable for)

	Answer
	#
	Quality
	Compatibility 
	     

	
	1
	Timber is readily available and as such is a cost effective building material 
	Timber in construction is generally used for framing and  support beams in walls and roofs, it is however susceptible to elements like water and to pets/termites so would need to be treated, and not to sit in or around water  
	

	
	2
	The use of ceramics such as ties offer a hard surface or areas such as floors and walls, the range available is large and the cost can be from as little as $20 s meter to those that are more expensive decorative/imported tiles. 
	Tiles provide a surface that is more durable than carpet and is easier to clean, especially in high traffic areas and bathrooms, however incorrectly laid tiles without the correct preparation can lead to them cracking as they are a brittle material. 
	

	
	3
	Concrete is a material that is mostly used to lay the base/ foundation of a building site  as it offers strength and durability, due to the labour and processing required to make concrete it can be costly 
	Being a fluid mix, concrete has limitations to the materials until it has been formed and allowed to set, once set it can be used for several things other than for the slab of a site, it can be formed into sleepers, driveway edging, pillars
	

	
	4
	Bricks have evolved from being
created from simple mud / clay
by hand into the more
commonly known material used
in construction today by
colouring and cutting them to
size in mass production. Bricks
are fire resistant and so are
suitable for exterior and interior
walls. They require a fair
amount of energy to produce
are not the cheapest material
however offer long term
durability  
	They do need reinforcing to
provide additional strength if
being used for such a
construction as a retaining wall
	

	
	5
	Glass required minimal
processing and is considered to
be one of the Natural building
materials, however is
considered brittle and is not a  great product when it comes to
insulation against the heat and
the cold
	Ideal for covering small and
large openings in the structures
allowing light to enter, not so
ideal for any structure requiring
less light and more durability
	



Q7.  [bookmark: _Ref536083435]Identify five (5) physical characteristics that may be considered when evaluating potential building materials.

	Answer
	Strength
Electrical conductivity
Thermal conductivity and capacity
Moisture absorption
     Acoustics
	




Q8.  [bookmark: _Ref536095924]Match the terms and definitions below by writing the appropriate letter next to each number in the centre column.

	Answer
	Term
	Answers
	Definition
	

	
	1
	Carbon footprint
	1 -B
	A
	The amount of energy required to manufacture a product
	

	
	2
	CO2e
	2 -E
	B
	Total GHD emissions produced during manufacture construction and use
	

	
	3
	Embodied energy
	3 -A
	C
	Greenhouse gas emissions
	

	
	4
	Embodied water
	4 -D
	D
	The amount of water required to manufacture a product
	

	
	5
	GHG
	5 -C
	E
	CO2equivalent tonnes emitted into the atmosphere
	




Q9.  [bookmark: _Ref536083463]Which of the following materials would be considered as ‘low energy content’? Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
		Bricks
	

	
		By-products of other industrial processes
	

	
		Cement
	

	
		Glass
	

	
		Metals
	

	
		Plastics
	

	
		Sand
	

	
		Stone
	

	
		Timber
	



Q10.  [bookmark: _Ref536099133]Refer to the table below and identify the wall material type that has the smallest embodied energy and emission impact.

[image: ]

	Answer
	Timber frame fibro clad
	





Q11.  [bookmark: _Ref536095926]Identify the Volume and Parts of the NCC that relate to energy efficiency of materials for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	Volume 2 Section 2 Part 3.12
	Volume 1 section J Part J1.2
	




Q12.  [bookmark: _Ref536097820]Identify the relevant section of the Standards and Tolerances Guide and the associated Australian Standard that addresses residential slabs and footings.

	Answer
	Standards and Tolerances Guide
	Australian Standard 
	

	
	Part 3
	AS 2870
	




Q13.  [bookmark: _Ref536097822]Identify the relevant section of the Standards and Tolerances Guide and the associated Australian Standard that addresses roof tiles.

	Answer
	Standards and Tolerances Guide
	Australian Standard 
	

	
	Part 7.4
	AS2049 and AS2050
	




Q14.  [bookmark: _Ref536106144]Identify the Volume and Parts of the NCC that relate to safety barriers for swimming pools for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	 Volume 2 part 3.10.1 
	Volume 1 Part G1 - GP1.1 
	




Q15.  [bookmark: _Ref536106145]In some states, barriers and fences for swimming pools are not entirely regulated by the NCC, as noted in the Ancillary Provisions and State and Territory Variations. Identify the applicable Act and Regulation that regulate safety barriers for swimming pools in your jurisdiction.

	Answer
	Qld development code Mandatory Part  3.4  Special buildings and in accordance with Australian standard AS 1926.1 and AS 1926.2
	



Q16.  [bookmark: _Ref536106146]Identify the Australian Standard that relates to safety barriers for swimming pools.

	Answer
	Australian Standard AS 1926.1 – 2012
	




Q17.  [bookmark: _Ref536107455]True or False (Tick your response): According to the Standard in Q16. all gates must be fitted with a self-closing device that will return the gate to a closed position from any position without the use of manual force.

	Answer
		True 
	
	

	
		False 
	
	




Q18.  [bookmark: _Ref536170034]Identify the Volume and Parts of the NCC that relate to fire-resistance of building elements for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	

	
	Volume 2 Schedule 5
	Volume 1 Section C
	




Q19.  [bookmark: _Ref536170036]Identify the Australian Standard that relates to fire-resistance tests for elements of construction.

	Answer
	Australian Standards AS 1530.4 and AS4072.1
	




Q20.  [bookmark: _Ref536169328]For all NCC Classes, where the ground or subfloor space is excessively damp or subject to frequent flooding, which durability class must the subfloor framing must be used where above ground?

	Answer
	Durability class 1 or 2 or H3 preservative treated timbers 
	





Q21.  [bookmark: _Ref536170040]Identify the Australian Standards that must be observed when meeting the requirements for Q20. 

	Answer
	AS 1684.2, AS 1684.3
	




Q22.  [bookmark: _Ref536170043]True or False (Tick your response): Where materials are not used as intended (or without considering NCC requirements), this can make a significant difference to the life or serviceability of the structure.

	Answer
		True 
	
	

	
		False 
	
	




Q23.  [bookmark: _Ref536170044]Explain why durability and serviceability impact on the cost effectiveness of chosen materials.

	Answer
	Different materials all have various degrees of durability and strength. The more durable and resistant to elements such as moisture or attack form pests are generally more expensive however provide a better long term durability for the structure  
	




Q24.  [bookmark: _Ref536172033]Provide an example of short term degradation of materials and describe its effects on a building on structure.

	Answer
	The use of certain stone such as limestone can degrade in the short term as it is considered to be a softer rock. Constant exposure to the wind and the rain will erode the surface or and if exposed to colder climates can crack and break it.
	





Q25.  [bookmark: _Ref536172034]Provide an example of long term degradation of materials and describe its effects on a building on structure.

	Answer
	Corrosion in metal is a long term degradation process that occurs when metal is exposed to liquid, this results in oxidation which causes rust to form. This will lead to impacting the strength of the material compromising the strength it was designed for. 
	




Q26.  [bookmark: _Ref425327163][bookmark: _Ref425327708]You have spoken to a supplier who has indicated that some of the client’s desired materials are unavailable. When considering alternative building materials what must be taken into consideration (i.e. other than the client’s requirements)?

	Answer
	Short and long term degradation
Compatibility
Environmental impact
Transportation
Life-Cycle cost
Fire resistance rating

	




Q27.  [bookmark: _Ref536177031]Identify two (2) things that you should look for when receiving a delivery of materials.

	Answer
	Confirm the quantity ordered is what is being delivered by inspecting the package
The condition of the goods that are being delivered are in perfect condition 
	




Q28.  [bookmark: _Ref536177032]If you encounter issues with delivery, what two (2) options do you have?

	Answer
	Reject the delivery if the damage is extensive
Prepare for the delay in receiving the replacement items 
	




Q29.  [bookmark: _Ref409518704][bookmark: _Ref408838393]Which of the following should be assessed before shifting materials? Tick all that apply. 

	Answer
	Choice
	Possible Answers
	

	
		What needs to be relocated (e.g. size, weight)
	

	
		The relocation area, site layout and obstacles
	

	
		Distance and time to relocate load
	

	
		Whether a team is available and/or appropriate
	

	
		Whether PPE must be worn (e.g. for hazardous materials)
	




Q30.  [bookmark: _Ref536178585]What document should you refer to for guidance on how to handle and store hazardous chemicals? 

	Answer
	Safety Data Sheet
	




Q31.  [bookmark: _Ref408838395][bookmark: _Ref409519364]Name three (3) ways you can reduce the risk of injury if a load is too heavy for one person to carry, push or pull. 

	Answer
	Team lift, lighten the load and use a mechanical aid
	





Q32.  [bookmark: _Ref401922320]In the diagram below a person is lifting a tool box.
Filling in the table, indicate how each body part should be used/placed. 
 (
F. Hands
) (
E. Knees
) (
D. Shoulders
) (
C. Feet
) (
B. Back
) (
A. Neck
)[image: lifting]
	Answer
	Area of body (Letter)
	How it should be placed
	

	
	D
	Level
	

	
	A
	Upright
	

	
	F
	Good grip
	

	
	B
	Natural curve
	

	
	E
	Bent
	

	
	C
	Flat, facing load
	




Q33.  [bookmark: _Ref404158235]How should construction materials and components be handled? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
		Sorted to suit material type and size, separating hazardous material
	

	
		Stacked or stockpiled for ease of identification and retrieval
	

	
		Stored in access ways for ease of retrieval
	

	
		Stored clear of access ways
	

	
		Handled and positioned ready for installation
	




Q34.  [bookmark: _Ref536180244]Identify the Australian Standard that relates to the storage and handling of LP gas.

	Answer
	Australian Standard AS/NZ 1596:2008
	



Q35.  [bookmark: _Ref536194481]List one (1) testing method for each of the building materials listed below.

	Answer
	Material name
	Properties
	

	
	Concrete
	Concrete is tested on site (the slump test
	

	
	Metals
	The strength of metals is reduced if they are repeatedly loaded alternately in tension and compression. This test is called ‘repeated loading’ if the load is applied several hundred or thousands of times, and fatigue loading if the load is applied millions of times
	

	
	Timber
	Timber is tested by the use of a grading machine which tests every individual piece of timber using a very fast and method. Each piece of timber is deflected at several points along its length, and the deflection category marked by means of a spot of dye. The timber is then classified visually by these markings. 

	




Q36.  [bookmark: _Ref536181364]What Code gives detailed tables which state the required grade of timber for specific sizes and uses?

	Answer
	 The Australian Timber Framing Code
	




Q37.  [bookmark: _Ref536181366]Name two (2) ways that defects may be seen in timber.

	Answer
	Splits in the timber  and insect damage
	




Q38.  [bookmark: _Ref536181368]Identify two (2) tests that may be performed to determine the durability of stone.

	Answer
	acid immersion and  a porosity test
	



Q39.  [bookmark: _Ref536181370]Name two (2) ways that defects may be seen in stone.

	Answer
	cracks and fissures in the stone
	




Q40.  [bookmark: _Ref536187863]True or False (Tick your response): Under a contract, builders and other specialist tradespersons are the ones most likely to rectify or remedy problems that arise from incorrect installation, application or placement of materials.

	Answer
		True 
	
	

	
		False 
	
	




Q41.  [bookmark: _Ref536187427]Name two (2) established methods that may be used to preserve timber.

	Answer
	Applying paint  and impregnating wood with chemicals which are toxic to fungi and insects 
	




Q42.  [bookmark: _Ref536187429]Identify two (2) established methods that may be used to protect ferrous metals.

	Answer
	Applying epoxy paint systems or galvanising
	





Q43.  [bookmark: _Ref536187430]Explain why the corrosion resistance of non-ferrous metals is superior to that of ordinary steel.

	Answer
	Iron and steel are reactive metals which oxidise in the atmosphere to form rust. The control and prevention of any corrosion results in requiring an additional process that can reduce or eliminate this reaction however add costs.
Non-ferrous metals are more expensive however they are also more resistant to corrosion 
	




Q44.  [bookmark: _Ref536187432]When should aluminium be coated with bituminous paint? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	

	
		At all times
	

	
		When it is buried in soil
	

	
		When it comes in contact with chemical materials
	

	
		When it is immersed in water
	

	
		When it is used on bitumen
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	PRACTICAL ASSESSMENT INSTRUCTIONS

· The following practical assessment will require the Participant to complete work related activities.
· The Assessor will conduct observations of the Participant’s work to determine whether they display sufficient practical skills and knowledge. 
· Please fill in the details below – providing your name, signature and date of assessment.
· The Participant’s signature acknowledges that the Assessor provided clear instructions and the Participant understood what was required to complete this assessment.
· The Assessor may substitute a Practical Task with an alternate task of equal value.
· Alternate tasks must be fully documented by the assessor in the Assessor Comments area.





	Participant name
	Christine Muter

	
	

	Participant signature
	
	
	

	Date
	21/12/2021



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.





	Task
	Task outcome (Tick)

	
	Satisfactory
	Not Yet Satisfactory

	Task 1 (Occasion 1)
		
	Task 1 (Occasion 2)
		



	ASSESSOR COMMENTS

	


CPCCBC4006B
Select, procure and store construction materials for low rise projects

	Practical Task 1 (2X)

	Description of task:
On two (2) occasions, a suitable observer is to verify the participant’s ability to supervise systems through which materials are selected, acquired and stored on site for the following projects:
· Occasion 1: Construction classified as Class 1 and 10 construction
· Occasion 2: Construction classified in Classes 2 to 9 with a gross floor area not exceeding 2000 square metres, not including Type A or Type B construction

The participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. Evidence to be submitted may include: 
· Copy of PO sent to site team for materials.
· Email correspondence sighting need for materials, delivery of materials and storage of materials (if relevant).

The observer is to provide detailed comments on the tasks completed by the participant. The assessor is to verify the observer’s comments in the Assessor Comments section, and provide the Practical Assessment outcome on the front cover of this document.

	Resources required: 
Computer, Building Contract, Drawings, Specifications, Building materials (including timber, and ferrous and non-ferrous metal).

	Assessment of task

	Name of participant:
	Christine Muter

	Name of observer:
	John Gammon

	Role of observer 
(Confirm suitability to sign)
	Construction Manager

	Email address of observer
	John.gammon@tbs.com.au

	Signature of observer:
	
	Date:
	21/12/2021

	[bookmark: _GoBack]When completing the task, did the participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	
	1st
Occasion
	2nd
Occasion

	1 Evaluate building materials

	1.1A.  [bookmark: _Ref535842396]Identify suitability of materials commonly used in the region for low rise buildings. 
	TBS don’t often carry out large rectification works on commercial projects
	

	1.1B.  [bookmark: _Ref535842402][bookmark: _Ref536020766]Through research and testing, identify properties of different materials, their quality and compatibility and non-compatibility and maintain effective sampling and organisational record-keeping processes.
	TBS don’t often carry out large rectification works on commercial projects
	These are carried out by TBS elected engineers 

	1.1C.  [bookmark: _Ref535842408]Identify the environmental impacts of different materials. 
	TBS don’t often carry out large rectification works on commercial projects
	

	1.1D.  [bookmark: _Ref535842411]Identify the impact of allowable tolerances on the conversion of naturally occurring materials. 
	TBS don’t often carry out large rectification works on commercial projects
	Confirmed by one on one discussions with Christine

	1.1E.  [bookmark: _Ref535842424]Identify and check tolerances for installing and assembling materials with regard to the nature of the work being performed and the requirements of relevant construction industry Australian standards. 
	TBS don’t often carry out large rectification works on commercial projects
	Confirmed by one on one discussions with Christine

	2 Material selection 

	1.2A.  [bookmark: _Ref535842432]Select materials structurally adequate and appropriate for the building system specified in the contract, drawings and specifications. 
	TBS don’t often carry out large rectification works on commercial projects
	

	1.2B.  [bookmark: _Ref535842436]Select materials after considering:
· Safety
· Required fire resistance rating
· Suitability to the application
· Durability
· Serviceability and cost effectiveness
· Compliance with NCC, legislation, regulations and Australian Standards
	TBS don’t often carry out large rectification works on commercial projects
	

	1.2C.  [bookmark: _Ref535842439]Consider short and long-term degradation of materials in relation to the building’s proposed life cycle. 
	TBS don’t often carry out large rectification works on commercial projects
	Confirmed by one on one discussions with Christine

	1.2D.  [bookmark: _Ref535842441][bookmark: _Ref536188601]Select and evaluate alternative materials, if specified materials were unavailable or unsuitable – justifying decisions to regulatory authorities, as necessary
	TBS don’t often carry out large rectification works on commercial projects
	Confirmed by one on one discussions with Christine

	1.2E.  [bookmark: _Ref535842446]Finalise selection of materials in accordance with contractual requirements and in consultation with relevant professionals and the client, compiling results in a report.
	TBS don’t often carry out large rectification works on commercial projects
	Confirmed by one on one discussions with Christine

	1.2F.  [bookmark: _Ref535842459]Effectively communicate using the following methods:
· Language/concepts appropriate to cultural differences
· Non-verbal communication
	TBS don’t often carry out large rectification works on commercial projects
	

	3 Supervising materials on site 

	1.3A.  [bookmark: _Ref535842490]Determine limitations and effects of transportation on material and components, taking action in potentially damaging circumstances. 
	TBS don’t often carry out large rectification works on commercial projects
	

	1.3B.  [bookmark: _Ref535842494]Ensure materials were correctly and safely handled on site using appropriate equipment and safe work practices. 
	TBS don’t often carry out large rectification works on commercial projects
	

	1.3C.  [bookmark: _Ref535842471]Communicate with manufacturers and suppliers to ensure materials are stored in accordance with specifications and Australian standards. 
	TBS don’t often carry out large rectification works on commercial projects
	

	1.3D.  [bookmark: _Ref535842501]Implement processes for inspecting all materials delivered on site for naturally occurring and/or manufactured defects before installation. 
	TBS don’t often carry out large rectification works on commercial projects
	

	1.3E.  [bookmark: _Ref535842506]Ensure personnel were aware of actions to be taken in the case of defects caused by incorrect installation, application or placement. 
	TBS don’t often carry out large rectification works on commercial projects
	

	1.3F.  [bookmark: _Ref535842510]Preserve and protect timber and ferrous and non-ferrous metal used in the construction process.
	TBS don’t often carry out large rectification works on commercial projects
	

	The Participant’s performance was:  Satisfactory     Not Satisfactory





	OBSERVER COMMENTS

	Although the company is primarily an Insurance builder, we do stipulate the types of materials that our trades are required to use to complete the works required.

Christine is proficient in sending purchase orders outlining the types of materials required to carry out works and is also required to liaise with trades in identifying any on site delivery requirements for each project. Christine also has a strong understanding in the process/ steps of each project from the demolition state to final Completion and the correct order that each must be carried out in order for the project to be completed on time and within budget, some examples can be forwarded if required.

In regards to the type of material best suited for the works, we are restricted in relation to insuring a “like for like” replacement, this is stipulated when carrying out work for an insurance company. If the area of a property requires to be changed in accordance with any new changes to legislation however – i.e. roof batten upgrades, TBS will then identify the type of material to best use in accordance with the Australian standards, advise the insurance company of this requirement and implement this as part of our Scope of Works for the project. 

 

 




CSTC Pty Ltd_RTO#0699_v1-4_02/10/2019	Page 5 of 6
image2.jpeg




image3.png
Kg

o2l
COMPONENT Wwm2 | m2
indoor | indoor
floor area | floor area
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Floor suspended timber on stumps 76 2
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length
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