
Job Scopes and specifications

Before work commences pool to be covered with soft and hard cover 

Deck Board Type - Brite Deck Titanium in Willow Oak 140mm x 29mm  x 6 m in length
All Steel work as per engineering drawings  (Hot dip Galvanised Cyclonic Rated)
Pool Fencing Aluminium Powder coated - single rail top and bottom (50 x 50 Post)
F14 H4 Structure Timber

Work Outline

Main Pool Section (Before the walk path)

Demolition Work
Decking Boards
Screening located around toilets and pool pump
Pool fencing
Framing
Posts
Bearer & Joists
Remove deck and under structure & Repack the ground
Cart away removed materials and debris from site

WHS Standard fence and compliance

Plumbing and Electrical Works
BBQ Pool Pump, filter and heater removed, stored and later re-instated.
Street lamp removed and re-instated or worked around and re-instated.

Main Pool Work Scopes
Decking
Supply and install Decking board in Brite Deck Titanium in Willow Oak 140mm x 29mm  x 6 m in length
Decking board to picture frame the exterior top edge of the deck
Concealed T clip system to secure the decking boards to the frame
Matching Fascia Boards to conceal the ends of joists
Include removable access panel through deck to storm water manhole where marked on drawings.  
Joist/Bearer tape to be applied to all top edges of horizontal members including joists, bearers for moisture protection before decking is installed.
Install conduit piping under decking boards for future use to carry cables – to run from store room in toilet block to lamp post at pool gate on north side (Maryvale Street) and to run from store room in toilet block to lamp post  at pool gate on south side (Jephson Street). 

Under-structure of Deck to be built as per engineers drawings
Deck frame to be supported with 75 x 75 x 4 mm SHS posts as per engineering drawings

New  pool fencing, gates and steps
Aluminium Powder Coated Green Pool Fence 1200mm high Panels and  maximum of 2450 mm long
Pool fence posts 50 x 50mm
Posts to be bolted to side of deck frame to suit the 1200 m high panels.
All brackets attached to posts and panels attached to bracket with short tek screws 
Seven pool gates as per drawings 1200mm high with tensioned hinges and pool safe magna lock

New steps near pool hut to garden area - hardwood timber treads on propriety hot dipped galvanised steel stringers
Suitable hand rail/balustrade for steps to match pool fencing 

Steps near pool equipment to be re-instated

Privacy Screens
Powder  coated aluminium privacy screens to screen toilets and pool equipment 
Privacy screens to be horizontal slatted - 65mm x 16.5mm  “surf mist” colour (match pool hut)
Aluminium posts for screening to have a receiving channel to finish off ends.  
Monel pop-rivets to be used.


Pool Hut – Shade Structure - Pergola
Supply and install pool hut/shade structure as shown on plans
Materials for pool hut/shade structure as per quote from Delta but adjusted to accord with plans
Four back posts of pool hut /shade structure part of the under-structure  - to run from ground to roof -  to be painted Cottage Green - as per engineer drawings - SC2 75x75x 4SHS Hot dipped galvanised.
Roof of pool hut/shade structure to be Delta Orb  with 75mm insulation
Insulated roof panel 75mm thick 4500mm long x 1000m wide top side Delta Orb profile surfmist -
under side of roof - flat profile colour surfmist installed to manufacturers specifications.
Fascia, 125mm Squareline Gutter and Trims  - to be painted Cottage Green
Roof beam to manufacturer's specifications.
[bookmark: _GoBack]Bracing to engineers specifications.  Diagonal  bracing to be galvanised hot dipped steel round bar. 
Insulated wall panels behind the BBQ to be insulated flat panels to a height of 1500
Above wall panel - Aluminium powder coated panel slats - horizontal slatted - 65mm x 16.5mm - “surf mist” colour.
Aluminium posts for screening to have a receiving channel to finish off ends.  
Monel pop-rivets to be used.
Behind BBQ - tiled splashback area using off-white 600h x 300w tiles
Lighting for pool hut/ shade structure as per drawings
1200 Twin LED tube batten lighting (with replaceable LED Tubes - WEATHERPROOF
All wiring concealed - to be contained in ceiling panels
3 x Light Switch as per drawings
2 x double GPO - WEATHERPROOF- 1100 mm above floor level

Re-instate  BBQ in  new pool hut/shade structure

Re-instate pool heater,  pool pump and filter
Re-instate Street Lamps

Re-Board Existing Walk Paths
New decking board - Brite Deck Titanium Willow 
Matching Fascia Boards to conceal the ends of joists
Concealed T clip system to secure the decking boards to the frame
Supply and install new fencing (to match  pool fencing) posts to be bolted to the side of bearers
Fence to be affixed to cream posts and small brick wall in 2 locations as indicated on drawings
Small wooden access gate to be replaced with powder coated aluminium gate to match fencing.


STANDARD CERTIFICATION PERMIT (if required)
Certification including 1 inspection and a Form 21 on completion.
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