 Material Delivery Documentation 

	Completed by
	Noreen Abu-Obeid

	Date completed
	11/7/2023

	Supplier
	WinDoSupplier **(not named for confidentiality purposes.  Thank you)



	Items
	Size
	Thickness (mm)
	Quantity (pcs)
	Requirements met
	Delivery

	
	Height (mm)
	Width (mm)
	
	
	Serviceability
	Suitability
	Durability
	Met in Qty and Qlty

	Category 1: Doors 
	

	Entry 
	2400
	1500
	40
	1
	Y
	Y
	Y
	Y

	Garage
	2400
	720
	40
	2
	Y
	Y
	Y
	Y

	Garage 
	2400
	5210
	40
	1
	Y
	Y
	Y
	Y

	Media room 
	2400
	820
	35
	1
	Y
	Y
	Y
	Y

	Bathroom
	2400
	820
	35
	1
	Y
	Y
	Y
	Y

	Living room
	2500
	6000
	35
	1
	Y
	Y
	Y
	Y

	Pantry
	2400
	820
	35
	1
	Y
	Y
	Y
	Y

	Laundry
	2400
	720
	35
	1
	Y
	Y
	Y
	Y

	Study
	2400
	820
	35
	1
	Y
	Y
	Y
	Y

	Study
	2400
	1000
	35
	1
	Y
	Y
	Y
	Y

	Bedroom 4
	2400
	820
	35
	1
	Y
	Y
	Y
	Y

	Bedroom 4
	2400
	720
	35
	1
	Y
	Y
	Y
	Y

	Bathroom
	2400
	720
	35
	1
	Y
	Y
	Y
	Y

	Bedroom 3
	2400
	3000
	35
	1
	Y
	Y
	Y
	Y

	Bedroom 3
	2400
	1200
	35
	1
	Y
	Y
	Y
	Y

	Bedroom 2
	2400
	820
	35
	1
	Y
	Y
	Y
	Y

	Bedroom 2
	2400
	2450
	35
	1
	Y
	Y
	Y
	Y

	Master bedroom
	2400
	820
	35
	1
	Y
	Y
	Y
	Y

	Wardrobe
	2400
	820
	35
	1
	Y
	Y
	Y
	Y

	Ensuite
	2400
	820
	35
	1
	Y
	Y
	Y
	Y

	Category 2: Windows
	
	
	
	
	Y
	Y
	Y
	Y

	Entry
	600
	3000
	3
	2
	Y
	Y
	Y
	Y

	Dining
	2700
	900
	3
	1
	Y
	Y
	Y
	Y

	Laundry
	1200
	600
	3
	1
	Y
	Y
	Y
	Y

	Study
	1200
	600
	3
	2
	Y
	Y
	Y
	Y

	Stair area
	1200
	900
	3
	1
	Y
	Y
	Y
	Y

	Stair area
	1200
	700
	3
	1
	Y
	Y
	Y
	Y

	Stair area
	2400
	900
	3
	5
	Y
	Y
	Y
	Y

	Master bedroom
	600
	900
	3
	1
	Y
	Y
	Y
	Y

	Master bedroom
	600
	1500
	3
	1
	Y
	Y
	Y
	Y

	Master bedroom
	2400
	900
	3
	1
	Y
	Y
	Y
	Y

	Master bedroom
	2400
	1500
	3
	1
	Y
	Y
	Y
	Y

	Ward robe
	300
	3000
	3
	1
	Y
	Y
	Y
	Y

	Ensuite
	2400
	600
	3
	1
	Y
	Y
	Y
	Y

	Bedroom 2
	600
	900
	3
	2
	Y
	Y
	Y
	Y

	Bedroom 2
	600
	1500
	3
	1
	Y
	Y
	Y
	Y

	Bedroom 3
	600
	1500
	3
	1
	Y
	Y
	Y
	Y

	Bath
	600
	1200
	3
	1
	Y
	Y
	Y
	Y

	Bedroom 4
	1200
	600
	3
	2
	Y
	Y
	Y
	Y

	Bedroom 4
	1200
	1800
	3
	1
	Y
	Y
	Y
	Y

	Roof skylight
	700
	1140
	3
	1
	Y
	Y
	Y
	Y



The above materials are sourced from QLD supplier (name kept in confidentiality please)
Safety: The doors and windows meet safety standards and have features such as sturdy locks, tempered glass, and proper installation techniques to enhance security.
Fire resistance rating: The external doors and windows with fire-resistant properties or ones that meet fire resistance regulations to help prevent the spread of fire.
Suitability: The doors and windows are suitable for the intended purpose and the architectural style of the building. Consider factors such as design, material, and functionality to ensure they match the requirements.
Durability: The doors and windows made from high-quality materials that can withstand environmental factors like humidity, temperature changes, and potential wear and tear over time. This helps ensure their long-term performance.
Serviceability: The Doors and windows are easy to maintain and repair if necessary. The suppliers offers warranty or after-sales services for the products.
Cost-effectiveness: The overall cost of the doors and windows, including their initial purchase price, installation costs, maintenance expenses, and potential energy savings and providing long-term benefits and value.
Short-term degradation: We have assess any potential short-term degradation issues, such as color fading, warping, or structural integrity concerns. The product had good reviews and recommendations to minimize the risk of immediate deterioration.
Long-term degradation: The expected lifespan of the doors and windows, as well as any potential long-term degradation, such as corrosion or deterioration of seals and insulation is minimal. By selecting the high-quality materials and well-known brands can help mitigate these issues.
Availability: These were readily available for the date and time required for our Project
COMPLY WITH:
Windows and external glazed doors are required to comply with the below: This is to ensure the association of the windows and external glazed doors with the building is compliant with the Building Act 1975 and the QBCC Act. 
· AS 2047 – Windows and external glazed doors in buildings; 
· NCC barrier fall protection requirements; and 
· provisions under Part 6AA of the Queensland Building and Construction Commission Act 1991 (QBCC Act), including ‘required information’ for installers. 
· AS 2047 requires window ratings that use the design wind speeds for Class 1 and 10 buildings to be determined in accordance with AS 4055 – Wind loads for housing. 
***ON DELIVERY:
	ITEM
	MET
	NOT MET

	Any damaged material
	Y
	

	Any inferior material
	Y
	

	Any variation to specified material
	Y
	

	Accurate quantity
	Y
	

	Expected quality
	Y
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