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CPCCBC4002A 
Manage occupational health and safety in the building and construction workplace


	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances. 
Answers will be documented and FT003 (Oral examination declaration form) must be completed.
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· If a participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a participant changes their response in writing, they must put their initials next to the written change.
· If a participant changes their response verbally, this must be noted on the exam paper by the assessor.
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	ASSESSOR COMMENTS

	


For each of the common building and construction jobs listed below, identify one (1) hazard specific to that job. 

	Answer
	Job
	Risks
	
	
	Construction equipment use (e.g. power tools, concrete mixers)
	Mechanical 
	

	
	High risk construction equipment use (e.g. lasers, EPT)
	Laser radiation
	

	
	Crane use
	plant rollover
	

	
	Demolition
	Falling objects
	

	
	Formwork
	Formwork collapsing
	

	
	Scaffolding use
	Serious fall 
	

	
	Work at heights
	Serious falll
	

	
	Welding
	Electric shock
	





[bookmark: _Ref531681425][bookmark: _Ref423948341]Using the risk table below, determine the level of risk for each of the hazards identified in 0Identify how each risk level was determined, by identifying the likelihood and consequences of each hazard.

	Matrix
	A:
Death or permanent disability
	B:
Serious injury
	C:
Lost time injury
	D:
Casualty Treatment
	E:
First Aid

	1: Very Likely
	E
	E
	H
	H
	M

	2: Likely
	E
	H
	H
	M
	M

	3: Possible
	H
	H
	M
	M
	L

	4: Unlikely
	H
	M
	M
	L
	L

	5: Very Unlikely
	M
	M
	L
	L
	L



	E: Extreme
	H: High
	M: Medium
	L: Low




	Answer
	Job
	Level of risk
	
	
	Construction equipment use (e.g. power tools, concrete mixers)
	3B
	

	
	High risk construction equipment use (e.g. lasers, EPT)
	3B
	

	
	Crane use
	3A
	

	
	Demolition
	3H
	

	
	Formwork
	3A
	

	
	Scaffolding use
	3B
	

	
	Work at heights
	3B
	

	
	Welding
	3B
	



[bookmark: _Ref531681445]Identify an appropriate control measure for each of the hazards identified in 0

	Answer
	Job
	Control measure
	
	
	Construction equipment use (e.g. power tools, concrete mixers)
	Ensure guards are fitted to power tools
	

	
	High risk construction equipment use (e.g. lasers, EPT)
	Protective clothing and eyewear to be worn
	

	
	Crane use
	Licensed operator
	

	
	Demolition
	Using a licensed person to carry out work
	

	
	Formwork
	Use of extra support measures
	

	
	Scaffolding use
	Inspection of scaffold and supporting structures by competent person
	

	
	Work at heights
	Edge protection
	

	
	Welding
	Appropriate protective clothing and eyewear to be worn
	





[bookmark: _Ref531681639]True or False (Tick your response): Risk control options can come from both internal sources (e.g. policies and procedures) and external sources (e.g. codes and standards).

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref531681647]Name two (2) workplace personnel you may speak to for safety advice.

	Answer
	Safety Officer
Prinicipal contractor
	



[bookmark: _Ref531686208]Referring to the WHS Regulations, explain how the following documents contribute towards identifying hazards and risks in the workplace.

	Answer
	Document
	Description
	
	
	Safe Work Method Statements
	It identifies hazards in the workplace and describes relevant control methods Div 2, 299.
	

	
	Site Safety Plan / WHS Management Plan
	This plan can assist the principal contractor to manage their workplace health and safety obligations. Div.2, 309
	




[bookmark: _Ref531690669]Identify two (2) advisory standards you might refer to safely undertake building and construction work and briefly summarise their requirements.

	Answer
	Standard name
	Requirements
	
	
	WHS Act
	To protect the health and safety of workers and other people who might be affected by the work
	

	
	NCC
	Sets out minimum necessary safety requirements
	




Building and construction industry contracts require building legislation and the National Construction Code to be observed. Refer to these documents when responding to Q8. to Q10. 

[bookmark: _Ref531689010]Identify the requirements in the National Construction Code Volume 1 with regards to fire-isolated exits. Identify the relevant section of the Code and the Australian Standard referenced.

	Answer
	Code section(s)
	Requirements and Standards
	
	
	Part D1.3
	Every stairway or ramp serving as a required exit must be fire isolated
	




[bookmark: _Ref531689011]Identify the requirements in the National Construction Code Volume 2 with regards to smoke alarms. Identify the relevant section of the Code and the Australian Standard referenced.

	Answer
	Code section(s)
	Requirements and Standards
	
	
	3.7.2
AS 3786
	Smoke alarms must be located in Class 1a and Class 1b buildings
	




[bookmark: _Ref531691201]Name the building legislation (Act and Regulations) that apply within your jurisdiction.

	Answer
	Building Act 1975
Building regulation 2006
	



[bookmark: _Ref531681692]Which of the following should be considered when developing a risk control plan? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		How and when controls will be implemented
	

	
		Evaluation processes for implemented controls
	

	
		Consultation with individuals and parties
	

	
		Responsibilities for implementation
	




[bookmark: _Ref531681716]True or False (Tick your response): If control measures do not adequately control risks, they must be revised.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref531681755]Which of the following are appropriate techniques, tools and processes for identifying hazards and risks? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Workplace inspections
	

	
		Compensation claim information
	

	
		Safe Work Method Statements
	

	
		Information issued by WHS regulators
	




[bookmark: _Ref531681867]Which of the following can be used to assist with workplace inspections? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Hazard and risk checklists 
	

	
		Job Safety Analysis (JSA)
	

	
		Manifests and registers
	

	
		Surveys
	

	
		Workplace walk-through
	




[bookmark: _Ref531681976]Which of the following are limitations of using a generic hazard/risk assessment checklist? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Specifics of the workplace are not considered
	

	
		Not all checklist points will be applicable
	

	
		Such checklists/processes must be completed on a computer 
	

	
		You always have to purchase these checklists
	





[bookmark: _Ref531682022]Identify the applicable WHS Act in your jurisdiction. Identify its requirements for PCBUs with regards to identifying hazards and risks.

	Answer
	Act name and section(s)
	Requirements
	
	
	Work Health and Safety Act 2011
Sec 19
	PCBUs  need to consult their workers, review available information, look for trends and observe manual tasks to identify possible hazards and risks
	




[bookmark: _Ref531682034]Identify the applicable WHS Regulation in your jurisdiction. Identify its requirements for PCBUs with regards to identifying hazards and risks.

	Answer
	Regulation name and section(s)
	Requirements
	
	
	Work health and Safety regulations 2011 Part 3.1
	A PCBU must identify reasonably foreseeable risks and hazards and manage accordingly
	




[bookmark: _Ref531682039]Identify a relevant policy in your organisation with regards to identifying hazards and risks and briefly describe its requirements. 

	Answer
	Policy name
	Requirements
	
	
	Use of hazardous products
	Appropriate protective clothing and eyewear is to be worn while these products are being used 
	



[bookmark: _Ref531682218]Identify the statutory requirements in your jurisdiction with regards to the completion of inspection reports.

	Answer
	Legislation name and section(s)
	Requirements
	
	
	Work Health and Safety Act 
Sec 103E
	Once the assessment has been carried out a report must be done and given to the Safety officer or the person conducting the business within 30 days of the assessment.
	




[bookmark: _Ref531682429]Which of the following individuals and parties may require information about workplace hazards and proposed risk controls? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Health and Safety Committees
	

	
		PCBU
	

	
		All members of the public
	

	
		Workers
	




[bookmark: _Ref531682449]Identify the requirements in the Code of Practice with regards to consulting parties when managing risks.

	Answer
	Legislation name and section(s)
	Requirements
	
	
	Work Health and safety consultation, cooperation and coordination – Code of Practice 
2.1
	Consultation is required when identifying hazards, assessing risks and deciding on measures to eliminate or minimise those risks
	




[bookmark: _Ref531682469]Identify the requirements in the Code of Practice with regards to consulting parties when developing procedures for communicating WHS policy and practice requirements.

	Answer
	Legislation name and section(s)
	Requirements
	
	
	Work Health and safety consultation, cooperation and coordination – Code of Practice 2.4

	Affected workers must be consulted 
	




[bookmark: _Ref531682553]Name three (3) parties who should consult to determine effective strategies for communicating WHS policy and practice.

	Answer
	Employees, contractors and their employees
	



[bookmark: _Ref531682564]Name two (2) communication strategies that may be used in the building and construction industry.

	Answer
	Verbal and written
	



[bookmark: _Ref531682565]Name two (2) education programs that may be implemented in the building and construction industry.

	Answer
	Site specific inductions and specialist training
	


[bookmark: _Ref422743346][bookmark: _Ref531682593]Fill in the blanks for the statement below:

 (
consulted
) (
training
)The ‘How to manage work health and safety risks Code of Practice 2011’ identifies that control measures are more effective when ______________________ is provided and when workers are _____________________. 

	Answer
	
	



[bookmark: _Ref531682611]Explain why it is important to review the effectiveness of communications and educational programs.

	Answer
	To ensure that the consultation meets the WHS Act and regulations.
	



[bookmark: _Ref531682612][bookmark: _GoBack]List three (3) methods for reviewing the effectiveness of communication and educational programs.

	Answer
	Review incident reports
Conduct post training surveys
Review training materials to ensure that it is still relevant
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