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CPCCBC4014A 
Prepare simple building sketches and drawings


	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances. 
Answers will be documented and FT003 (Oral examination declaration form) must be completed.
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· If a participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a participant changes their response in writing, they must put their initials next to the written change.
· If a participant changes their response verbally, this must be noted on the exam paper by the assessor.
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	Assessor name
	Brett Stoward 

	

	

	Assessor signature
	



	Date
	21/05/2019




	Number of questions
	Number of questions answered correctly
	Satisfactory?

	23
	
	Yes
	No

	
	
		

	ASSESSOR COMMENTS

	


Identify three (3) two-dimensional drawings/sketches that may be used to clarify or communicate ideas to clients or other parties. For each drawing/sketch, identify four (4) key features that may be shown. 

	Answer
	Drawing/sketch type
	Key features
	
	
	Floor Plan
	Shows the layout/arrangement of rooms and other parts of a house interior
	

	
	Land Boundaries
	Shows the boundaries, critical adjoining of the building properties, levels on the site
	

	
	Sectional Views
	A view of the house or structure after it has been cut vertically at some point to show detail of structural parts.
	




[bookmark: _Ref1652804]Name two (2) advantages of a three-dimensional sketch/drawing. 

	Answer
	1. 3D drawings/sketches provide a more realistic picture of a space.
2. Designs in 3D is done in one model.

	



[bookmark: _Ref1652809]Name one (1) individual you might contact to establish the scope and standard of the job being undertaken. 

	Answer
	Clients, supervisors
	



[bookmark: _Ref1652872]You need to inspect the relevant area to take measurements for your drawings/sketches. Identify two (2) safety requirements you would need to observe on site. 

	Answer
	· Any additional forms or documents needed to complete at this visit
· Considered health and safety requirements so you have all the required tools and equipment, not only for measuring and inspecting the job but also for the safety of all people on site
· PPE SAFETY WEAR

	



[bookmark: _Ref1629720]Identify two (2) types of tools/equipment you would use when inspecting the area to take measurements. 

	Answer
	Measuring wheel – used for measuring quickly over long distances where a long tape would not be as efficient.
Open–frame tape – (50 and 100m) used for measuring site boundary dimensions and other site measurements in metres and millimetres. 

	



[bookmark: _Ref1629725]Identify two (2) types of tools/equipment you might need when completing sketches/drawings. 

	Answer
	Writing and sketching equipment – including HB pencils, rubber and biro.
Clipboard and paper – used to record all site details (written and sketch formats).

	



[bookmark: _Ref415490119]What action should be taken if any of the tools/equipment identified in Q5. and Q6. are found to be defective? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Report, Record
	

	
		Stop, Report, Record
	

	
		Stop, Tag, Report, Record
	

	
		Stop, Fix, Report, Record
	




[bookmark: _Ref875165]True or False (Tick your response): It is best practice to double check measurements before recording them.

	Answer
		True 
	
	
	
		False 
	
	



[bookmark: _Ref1653135]Explain the purpose of the scale on sketches/drawings. 

	Answer
	· Clarify or communicate ideas
· Capture design concepts 
· Make estimates
· Show measurements

	



[bookmark: _Ref1653139]You have measured a wall that is 2.4m high. Using a scale of 1:100, what size will this be drawn? Provide your answer in mm. Show your workings.

	Answer
	2.4 = 1:2.400MM
SCALE OF 1:100 2400
	



[bookmark: _Ref1653143]Explain the purpose of a key or legend on sketches/drawings. 

	Answer
	It set out ideas on room relationships, room sizes, house orientation, the stylistic treatment of the house, colour schemes and landscaping

	



[bookmark: _Ref1653145]Which of the following are true about drawing contours? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Equally spaced contour lines indicate uniform slope
	

	
		Closely spaced contour lines indicate flat surface
	

	
		Closely spaced contour lines indicate steep ground
	

	
		Concentric closed contours with decreasing values toward the centre indicate a pond
	

	
		Concentric closed contours with decreasing values toward the centre indicate a hill
	



[bookmark: _Ref427235149]Identify the Volume and Parts of the NCC that relate to metal sheet roof cladding for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	VOLUME 2 PARTS 3.5.1.0 AND 3.5.5.0
	VOLUME 1 PARTS B1 AND F 1.5
	




[bookmark: _Ref531355745]Which Australian Standard is referenced in the NCC with regards to the requirements for the design and installation of metal sheet roof cladding?

	Answer
	AS 1562
	



[bookmark: _Ref427733304]Sketch the following standard design symbols.

	Answer
	Item
	Sketch
	
	
	Compass (North)
		

	
	Sink with one bowl
		

	
	Stairs
		

	
	Toilet
		





[bookmark: _Ref427219196]Explain the meaning of the abbreviations in the table below.

	Answer
	Abbreviation
	Meaning
	
	
	BK
	Brick 
	

	
	CBD / CPD
	Cupboard
	

	
	DP
	Damp Proof
	

	
	INSUL
	Insulation
	

	
	KIT
	Kitchen
	

	
	MSB
	Main Switch Board
	

	
	PBD
	Plasterboard
	

	
	RWT
	Rain Water Tank
	

	
	SHR
	Shower
	

	
	TEL
	Telephone
	

	
	WC
	Toilet
	




[bookmark: _Ref1653550]True or False (Tick your response): The dashed/chain lines on the section view shown below represent the portions that have been in contact with the cutting plane. 

[image: ][image: ]

Source: https://www.mcvts.net/cms/lib/NJ01911694/Centricity/Domain/131/Section_Views.pdf

	Answer
		True 
	
	
	
		False 
	
	



[bookmark: _Ref1653558]Explain the use of hatching lines for sectional drawings.

	Answer
	Using the hatching lines is an indicating the nature of the materials used. Hatching lines are thin lines normally drawn 45 degree to the horizonal right or left. A key/legend can be used for lines representing different materials.
	



[bookmark: _Ref1653570]True or False (Tick your response): In an offset sectional drawing, the cutting plane does not travel in a straight line.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref1653501]Which of the following information should be included in the title block for a sketch/drawing? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Client details
	

	
		Contact details for person who prepared drawings
	

	
		Date drawing was completed
	

	
		Drawing number
	

	
		Drawing title
	

	
		Job number
	

	
		Project name and address
	

	
		Revisions / Amendments (if applicable)
	

	
		Scale
	




[bookmark: _Ref1653504]True or False (Tick your response): Amendments usually have to be signed or initialled by both the builder and the client to show they both agree.

	Answer
		True 
	
	
	
		False 
	
	



[bookmark: _Ref1653930]Explain why it is good practice to have a single repository for sketches/drawings.

	Answer
	Because it resembles having a central location where documents are stored means there is a reference point to check that the sketches/drawings being used are the most current. The title block of a document, provides the history of that documents, but not if any future changes have been made.
	



[bookmark: _Ref355889][bookmark: _Ref1653905]Name the Regulation and identify the section that outlines the requirement for structure designers to produce a safety report. 
Briefly describe the requirements. 

	Answer
	Section of Act
	Requirements
	
	
	In NSW work health and safety Regulation Act 2011 NSW section 295
	[bookmark: _GoBack]The designer of a structure must give the PCBU who has commissioned the design a written report specifies the hazards relating to the design which create a risk to those carrying out construction work
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