Activity 2

Overall Height – Certification 
· Submit to Development Assessment Certification from a licensed surveyor that the as constructed floor and roof levels are in accordance with this condition
Landscape the Site – Certification 
· Prepare a detailed Landscape Plan for the areas nominated on the approved drawings, in accordance with the approved Site Plan and Landscape Concept Plan, the relevant Brisbane Planning Scheme codes/Policies. On completion of works a Certification	will be submit from:
· A registered Landscape Architect or Landscape Designer that the detailed Landscape Plan complies with the City Plan (From CC10616 Landscape Design Certificate) and;
· A registered Landscape Architect and registered Landscape Contractor that the completed Landscape work complies with the detailed Landscape Plan (From CC10613 Landscape Works Certificate).
· A copy of the as-constructed detailed Landscape Plan must accompany the Completed Compliance Certificates.
Streetscape Works – Subtropical Boulevard (Out of Centre) – As Constructed Drawings 
· Submit “As Constructed” plans including an asset register, checked by a registered professional engineer Queensland, certifying that the concrete path works have been completed in accordance with relevant Brisbane Planning Scheme Codes/Policies. 
Streetscape Works – Neighbourhood Street – As Constructed Drawings 
· Submit “As Constructed” plans including an asset register, checked by a registered professional engineer Queensland, certifying that the concrete path works have been completed in accordance with relevant Brisbane Planning Scheme Codes/Policies. 
Acoustic Barrier – Certification
· Submit certification from an appropriately qualified professional that the constructed acoustic barrier complies with requirements.
Buildings in Transport Noise Corridors 
· Submit design to a Building Certifier as part of the subsequent development application for a development permit to carry out building work, details of the design of the development to demonstrate compliance wit this condition. 
· Submit construction to the Building Certifier, certification from a suitably qualified person, that the approved details of the design of the development to demonstrate compliance with the condition have been implemented. 
Retaining Walls – Certification
· For retaining walls over 1m in height obtain certification from a registered professional engineer Queensland that the design and construction of the retaining wall and ancillary draining is in accordance with this condition. 
Protest Existing Infrastructure – As Constructed Drawings
· If alterations to existing infrastructure are required then submit to Development Assessment “As constructed: Drawings, showing all new and/or rectification works and an asset register, prepared and certified by a registered professional engineer Queensland certifying that the works have been completed in accordance with any other relevant infrastructure requirements. 
Filling and Excavation – Earthwork Drawings 
· Submit the approval of Development Assessment earthworks drawings prepared in accordance with the approved drawings and documents, the relevant Brisbane planning scheme goes, checked, and certified by a registered professional engineer Queensland. 
Provide Certified Site Survey Levels – Drawings 
· Submit to Development Assessment, “As Constructed” drawings prepared by a Registered Surveyor certifying that the drawings are in accordance with the relevant Brisbane Planning Scheme Codes and show finished surface level information over the completed development. 
Remove Improvements & Obstruction From Truncation and Dedication – Certification
· Submit to development assessment certification from a registered surveyor or registered professional engineer Queensland that the above work has been completed in accordance with this condition. 
Access, Grades, Manoeuvring, Carparks, Signs and Line Marking – Certification
· Submit to Development Assessment, certification from a registered professional engineer Queensland, that the requirements have been implemented in accordance with this condition.
Dedicated As road – Non Trunk – Plan For Subdivision
· Submit for the Approval of Development Assessment, as a draft plan of subdivision showing the land to e dedicated for the road to demonstrate the road dedication complies with the road design parameters of this condition. 
· Lodge the notated plan of subdivision by Council pursuant to Schedule 19 of the Sustainable Planning Regulation 2009 with the Register of Titles for the relevant Queensland State Government Authority.
Site Draining – Major – Drawings 
· Submit and obtain Approval from Development Assessment, site drainage drawings and engineering calculations, prepared and certified by a registered professional engineer Queensland, in accordance with the relevant Brisbane Planning g Scheme Codes. 
· Submit “As Constructed Drawings” prepared by a registered professional engineer Queensland certifying that the works have been completed in accordance with the approved site drainage drawings. 



Service Conduits and Mains – Drawings
· Submit to Development Assessment “As Constructed” drawings, including an asset register, prepared by a registered professional engineer Queensland certifying that the above works are in accordance with this condition. 
Telecommunications – Certification
· Submit to Development Assessment, certification from an authorised telecommunications carrier/contractor, that the following works and infrastructure have been undertaken and installed in accordance with telecommunications industry standards. 
Agreement with Electricity Supplier – Agreement 
· Submit to Development Assessment, evidence of an agreement with an electricity supplier to provide necessary services to the development in accordance with the relevant Brisbane Planning Scheme Codes. 
Final Inspection – Carried out by Building Certifier. 


