Construction Plan Details Verification Checklist 

INSTRUCTIONS TO THE ASSESSOR: 
The specifications below are not specific to any building and construction project. Before the actual assessment, access and review the specifications for the building and construction project the candidate is undertaking as part  of this assessment. Update/adapt/revise the checklist below to ensure they reflect these specifications. 

	Completed by
	Noreen Abu-Obeid

	Date completed
	25/10/22



	Plans
	Version No.
	Date Published

	Architectural plans 
	3
	7/2/22

	Structural Plans 
	     
	     

	Mechanical Plans 
	     
	     

	Electrical Plans
	     
	     

	Plumbing and Drainage Plans
	4
	7/2/22





	Specifications
	Complied?
	Reasons for non-compliance of critical points indicated

	Category: Fixtures and Finishes - Foyer

	Main flooring - TMF12441, TMF12440, TMF12442, TMF12443
Check Pattern Lay with GG
	☒YES    ☐ NO
	     

	Stairwell timber steps - To be sanded back and refinished. Stain to be confirmed on site with LD & flooring specialist
	☒YES    ☐ NO
	     

	Hand rail - 40mm round Victorian Ash timber rail with clear coat sealer and the feature bracket - Victorian Ash clear coat sealer 150dia x 130d
	☒YES    ☐ NO
	     

	Panelling paint - Plum Intended. To wrap around all foyer walls and colour to be confirmed by LD on site prior to painting
	☒YES    ☐ NO
	     

	Timber door - Vertical panel timber door. Replace existing
	☒YES    ☐ NO
	     

	Timber door handle - Round Niki Dished Timber pull pair Internal/External fixing. American Oak. 250mm dia
	☒YES    ☐ NO
	     

	Mirror cabinetry/cabinetry - Laminex Kalamatta with 6mm clear silver mirror with polished square edges
	☒YES    ☐ NO
	     

	Category: Fixtures and Finishes – Wall, Ceiling, Floor finish
	
	

	Wall/Ceiling - Dulux Lexicon Half and colour to be confirmed by LD on site prior to painting
	☒YES    ☐ NO
	     

	Trim paint - Dulux Lexicon Half. Paint out existing timber trims.
	☒YES    ☐ NO
	     

	Existing timber flooring - To be sanded back and refinished. Stain to be confirmed on site with LD & flooring specialist
	☒YES    ☐ NO
	     

	Ceiling Fan Main Bedroom + Living Rooms - Airfusion Climate III 132 Fan white. Extension Rods required
	☒YES    ☐ NO
	     

	Ceiling Fan Back Bedrooms - Airfusion Airlie 122 Fan white
	☒YES    ☐ NO
	     

	Category: Fixtures and Finishes – Kitchen
Notes:
moisture resistant board to all wet areas
All joinery door hinges to be fully concealed within unit
Blum mechs to be used unless otherwise stated
Draw runners to be soft close
	
	

	Flooring - Southern Cross Creamics 200x200 Poco Gravity
	☒YES    ☐ NO
	     

	Stairs - Timber steps to be extended in timber. Stain to be confirmed
on site with LD & flooring specialist
	☒YES    ☐ NO
	     

	Joinery Fridge Elevation - Laminex Sublime Teak
Joinery Shelving Fridge Elevation - Laminex Green Slate
	☒YES    ☐ NO
	     

	Joinery Undercounter -  Laminex Green Slate with Recessed Handles
	☒YES    ☐ NO
	     

	Joinery Island Bench - Laminex Sublime Teak
	☒YES    ☐ NO
	     

	Cabinets - Cutlery draw inserts to suit draw size
	☒YES    ☐ NO
	     

	Bench tops - Pure white 40mm Stone Aris Mitred Edge
	☒YES    ☐ NO
	     

	Island Circular Bench - Polarity Terrazzo. 600x600 tiles. Sealing required. Construction tbc with Joiner & Builder
	☒YES    ☐ NO
	     

	Tile Splash / Ceiling - 50x50 white mosaic gloss
	☒YES    ☐ NO
	     

	Rangehood Tile - 97x97 white satin spectrum
Cabinetry edge - 97x97 white satin spectrum
	☒YES    ☐ NO
	     

	Fridge Elevation Handles - Wavy timber handle 550x65x19
	☒YES    ☐ NO
	     

	Bin - Fully Integrated Hideaway Compact 2x 40L waste bin with lid
cover plate. Cinder finish.
	☒YES    ☐ NO
	     

	Tapware kitchen - Brodware City Stik Pull Out Kitchen Mixer Chrome 1.9908.04.0.01
	☒YES    ☐ NO
	     

	Sink kitchen - Oliveri Sonetto Double Bowl Undermount Sink SN1063U Stainless Steel 785l x 405w x 211d
	☒YES    ☐ NO
	     

	Int fridge/freezer - F&P RS90A1 Intergrated French Door fridge/freezer
	☒YES    ☐ NO
	     

	Zip tap - Hydro tap G5 ARC Chrome
	☒YES    ☐ NO
	     

	Cooktop - ASKO 90CM PRO SERIES INDUCTION HL1995G
	☒YES    ☐ NO
	     

	Category: Fixtures and Finishes – Laundry
Notes:
moisture resistant board to all wet areas
All joinery door hinges to be fully concealed within unit
Blum mechs to be used unless otherwise stated
Draw runners to be soft close
	
	

	Floor and skirting - Southern Cross Creamics 200x200 Poco Tundra
	☒YES    ☐ NO
	     

	Floor/door threshold - TMF12443
	☒YES    ☐ NO
	     

	Laundry basket - Hafele Hideaway Concelo Laundry hamper Arctic White
	☒YES    ☐ NO
	     

	Sink - Oliveri DU490U Single Undermount Laundry Tub 590 x 400 x
235
	☒YES    ☐ NO
	     

	Category: Fixtures and Finishes – Main bedroom

	
	

	Bedroom floor - Serinity Meridan 12 Mythical
	☒YES    ☐ NO
	     

	Mirror door - Custom length, 6mm clear silver mirror with polished square edge
	☒YES    ☐ NO
	     

	Mirror door handles - Leather Recessed Pulls | Saddle Tan | Matching Edge | Raw Oak Core 195mm
	☒YES    ☐ NO
	     

	Category: Fixtures and Finishes – Main bedroom  Ensuite 
Notes:
moisture resistant board to all wet areas
All joinery door hinges to be fully concealed within unit
Draw runners to be soft close
	
	

	Flooring - Southern Cross Creamics 200x200 Veloce Hailstorm
	☒YES    ☐ NO
	     

	Main wall tile - 120x140 white satin
	☒YES    ☐ NO
	     

	Feature wall tile - TMF13318
	☒YES    ☐ NO
	     

	Tapware - Brodware - City Stik Wall Mixer Set - 1.9906.04.0.01 - Chrome
	☒YES    ☐ NO
	     

	Rail shower - Brodware - City Plus Handshower Set - 1.9734.03.0.01 - Chrome
	☒YES    ☐ NO
	     

	Mirror - Custom Shaving cabinet full length, 6mm clear silver mirror
with polished square edge. Overhand opening
	☒YES    ☐ NO
	     

	Category: Fixtures and Finishes – Main bath 
Notes:
moisture resistant board to all wet areas
All joinery door hinges to be fully concealed within unit
Draw runners to be soft close
	
	

	Bedroom 2/3/4 Hallway Floor - Serinity Belanger 11 Aster
	☒YES    ☐ NO
	     

	Flooring - Southern Cross Creamics 200x200 Macintosh Mistletoe
	☒YES    ☐ NO
	     

	Main tile wall - 120x140 white satin
	☒YES    ☐ NO
	     

	Basin - Roca Inspira Undercounter Basin 604x390 without Overflow
ceramic waste
	☒YES    ☐ NO
	     

	Bath spout/mixer - Brodware - City Stik Wall Mixer Set - 1.9906.04.0.01 - Chrome
	☒YES    ☐ NO
	     

	Mirror shelf – Laminex spinafex
	☒YES    ☐ NO
	     

	Wall floor trim - Trim to all external edges to colour match tile where not mitred
	☒YES    ☐ NO
	     

	Floor waste – Tile insert floor waste
	☒YES    ☐ NO
	     

	Shower screen - Framless Shower Screen, toughened glass, chrome fittings
glass to be treated with nanoprotection/enduroshield
	☒YES    ☐ NO
	     



Note to Assessor: The categories above and items under each category are based on a fictitious company’s project specifications. The assessor must update/adapt/revise the above to ensure they reflect the actual specifications for the building project. 
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