BSBWHS409 – Practical Task

Sampling Process Plan 

This process has been created for the monitoring of Isopropyl Alcohol Vapor in the workplace and determines to what extent workers are being exposed. The Isopropyl Alcohol is a high flammable liquid, colorless substance that has a unique odour. If the chemical comes into contact with eyes, skin and/or respiratory system will cause irritation and may cause drowsiness or dizziness. If the chemical is ingested and/or there is an overexposure it may cause specific target organ toxicity. 
[bookmark: _GoBack]To measure the concentration levels of Isopropyl Alcohol in the atmosphere in the workplace there will be multiple devices used to account for reading the amount of chemicals in the workplace area and what the workers are actually exposed to as they are traveling around different parts of the workplace. A direct reading device will be used to measure the atmosphere in the overall workplace and will be more accurate in way of recording the different levels of the chemical throughout the day. The direct reading device will not be able read what the worker is actually being exposed to. To combat this problem an Isopropyl Alcohol Vapor monitor will be used which will be placed on the worker. This monitor will react to the Isopropyl Alcohol Vapor in the atmosphere over the timeframe it has been placed on the worker and will show if the worker has been overexposed to the chemical. When the testing timeframe is completed the monitoring device will be sent to a laboratory for results. The tests will be carried out everyday over a two period. This is because the chemical is not used on a continuous way throughout each day and will help establish an average of how much the chemical is being used in the workplace.
The areas of the workplace where the measures will be taken will the spraying booth where the chemical is primary used in the surrounding areas where the chemical may be traveling. 
In terms of consultation before the sampling if carried out workers are made aware of the monitoring that is been planed. Ensure them that the monitoring equipment will not affect their work and they should carry out their worker as normal. The purpose and the process of the workplace monitoring will be effectively explained to workers and other affected by the process and consent of the workers will be given for the monitoring. Consultation with PCBU’s, Work Supervisors, Officers and Workers regarding to overall Process Plan to source feedback and information that can be contributed to the process, making it more effective.
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