Material Inspection and Delivery Checklist

Inspected by Noreen Abu-Obeid
Date: 5/3/2023


	Material
	Description
	Delivery Date 
	Quantity- Met as agreed 
	Quality – Met as agreed

	Demolition – Jack Hammer
	Demolish the 17 sqm of existing storage, supporting walls, wall tiles, flooring, sink etc. at all levels as required carefully and disposing off and clearing away the debris 
	5/03/2023
	Y
	Y

	Kitchen 
Elevation
Bench
Drawers
Spice rack
Brushed stainless steel laminate
Ducting
Overheads
Shelves
Caesarstone bench top
Island
Sink cupboard
Paint
Cabinetry - Blum Tandembox antaro h. Fronted pull-out C - DQC5JY, D - DQC69A, DQCB6M
Urbane Castella 192mmCTC handle

	Kitchen elevation 2730x2550Hx600mm diameter or expressed as 2.7mx2.55mx0.6m
Bench height 1000mm with 3 sets of 3 blum tip drawers with 1 of orga line spice rack insert
Brushed stainless steel laminate kick face
Ducting for downdraft cooktop to run behind draws
Overheads 650mm Height with 1 of adjustable shelf with doors hanging below as finger pull and LED strip lighting to underside
Internal 16mm HMR with 1mm ABS PVC match edge
Fronts in 18mm white sating with 2 pac satin finish
40mm Caesarstone bianco drift bench top with cutout for drop in cooktop
Kitchen island 3000x1000Wx1000 D – LH side with pull out drawer with 2x35L bin inserts
Sink cupboard with 1 door housing undermount single bowl sink with 3 sets of 4 blum tip on drawers with 1 of cutlery insert and 2 of utensil insert. Internals 16mmwh HMR with 1mm ABS PVC matching edge. All fronts in 18mm wh sat with 2pac satin finish

	5/03/2023
	Y
	Y

	Butlers Pantry
Door sink cupbard
Bins
Dishwasher
Drawers
Shelves
Overheads
Paint
	4480x2550 Hx620mm D pantry or expressed as 4.48m x 2.550m x 0.620m with door sink cupboard and 2x20L bins
Dishwasher opening 600mm
3 sets of 3 blum tip on drawers with 885mm pantyr to RH side
2 door pantry unit with 5 blum soft close internal drawers and 4 adj shelves
Overheads 3595x650 Hx400mm D with 1 adj shelf with doors hanging below as finger pull
	5/032023
	Y
	Y

	Laundry
Laundry tub unit
Shelves
Bench
Caesartone top 6131 Bianco Drift, 4600 Organic white
Shute cupboard
Overheads
Drawers
Tall cupboard
Brushed SS laminate
Single door cupboard
Paint
	L shaped laundry 2450x2520x2550mm or expressed as 2.45m x 2.52m x 2.55m with 4 door laundry tub unit with 1 adj shelf with bench at 1000mm H
40mm Caesarstone organic white top running wall to wall below laundry shute cupboard and 20mm thick splashback 150mm height
4 door overhead cupboard with 2 adj shelves and dorrs hanging down as finger pull above dryer and washing machine openings with flat pull out shelves and 1 of blum soft close drawer below
2 door Tall broom storage cupboard to right side with 1 of blum soft close drawer below 1 0f internal adj shelf
Brushed stainless steel laminate kick face
Single door cupboard 600x600mm on opposite wall 1000mm height bench top.
All internals 16mm white HMR with 1mm ABS PVCedge.  All fronts in 18mm white sating with 2 pac satin finish
Dryer and washing machine panels, bottoms in 32mm MDF with 2pac finish
	6/3/2023
	Y
	Y

	Plumbing
Franke Ancona single bowl undermount sink
Double bowl undermount sink
Mizu drift sink mixer
Mizu smothe sq sink mixer
	Island & laundry - franke ancona single bowl undermount sink – anx 110-48
Pantry - franke ancona double bowl undermount sink - anx 120
Island & pantry - mizu drift mk2 gooseneck sink mixer pull-out
Laundry - mizu soothe square gooseneck sink mixer

	8/3/2023
	Y
	Y

	Electrical
Light
LED tape
	Beacon Herman 1 light pendant
14 watt led tape and recess led profile under overhead cupboards
Single phase underground power connection from existing supply point. 
Led light strip under island bench
Cooktop isolation switch

	28/4/2023
	Y
	Y

	Tiling
Timber look tile flooring
Ceramic tile splashback – kitchen and laundry
Kitchen timber look tile to match floors
Brushed stainless steel laminate

	New timber look tile flooring 
Kitchen – timber look tiles to match floors 1200x x230mm
Laundry and kitchen - ceramic tile splashback - Snow Brillo Tile Sc19 A7615, Amber Tiles To Match Cabinets. 130mmx130mm
Brushed stainless steel laminate kick face
130 sqm 
	20/4/2023
	Y
	Y

	Butlers Pantry - Fixed Glass Window
	New fixed glass window to suit existing opening width frame
1800x600mm
Colour to match exiting and tinted to client requirement (customized)

	2/5/2023
	Y
	Y

	French Doors - Triple Slider
	New Triple Slider With Screens To Match Existing Profile & Colour
2710x2100mm

	2/5/2023
	Y
	Y

	Dining Room Slider - Reverse Opening
	Slider with reversed opening with screen to match existing profile and colour
1810mmx2100mm
	2/5/2023
	Y
	Y

	Removal of Debris
Cleaning material
Skip bin

	Cleaning materials

Skip bins
	5/5/2023
	Y
	Y



