COMMERCIAL PROJECT

DOCUMENT FOR 123 Commercial street, QLD

· Public Liability Insurance will be provided by Knights CBI and to remain in force for the period of the contract – 10M
· Workers Compensation Insurance will be provided by Knights CBI and to remain in force for the period of the contract
· Occupational Health and Safety
Knights CBI shall: 
· Comply with all requirements of the contract and all statutory requirements for Occupational Health and Safety. 
· Ensure that each of its Subcontractors and workers comply in like manner. 
· Demonstrate to the Client whenever requested that requirements of the contract and statutory requirements for Occupational Health and Safety are being met. 
· Protection of the Environment
Knights CBI shall; 
· Comply with all statutory requirements and accepted current practices for Environmental management. 
· Comply in every respect with the Erosion and Sedimentation Plan pertaining to this contract. 
· Ensure that each of its subcontractors and workers comply in like manner. 


SCOPE OF WORKS:

Demolish existing building make site good then design and construct change rooms as per scope and drawings provided. 

DESIGN PHASE
· Demolish existing building, design and construct a new building. 
· Detail design for construction. 
· Your tender submission for the initial design must be based upon the concept drawing proposal. 
· Consult with planning authorities to determine constraints 
· Liaise with Power and Water and sewer connection during design phase 
· Obtain planning permit required if require. 
· Obtain Building permit 
· Obtain AAPA clearance required. 
· Obtain heritage approval required if require. 
· Certification for drawings (Electrical, Plumbing, Structural, Glazing) as required from certifier. 
· Ensure all OHS policies and procedures are followed 
· Risk assessment 
· All works to be to the latest Australian Standards and Building Codes of Australia

CCTV SYSTEM REQUIREMENTS 
· A CCTV system to monitor all external building entry points to the facility. 
· System must be compatible with Digifort systems. 
· Have the capability of multiple remote access to all sites
· To program multiple user's with invigilate rights 
· System must be remotely accessible from server via 4G mobile network. 
· Camera must have a minimum capability of Day/night 100 Meter Infra-red 8  Mega pixel. 
· Communicate alarms to telecommunication network. 
· Advanced reporting and site research capabilities. 
· Must have proven resources available to remotely change ,program analytics 
· Remote access for copying of footage and system maintenance. 
· Office capabilities to remote camera checks and produce camera conditions and system reports 
· Recording system must be able to operate -5 to +65 

· ELECTRICAL REQUIREMENTS
· Power points in Bar/ Canteen - there are 4 x Double GPO's in each room. (8 x double GPO’s) 
· Power in Office - 2 x Double GPO's 
· Power in Referee's Room - 2 x Double GPO's (4 x double GPO) 
· Power in Medical room - 2 x Double GPO's (4 x Double GPO) 
· Power in storage - 2 x Double GPO's for each area. 
· Power in each change rooms - 2 x Double GPO's if possible. (4 x double GPO) 
· Lighting to be suitable and meet standard requirement. 

CONSTRUCTION PHASE
· Liaise with Power, Water and sewer connection during construction phase 
· Certification (Electrical, Plumbing, Structural, Glazing) as required. 
· Demolish existing building. 
· Construct new building as per design drawing from engages architecture/Engineering Consultant firms. 
· Provide construction programme and weekly report to client
· Demolish existing building and construction change rooms, toilets and canteen room, to be constructed at 123 Commercial St, QLD includes but is not limited to the following: 
· The erection of temporary fencing and gates around the construction site and the site office. The temporary fencing and gates are to be removed prior to handover of the works. 
· Locate and mark all underground services in the proximity of the proposed works. 
· The demolition and removal of all redundant services in the construction area. Retain all required service connection points for reuse. 
· The preparation of the building pad. 
· The extension and connection to existing water, power and sewer main. Liaise with Power and Water authority and the works to be carried by credits licence contractors/sub- contractors. 
· The design and certification of the Hydraulic trade.
· The commissioning of the new services.
· The installation of new concrete paving around the new building. 
· Final clean up - General: Before practical completion, clean throughout, including interior and exterior surfaces exposed to view. Vacuum carpeted and soft surfaces. Clean debris from the site, roofs, gutters, downpipes and drainage systems. Remove waste and surplus materials
· Removal of plant and temporary materials - General: Within 10 working days after practical completion, remove temporary works and construction plant no longer required. 
· Commissioning test for practical completion – Electrical services
· Knights CBI will provide Traffic Management Plans and erect all necessary fences, barricades, warning lights as may be necessary for the protection of the works and the safety of the public and vehicles all to conform to Australian Standard AS 1742.3 - 1996. 





	SPECIFICATIONS

	EXTERNAL FINISHES

	LOCATION
	MATERIAL
	FINISH
	COLOUR

	Roof sheeting 
	Custom Orb 
	Colourbond
	Surf mist

	Flashings, cappings & trims 
	Sheet metal  
	Colourbond
	Surf mist

	Walls 
	Face blockwork 
	Wattyl poly U anti-graffiti
	Sandstone

	Lattice 
	Steel 
	Colourbond
	Classic cream

	Exposed structural steel 
	Steel 
	Exterior full gloss latex
	Dulux Goanna grey PG2C8

	Door frames 
	Pressed metal
	Exterior full gloss latex
	Dulux Goanna grey PG2C8

	Doors 
	Sealeck Primaguard 
	Colourbond
	Classic cream

	Gates
	Steel 
	Exterior full gloss latex
	Dulux Jodhpurs P14F1 


	Paving
	Concrete
	Broom finish nitofloor FC100
	Clear

	INTERNAL FINISHES

	Floor
	Concrete/Oxide 
	Polished
	Oxide: Charcoal
Epirez primer 123 and 2 coats of Eziseal Clear 


	Walls
	Face Blockwork /Wall tiles 150 x 150mm x 6mm
	Wattyl poly U anti-graffiti / ceramic
	Sandstone/clear / white

	Toilet Partitions 
	Compressed fibre cement
	Polyurethane paint
	Charcoal

	Door frame
	Pressed metal
	Low VOC full gloss latex Bourne
	Dulux Goanna Grey PG2C8 


	Timber door
	Solid core
	Low VOC full gloss latex Bourne
	Dulux Jodhpurs P14F1 


	Fixed Furniture
	Benchtop
	2 pack polyurethane
	Dulux Jodhpurs P14F1 


	
	Steelframe
	Powder coat
	Charcoal

	
	shelf
	melamine
	white

	
	
	
	

	FIXTURES

	Female toilet
	Toilet suite
	Britex Grandeur Pan 6/3 Litre flush 

	

	
	Wash trough
	Britex Pattern Trough No. 3

	

	Female accessible tooilets
	Toilet suite
	Britex Grandeur Disabled

	

	
	Grab rails
	To comply with AS 1428.1 
	

	Baby change
	Hand basin
	Britex HBS hand basin single tap hole 

	

	cleaner
	Cleaners sink
	Caroma Vitreous China on bolt on brackets 

	

	Male toilet
	Toilet Suite 
Wash Trough 
Urinal 

	Britex Grandeur Pan 6/3 Litre flush
Britex Pattern Trough No. 3
Britex Water Saving Urinal x 6 

	

	Male accessible toilet
	Toilet suite
	Britex Grandeur Disabled

	

	
	Grab rails
	To comply with AS 1428.1
	

	tapware
	Caroma and chrome plated
	
	

	Cover plates
	Where exposed water lines emerge from wall, floor or ceiling finishes, provide cover plates of non-ferrous metal, finished to match the pipe, or of stainless steel 

	Pipe diameter:
Up to 20 mm: plate = 65mm
21 mm to 50 mm: plate 100mm
And Larger than 50 mm: 50mm larger than pipe
	


· Concrete 
Concrete Class to AS 1379 with grout S20 and N25 strength 20 MPa and structural concrete 25MPa with cement content 300kg/cubm
External Concrete Finish: 
Broom finish: When most of the water glaze or sheen has disappeared and before the concrete becomes non-plastic, texture the whole surface of the pavement at right angles to the direction of the placing of the concrete by means of coarse brooms at least 500 mm wide with bristles of nylon or flexible wire. Wash brooms regularly to remove slurry. 

Joints and edges: Finish with a jointing tool. 
Finished pavement surface: Provide a surface uniform in appearance and free from depressions in which water can lie, with an average texture depth of 2 to 2.5 mm. 
Internal Concrete Finish: Polished Concrete coated with Epirez primer 123 and 2 coats of Eziseal Clear Topcoat complete with glass beads between top coats 
· Structural Steel 

o Materials And Components 
Materials generally: To AS 4100 Section 2. Cold-formed sections: To AS/NZS 4600. 
Grade 300+
Protective coating schedule to AS 1627 inorganic zinc silicate
· Masonry
Concrete masonry units to AS/NZS4455, blockwork with standard 200 series
Grading 20
Mortar joints finish – rodded and mortar mix 1:1:6
· Roofing 
Use a proprietary system of preformed sheet and purpose-made accessories. Design and installation: To AS 1562.1 and to manufacturer’s instructions. 
Material: Proprietary item: 
Thickness: Finish: Colour: 
Metal roof sheeting Lysaght Custom Orb 
0.48mm BMT
Colorbond
Refer to Finishes Schedule 
· Cladding
o Metal Cladding 
Provide a proprietary system of prefinished profiled metal cladding complete with accessories, trim and flashings. 
Proprietary item: Gramlat Lattice 
Finish: Colorbond
Colour: Refer to Finishes Schedule. 
Trim: Standard proprietary trims. 

· Doors

o SEALECK Doors 
Proprietary Item: Sealeck Primaguard Door
Installation
Fit doors with an even tolerance of 2 to 3mm to the frames. 
Door thickness: 42 mm. 

· Hardware 
o Hardware Fixtures

GRAB RAILS
Type: Stainless steel grab rail standard to AS 1428.1.
Size and location: Shown on drawings.
TOILET ROLL HOLDERS
Proprietary item: Britex Stainless Steel Jumbo Toilet Roll Dispenser 
Location: Adjacent to each WC.

PAPER TOWEL DISPENSERS
Proprietary item: Air Towel PTDRSS-A4093
Location: Adjacent to each Hand Basin or Wash Trough.

TOILET SHELF BRACKETS
Proprietary item: Lanes 'Strongline' no. 355 - 200 x 150 mm white. Fixing: Screw fix to wall at 600 max crs. 
· Partitions
o Toilet Cubicles 
Description 
Provide a proprietary cubicle system complete with doors and hardware

Partition System 
SYSTEM: Partitions consisting of divisions, fronts, nibs and doors made from compressed fibre cement sheets with the necessary fixings and hardware, fixed where shown on the drawings or specified. 
Proprietary Item: Kyissa K4 Partition Systems. 

PANELS: Factory prefinished double faced compressed fibre cement sheets with square stone cut edges ground smooth and arrised, slightly nosed. 

DIVISIONS: 18 mm thick in two sections joined horizontally with stainless steel threaded dowels and finished flush. 
HEIGHT OF DIVISIONS OFF FLOOR: 150 

FRONTALS: 18 mm thick compressed sheet fixed to floor with 55 mm x 6 mm diameter threaded stainless steel dowels and epoxy adhesive. 

JOINTS: Join divisions to frontals with proprietary PVC trims screwed and epoxy adhesive fixed to the frontals and epoxy adhesive fixed to the divisions. 

FIXING: Fix divisions and nibs to walls with threaded stainless steel dowels at 300 mm centres and epoxy adhesive. 

HEAD CHANNEL: Aluminium channel continuous across fronts and screw fixed to tops of fronts and nibs. Form the channel into a box section over doorways by snapping in a mating channel insert. 

FINISH: powder coated 

DOORS: 18 mm thick high moisture resistant medium density fibreboard ( HMR MDF ) with hardware fixing holes completed before application of 2 pack polyurethane finish. 

FINISH: Factory finished 2 pack polyurethane to APAS 2911 to give a high gloss long lasting finish. 

COLOUR: Refer to the Finishes Schedule.

FURNITURE: Satin finished stainless steel sets consisting of: 
· −  Gravity Hold Open Hinges 
· −  Door privacy indicator with emergency access 
· −  Bumper and Staple
· − Rubber tipped bumper and coat hook. 

Proprietary Item: Lincoln Sentry washroom partition hardware. 

· Benchtops 
Paint finish benchtops 
Material: 32mm thick moisture resistant HMR MDF laminate finish. 
Finish: 2 Pack Polyurethane paint. 
Colour: Refer to the FINISHES SCHEDULE. 
Installation: Scribe to walls. Fix to carcass at not less than twice per 600 mm length of benchtop. 
Joint sealing: Fill joint with sealant matching finish and clamp with proprietary mechanical connectors. 
Splashbacks / ceramic tiles

· Waterproofing Wet Areas Standard 
To AS 3740 and to the requirements of the BCA. 
Membrane 
Use a proprietary liquid applied or sheet membrane. Use suitably qualified applicators. Floor wastes: Turn membrane down onto the floor waste puddle flanges, and adhere. Curing: Allow membrane to fully cure before tiling. 

PRELIMINARIES
General conditions – all builders/tradespeople on site to be licenced appropriately
Site temporary works - Temporary works: Provide and maintain required barricades, guards, fencing, shoring, temporary roadways, footpaths, signs, lighting, watching and traffic flagging. 
Site Accessways, services: Do not obstruct or damage roadways and footpaths, drains and watercourses and other existing services in use on or adjacent to the site. Determine the location of such services. 
Site and Property: Do not interfere with or damage property which is to remain on or adjacent to the site, including adjoining property encroaching onto the site, and trees. 
Occupational Health and Safety – as per WHS

QUOTATION – New Changerooms and Toilets
	Description
	Unit
	Qty
	Rate ($) 
	Amount ($) 

	Away Changeroom
	sqm
	55
	$2500
	$137500

	Home Changeroom
	sqm
	55
	$2500
	$137500

	Away Shower/WC
	sqm
	21
	$3500
	$73500

	Home Shower/WC
	sqm
	21
	$3500
	$73500

	Public toilets - Male/ Female/UAT
	sqm
	26
	$3500
	$91000

	Store 1
	sqm
	15
	$1800
	$27000

	Store 2
	sqm
	15
	$1800
	$27000

	First Aid Room
	sqm
	15
	$2200
	$33000

	Umpires Room 1
	sqm
	20
	$2500
	$50000

	Kitchen
	sqm
	20
	$3500
	$70000

	Ancilliary room - office
	sqm
	25
	$2500
	$62500

	Veranda/paving
	sqm
	50
	$450
	$22500

	Circulation and services
	sqm
	40
	$2000
	$80000

	Allowance for kitchen appliances
	item
	
	
	$25000

	Sewer connection
	item
	80
	$125
	$10000

	SUB TOTAL
	
	378
	
	$920000

	GST 10%
	
	
	
	$92000

	TOTAL
	
	
	
	$1012000



PAYMENT OF THE WORKS
Anticipated progress payments 
General: At commencement of the works, submit a schedule of anticipated progress claims which will be made throughout the contract. Submit a revised schedule with each progress claim. 
Purpose of submission: Information only. 

DELIVERABLES
Knights CBI will deliver the Project within 60 days of commencement of Project

It shall be the responsibility of Knights CBI to ascertain all information relating to the services, the works and site conditions that may affect the progress or method of performing all services and works as specified within the scope of this contract and to prepare for every contingency that may arise. It is further understood that just provision for these contingencies have been accounted for, implicitly or explicitly within the lump sum price submitted. 

All work shall be completed in accordance with all the latest editions of relevant or listed Australian Standards (defined hereafter as Standards) and Codes of Practice and conforming to all requirements of the Building Code of Australia (BCA). 

All materials, unless otherwise specified by the Superintendent, are to be new and of the highest quality and installed in accordance with the manufacturer’s specifications and industry best practice. 
Completion: Prior to Practical Completion, submit a detailed schedule of defects and incomplete work to the Superintendent indicating that each item has been corrected or completed to satisfaction 

BUILDING TENDER NOTES

NOTES TO TENDER – Conditional Offer:
This Tender is subject to:
· the Client entering into a Building Contract with Knights CBI;
· the Client entering into a preliminary agreement for early services and 
· the Client entering into a contract for scope of works
occurring within 30 days from the date of this Tender.

The Client acknowledges that there has been no allowance made by Knights CBI for additional works which has not been expressly identified or detailed in this Tender.

The following items must be attended to, and necessary documents provided to Knights CBI after acceptance of the Tender;
· The Client must complete and sign and return back to Knights CBI, the letter of authority to commence construction (Authority to Commence) and the Client must provide evidence satisfactory to Knights CBI of its capacity to pay. 
· There shall be no Contract prior to the issue of a letter of acceptance. 

BUILDING TENDER ACCEPTANCE
1. I/We acknowledge that I/we have read and understood the Tender, including the standard
conditions and home inclusions and that I/we have discussed it with a representative of Knights CBI

2. I/We understand that this Tender is subject to and conditional on a Building Contract being
entered into by me/us and Knights CBI and that this Tender will form part of the Building
Contract and its conditions.

3. I/We accept that the amount identified in this Tender is only valid if:
a. I/We enter into an unconditional Building Contract with Knights CBI within the 30 days. 
b. If for any reason out of the control of Knights CBI a Building Contract is not entered into within this time, the price may be reviewed

4. I/We enter into a Preliminary Agreement with Knights CBI for early services.

5. I/We hereby instruct Knights CBI to complete associated construction documentation on
my/our behalf under and pursuant to the Preliminary Agreement.

6. I/We will make payments to Knights CBI, when required as per the contract and
building agreement 

7. I/We acknowledge that the copyright on all plans and sketches designed and or prepared by
Knights CBI remain the property of Knights CBI and nothing in this agreement gives the
right to me/us to use or copy any part of plans and sketches or to license anyone else to use or
copy plans and sketches without the prior written consent of Knights CBI 

8. I/We acknowledge that I/we have read and understood above points 1 to 8 and I/we accept the
tender price and conditions.

Client Signature
Date

Client  Signature
Date


KNIGHTS CBI STANDARD CONDITIONS OF CONTRACT

The Client acknowledges acceptance of the following standard conditions and requirements.

1. Finance may be required, and the client acknowledges that if finance is needed for the scope of works, they will submit a formal loan application within 5 days of this quotation being accepted.
2. The client will endeavour to provide Knights CBI with evidence of their formal loan approval within 10 days of acceptance of this tender, which demonstrates the client has sufficient funds to complete the purchase.
3. Contracts and Building Agreements provided to the client are signed and returned within 7 days to Knights CBI once the finance condition is satisfied.
4.  Payment of initial $1,000.00 deposit towards the reserving the job. 
(Note 1: Payment of 10% of the Building Contract value is required once finance is approved or invoiced by Knights CBI, as deposit. 
Note 2: The balance of payment will proceed as progressive payments as per the Contract
5. Loan documents are to be signed by the clients in accordance with their lender’s instruction, and once available provide Knights CBI with the lender’s written ‘Authority to Commence’ to ensure that construction proceeds in accordance with the terms of the Contracts.
6. It is acknowledged by the client and Knights CBI that this is a fixed price building quotation for specific works and inclusions noted within the quotation. Unless otherwise stated within this building quotation variations will be undertaken as an additional charge and will be documented and agreed by both parties prior.
7. It is acknowledged by the client that no plan changes, variations and/or colour selections will be accepted with this Building Contract. (In exceptional circumstances where any changes are accepted by Knights CBI the client will incur a minimum $400.00 administration fee in addition to the cost of any materials required to comply with the plan change, variation and/or colour selection.)
8. Knights CBI do not permit the use of client supplied items and/or labour, unless agreed upon by both parties prior.
9. The work be carried out under the Contract for 123 Commercial Street, QLD as per scope of works


TENDER DOCUMENTS - 	STRICTLY CONFIDENTIAL AND USED STRICTLY FOR THIS COURSE STUDY ONLY 
THIS SECTION COMPLETED BY THE TENDERER – Knights CBI
I/We, the undersigned, having examined and acquired an actual knowledge of the whole of this contract document do hereby tender to perform the whole of the Works described in, and in accordance with, the document in the amount of $1012000
$ (One million and twelve thousand dollars including GST) 
Date 15/1/2023
Name Noreen Abu-Obeid
On behalf of Knights CBI
ABN-12345678910 
Postal Address Knights CBI, 123 Mystreet, Myland, QLD
Telephone 1234567
Print Name: Noreen Abu-Obeid
(Full Name of Firm/Individual): Knights CBI
Signature:  NAO
Date 12/12/2022
Witness: HIM



DECLARATION

All Submitted information will be treated as confidential. 
I, NOREEN ABU-OBEID (Print name ), of Knights CBI (Tendering Organisation), do hereby solemnly declare and affirm the following ; 
1. I hold the position of Estimator/Contracts Administrator/Project Manager, and am duly authorised by the tendering organisation to lawfully proclaim the following and, after having made due inquiry believe the following to be completely accurate to the best of my knowledge. 
2. Neither the Tenderer nor the Tenderer’s Agents have entered into any contract or agreement to offer payment of any kind to a trade association, representative of the Superintendent or representative of the Principal in the event of a winning tender by this Organisation. 
3. Neither the Tenderer nor the Tenderer’s Agents have had any knowledge of the price of tenders submitted by it’s competitors nor did the Tenderer furnish the price of the enclosed tender to any source external to the Tendering Organisation prior to the close of the tender date as specified within this Contract. 
4. Neither the Tenderer nor the Tenderer’s Agents have entered into any contract or agreement to offer payment of any kind to an unsuccessful Tenderer in the event of a winning tender. 
5. The Tenderer is not aware of any facts which would affect the decision of the Principal in accepting the tender nor has the Tenderer attempted to acquire information relevant to the tender award process by soliciting the Principal, the Superintendent or their Representative’s Agents. 
6. Neither the Tenderer nor the Tenderer’s Agents have entered into any agreement with other Tenderers or third party which results in a payment of unsuccessful Tenderer’s fees. 
7. The contents of this document are true and correct to the best of my knowledge and in no way have been written under duress of any form. 
I make this solemn declaration as to the matter aforesaid, according to the law in this behalf made, and subject to the punishment by law provided for any wilfully false statement in any such declaration. 
Signature of Tenderer : NAO Subscribed and declared at : Knights CBI on This : 12th Day of December (Year)2022
Witness: HIM


BUSINESS STATUS

Company Name: Knights CBI
ABN-12345678910 
Directors – xyz 
Project manager – Noreen Abu-Obeid
Estimator/Contract administrator – Noreen Abu-Obeid
Postal Address: Knights CBI, 123 Mystreet, Myland, QLD
Telephone 1234567



CERTIFICATION 
I certify on behalf of Knights CBI (the Tenderer), that to the best of my knowledge: 
· none of the Proprietors, Directors, Managers have ever been bankrupt or a Director, Manager or Secretary of a Company that is being or has been wound up (whether voluntary or otherwise), and; 
· the business is not trading under: 
· an arrangement and/or reconstruction (ie. restructuring a public company)
· receiver and management
· official management
· an arrangement with creditors without sequestration (ie without the proprietors being made bankrupt) 
Signed: NAO
Date:15/1/2023
For: Knights CBI
Position Held: Estimator/Contract administrator/Project Manager



INSURANCE

WORKERS COMPENSATION
POLICY NUMBER - 456
NAME OF INSURER - DEF
DATE OF EXPIRY – 1/1/2025

PUBLIC LIABILITY – 10M
POLICY NUMBER - 789
NAME OF INSURER -GHI
DATE OF EXPIRY – 1/1/2025

Signed: NAO
Date:15/1/2023
For: Knights CBI
Position Held: Estimator/Contract administrator/Project Manager


Knights CBI PARTICULARS - PERSONNEL 
The Tenderer must complete and submit with tender All Submitted information will be treated as confidential 
Provide the names of all key personnel who will be engaged by the contractor in the execution of work covered by this contract. 

CONTRACTOR_________________________________ 
Qualifications _________________________________ 

KEY PERSONNEL 
Name 
Company role
Years of experience
Qualifications

Knights CBI PARTICULARS – CURRENT COMMITMENTS
The Tenderer must complete and submit with tender All Submitted information will be treated as confidential
List current projects Knights CBI is engaged in or committed to
Project name:
Client:
Contact details:
Site address:
Contract amount:
Estimated completion:
Description of works:


Knights CBI PARTICULARS – PROJECT HISTORY
The Tenderer must complete and submit with tender All Submitted information will be treated as confidential
List current projects Knights CBI has completed in the last 10 years
Introduction: We are a fully licenced family business who prides itself on its family culture and an Australian master builder over the past decade.  Our team has the local knowledge, skills, experience, technical expertise and capacity to deliver value and quality in projects we undertake. Our Projects consists of high-quality renovations, alterations, extensions, new builds to the needs of our customers and offer high standards for safety, quality and integrity. And we take pride in that we understand the skills, knowledge and expertise needed for the project, by understanding properly the information related to the evaluation criteria in place and reflect the procurement’s level of complexity
Project name:
Client:
Contact details:
Site address:
Contract amount:
Duration of project:
Description of works:


Knights CBI PARTICULARS – PRIOR TERMINATION OF PROJECTS
The Tenderer must complete and submit with tender All Submitted information will be treated as confidential
Has Knights CBI eer failed to complete a Project? No
If Yes (Y), provide details


Knights CBI PARTICULARS – SUBCONTRACTORS/SUPPLIER REGISTER
The Tenderer must complete and submit with tender All Submitted information will be treated as confidential
Details of selected subcontractors/Suppliers expected to use to execute the Works under the terms of this contract

	CONTRACTOR/SUPPLIER
	CONTACT DETAILS
	DESCRIPTION OF WORKS/MATERIALS

	Builder
	0123
	As per contract

	Carpenter
	1456
	As per contract

	Electrician
	0789
	As per contract

	Plumber
	0456
	As per contract

	Tiler
	1234
	As per contract

	Concreter
	5678
	As per contract

	Plasterer
	9101
	As per contract

	Painter
	1213
	As per contract




Knights CBI PARTICULARS – MACHINERY/ EQUIPMENT
The Tenderer must complete and submit with tender All Submitted information will be treated as confidential
Details of Major Equipment and Machinery proposed to execute the Works under the terms of this contract

	MAKE/MODEL
	DESCRIPTION
	OWNED/LEASED

	
	
	





