 


 
ASSESSMENT FOR 

	Student name
	Kevin Larney

	Date of assessment submission



	Trainer/Assessor’s name
	Tui

	Date of assessment marking

	Outcome for unit
	 Competent
 Not Yet Competent




TASK INSTRUCTIONS

· As part of the assessment for this unit of competency, you are required to complete a series of activities.
· Some of these activities will require you to provide a response within this document, others will require you to gather evidence to demonstrate your knowledge and skills.
· At all times, the responses in your assessment must reference Australian (Queensland or Federal) documentation, including legislation, regulations, codes of practice, standards and guidance publications. 
 

ACTIVITIES

	· 

	Identify/list the scope of the work to be carried out from the concept plan shown.








	Response 

	The main things that need work carried out on include: 
Garage, entry, public area, pedestrian access, screen, paved area, deck, and pod.




	Outcome for Activity 1
	 Satisfactory 	
 Not satisfactory

	Trainer/Assessor comments
	


 

	· 

	Identify/list the detail on the landscape plan shown.








	Response 

	The details on the landscape plan include:
Name, address, date, scale, direction, symbol key, materials, equipment and tools.




	Outcome for Activity 2
	 Satisfactory 	
 Not satisfactory

	Trainer/Assessor comments
	


 

	· 

	List the materials required to complete the water feature, by using the wall and water feature construction plan shown.











	Response 

	Concrete, sand, gravel or crushed stone, rocks and stones, wood mulch, wood timbers, soil, stone, brick, bituminous paving, filter mat, steel, re-bar, bolts and rod.




	Outcome for Activity 3
	 Satisfactory 	
 Not satisfactory

	Trainer/Assessor comments
	


 

	· 

	Research and list relevant laws and standards relating to concreting works 
(e.g. Building Codes, Australian Standards, Codes of Practice)




	
	Name of document

	· Laws
	Acts and regulations

	· Standards
	Bedding depth, level and falls
Shape, depth and dimensions of sub base level
Finished level of base material

	· Codes
	Code of practice 2019




	Outcome for Activity 4
	 Satisfactory 	
 Not satisfactory

	Trainer/Assessor comments
	


 

	· 

	List the components for four (4) common surface drainage systems used in landscape construction.




	System
	Components

	· Spoon
	U-shaped concrete channel
Grate cover
Dturdy and long lasting

	· Channel and grate
	Trash box and outlet options
End caps
Gratings

	· Pit
	Curbs
Gutters
Inlets

	· Contour
	Disturbed slopes
Stable outlets
End caps




	Outcome for Activity 5
	 Satisfactory 	
 Not satisfactory

	Trainer/Assessor comments
	



 

	· 

	List the advantages and disadvantages of drainage behind and through the build wall (as shown).








	Drainage pipe behind the wall

	Advantages

	Easier to install

	Disadvantages

	water flow is less efficient



	Drainage pipe through the wall 

	Advantages

	Water flow is more efficient

	Disadvantages

	Not as aesthetic 




	Outcome for Activity 6
	 Satisfactory 	
 Not satisfactory

	Trainer/Assessor comments
	



 

	· 

	Explain the purpose of a slump test. Describe the process of how such a test is conducted.




	Response 

	The slump test measures the consistency of fresh concrete before it sets. It is performed to check the workability of freshly made concrete, and therefore the ease with which concrete flows. Fill the cup with freshly mixed concrete and pack it well. Place the filled cup upside-down on a flat, rigid surface. With your hands, carefully vibrate the cup in a steady lifting motion without stopping. Measure the distance of the slump with a ruler.




	Outcome for Activity 7
	 Satisfactory 	
 Not satisfactory

	Trainer/Assessor comments
	


 

	· 

	Research and list a range of curing compounds and the advantages of using each type




	Curing compound
	Advantages

	· Eco-Cure
	No solvents, Hydrocarbons or Resins of any type
No wax or wax based additives
No odour before or after application

	· Evencure AA
	Reduces plastic shrinkage
Totally waterbased
Will not affect adhesion of after trades

	· Evencure AC
	Dries to a clear finish
Complies with Australian Standard AS3799
Achieves water retention of 90% or greater

	· Evencure BCP
	Complies with Australian Standards AS3799
Achieves water retention of >90%
Contains no wax




	Outcome for Activity 8
	 Satisfactory 	
 Not satisfactory

	Trainer/Assessor comments
	



 

	· 

	List environmentally safe products for cleaning.




	Response 

	On-Crete's General Purpose Concrete Cleaner
30 SECONDS® Outdoor Cleaner products




	Outcome for Activity 9
	 Satisfactory 	
 Not satisfactory

	Trainer/Assessor comments
	


 

	· 

	Have team members take photos and videos of your involvement with concrete features. 

Identify each photo / video with a letter label and describe each photo / video in the table below. Submit the photo / video files along with this workbook.




	Advantages

	A
	

	B
	

	C
	

	D
	

	E
	

	F
	

	G
	

	H
	

	I
	

	J
	

	K
	

	L
	

	M
	

	N
	

	O
	

	P
	

	Q
	

	R
	

	S
	

	T
	

	U
	

	V
	

	W
	

	X
	

	Y
	

	Z
	




	Outcome for Activity 10
	 Satisfactory 	
 Not satisfactory

	Trainer/Assessor comments
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