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CPCCBC4001 
Apply building codes and standards to the construction process for Class 1 and 10 buildings 

ASSESSMENT SUMMARY

The assessment activities for CPCCBC4001 Apply building codes and standards to the construction process for Class 1 and 10 buildings cover all aspects of the unit of competency. For Apprentices/Trainees, this includes supervisor completion of the Apprentice/Trainee Record (ATR). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be fair, flexible, valid and reliable. If a Participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a Participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the Participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a Participant does not answer all questions or perform all tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. 

The Trainer/Assessor can provide the Participant with additional information on interpreting the assessment outcomes and guide the Participant’s options. If a Participant is still deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result as per the process in the Student Handbook. 

By signing below, the Participant acknowledges:
· They understand the assessment instructions and requirements, and consent to being assessed. 
· The work submitted is to be their own work – with the work of/with others needing to be clearly acknowledged and documented. 
· They consent to any photo/video recording of their work that occurs during assessment. 

	Participant name
	Dawei Yang

	Participant signature
	


	Pre-requisite unit(s) to be achieved and authenticated prior to undertaking assessment

	 Not applicable



	Task
	Date completed
	Assessment Results 

	Theory Exam
	Select Date.
	 Satisfactory 
	 Not Satisfactory

	Workbook 
	Select Date.
	 Satisfactory 
	 Not Satisfactory

	Practical Assessment
	Select Date.
	 Satisfactory 
	 Not Satisfactory

	Outcome for CPCCBC4001
	Select Date.
	 Competent
	 Not Yet Competent



	Evidence requirements checklist (ticked by assessor and evidence supplied to RTO)

	 Theory Exam
 Workbook
 Practical Assessment
	 Fire protection inspection checklist
 Documentation of design and construction (suitability or evidence of suitability)



	Assessor name
	

	Assessor signature
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THEORY EXAM


	Participant name
	Dawei Yang




	FOR THE PARTICIPANT

	Instructions

	· You will complete written questions as outlined on the following pages. You must attempt all questions and provide enough detail in your responses to demonstrate your knowledge.
· It is anticipated that you should complete this assessment within two (2) hours, but additional time may be allowed upon negotiation with the Assessor.
· You must complete all questions unassisted by the Assessor or other personnel but may refer to reference material as needed. All questions must be answered correctly for a ‘Satisfactory’ assessment outcome to be awarded. 
· An oral examination may be allowed under certain circumstances, whereby your answers will be documented by another party. 
· Any written questions that are incomplete, or not answered satisfactorily will need to be completed again after further training support.
· If you answer a question incorrectly but modify your response, put your initials next to the written change (or the Assessor must initial a verbal change).

	Resources required

	Pen




	FOR THE ASSESSOR

	Instructions

	· Where oral examination has occurred, ensure that this is acknowledged in writing (e.g. FT001 and Assessor Comments)
· All questions must be satisfactorily demonstrated by the Participant for a Satisfactory determination (indicated by an Assessor tick to the right of the question).
· Assessors are to complete marking in pen of a different colour to the Participant.
· If the Participant verbally modifies their response, write in the modified response verbatim and put your initials next to the written change. 


[bookmark: _Ref396827952]

	[bookmark: _Hlk82780839]ASSESSOR COMMENTS

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	




[bookmark: _Ref127183513]Explain why it is important to understand references the NCC makes to Australian Standards.

	Answer
	 the NCC on behalf of the Commonwealth and State and Territory Governments. It provides the minimum mandatory requirements for safety, health, amenity, and sustainability for building works of both new and existing buildings throughout Australia. 
	




[bookmark: _Ref127184725]You have been asked to develop a tender proposal for a housing development taking State/Territory. Discuss in depth any legislation and Codes your submission must comply with?

	Answer
	Building Act 1975
Building Regulation 2006
Environmental Protection Act 1994 
Australian Consumer Law (ACL) 
Competition and Consumer Act (CCA) 2010
Disability (Access to Premises-Buildings) Standards 2010
Environment Protection and Biodiversity Conservation (EPBC) Act 1999
National Prequalification System for Civil (Road and Bridge) Construction Contracts
Native Title Act 1993
Work Health and Safety Act 2011
Work Health and Safety Act 2011
Qld Codes of Practice

	




[bookmark: _Ref127186634]Describe the listed NCC compliance assessment methods used to determine compliance using a Performance Solution pathway.

	Answer
	Assessment method
	Description
	

	
	Evidence of suitability
	 This entails showing evidence that the use of material, plumbing, and drainage product or form of construction or design meets the Performance Requirements or a DTS Provision. 
	

	
	Verification methods
	Verification Methods include quantifiable or predetermined acceptable criteria that must be achieved by the given compliance option. 
	

	
	Comparison with DTS Provisions
	This method applies to Performance Solutions. It involves doing a comparative analysis to determine whether Performance Solutions provide the superior or same level of health, safety, amenity, or sustainability as using the DTS provisions.
	

	
	Expert Judgement
	An expert can either be a person or an organisation with the necessary skills and experience to make a judgement concerning NCC compliance. 
	




[bookmark: _Ref127263388]Discuss the listed levels found in the NCC Performance Hierarchy.

	Answer
	Performance Hierarchy
	Description
	

	
	Objectives
	Middle level
	

	
	Functional statements
	Middle level
	

	
	Performance requirements
	Top level
	

	
	Building Solutions
	Level 3
	




[bookmark: _Ref127278250]Why may you need to use a combination of Performance Solutions and Deemed-to-Satisfy (DtS) solutions to comply with the Performance Requirements of the NCC?

	Answer
	 many components inside a building are protected by Performance Criteria.
	




[bookmark: _Ref128115391]The client is showing you the plans for them to build a duplex on their site. Determine what classification would be assigned to this building. Explain your answer.

	Answer
	Class two
A building containing two or more sole-occupancy units. Each unit must be a separate dwelling. 

	




[bookmark: _Ref128115393]Another client would like to install a swimming pool. Determine what classification would be assigned to this. Explain your answer.

	Answer
	Class 10b
	



[bookmark: _Ref128119881]Explain why the plans for a residential building with landscaping features may have more than one classification.

	Answer
	a building or part of a building may have multiple purposes and, therefore, multiple classifications.
	




[bookmark: _Ref128118928]AS 2870 is referenced in both NCC Volumes One and Two. Respond in the table, what the Australian Standard is referenced in relation to.

	Answer
	NCC Volume
	Referenced in relation to
	

	
	Volume One
	NCC Volume One contains technical design and construction requirements for all Class 2 to 9 buildingNCC Volume One contains technical design and construction requirements for all Class 2 to 9 buildings s 
	

	
	Volume Two
	NCC Volume Two contains technical design and construction requirements for certain residential and non-habitable buildings and structures. 
	




[bookmark: _Ref128120840]Outline workplace policies and procedures that should be held on-site.

	Answer
	Work Health and Safety Act 2011
Qld Codes of Practice

	



[bookmark: _Ref127188238]Why is it important to document quality assurance and quality control processes relevant to the build?

	Answer
	Having quality assurance in place helps companies maintain high standards of manufacturing. Quality control ensures that the final product reflects these high standards and satisfies the customer's needs
	




[bookmark: _Ref127863024]Discuss the basic principles of structural design that must be considered in any building design.

	Answer
	Structural design is the methodical investigation of the stability, strength and rigidity of structures. The basic objective in structural analysis and design is to produce a structure capable of resisting all applied loads without failure during its intended life.
	



[bookmark: _Ref128124628]Provide five conformity assessment pathways that can be used individually, or in combination, to demonstrate product compliance.

	Answer
1.



2.



3.



4.



5.
	
Testing



inspection


verification



Certification



accreditation



	




[bookmark: _Ref128122622]Provide the six (6) bushfire attack level ratings that AS 3959 uses to establish the requirements for construction. Explain each rating.

	Answer
1.



2.



3.



4.



5.



6.
	BAL Low
There is insufficient risk to warrant specific construction requirements

BAL 12.5
Ember attack. (BAL 12.5 Construction Requirements)

BAL 19
Increasing levels of ember attack and burning debris ignited by windborne embers, together with increasing heat flux. 

BAL 29
 Increasing levels of ember attack and burning debris ignited by windborne embers, together with increasing heat flux. (BAL 29 Construction Requirements)

BAL 40
Increasing levels of ember attack and burning debris ignited by windborne embers, together with increasing heat flux and with the increased likelihood of exposure to flames. (BAL 40 Construction Requirements)

BAL FZ
Direct exposure to flames from fire, in addition to heat flux and ember attack. (BAL FZ Construction Requirements)

	




[bookmark: _Ref128122625]Complete the table below by identifying the type of fire-resisting construction (i.e. Type A, Type B, or Type C) given the following class of building and number of storeys each class of building has.

	Answer
	Rise in Storeys
	Class of building:
2,3,9
	Class of building:
5,6,7,8
	

	
	4 or more
	A
	B
	

	
	3
	B
	B
	

	
	2
	B
	B
	

	
	1
	C
	C
	




[bookmark: _Ref128125400]Provide a brief explanation of each step of the development of Performance Solutions.

	Answer
	Steps in Developing Performance Solutions
	Brief explanation of each step
	

	
	Prepare a performance-based design brief
	a document that serves as a record of all the fundamental activities and outcomes of the Performance Solution design process, as agreed during the stakeholder negotiation process. When completed, the PBDB becomes the roadmap for the proposed solution. 
	

	
	Carry out analysis, modelling, or testing
	The method of analysis, modelling, or testing must be chosen according to what is appropriate to the complexity of your project and carried out following what is agreed by stakeholders in the PBDB.
	

	
	Collate and evaluate results
	The results from the previous step must be collated for analysis. Results from multiple trials or design scenarios may have to be considered. 
	

	
	Prepare a final report
	The final report is mandatory documentation that must clearly demonstrate compliance with the NCC Performance Requirements.
	



[bookmark: _Ref127265454]Discuss two (2) properties, two (2) characteristics and two (2) limitations of concrete when used for buildings. 

	Answer
	
	Concrete
	

	
	Properties
	1. Elastic Properties
	

	
	
	2. Durability
	

	
	Characteristics 
	1. workability
	

	
	
	2. Strength
	

	
	Limitations
	1. disintegration
	

	
	
	2.  cracking
	




[bookmark: _Ref127265456]Discuss three (3) benefits of using glass in buildings.

	Answer
1.





2.





3.
	
Waterproof and Dustproof.




Recyclable.






Easily Moulded

	



[bookmark: _Ref128129905]Respond to the following items regarding zero-energy building.

	Answer
	Item
	Zero energy building
	

	
	Definition
	Zero-energy building is the construction of buildings that produce as much energy as they consume.
	

	
	One (1) technique used in zero energy building
	 solar energy
	

	
	The procedure in implementing the technique you have identified
	Install the solar panel
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WORKBOOK


	Participant name
	Dawei Yang




	FOR THE PARTICIPANT

	Instructions

	· You will complete written activities as outlined on the following pages. You must attempt all questions and provide enough detail in your responses to demonstrate your knowledge.
· The timeframe for these tasks will be established by your Assessor or Training Plan, but additional time may be allowed upon negotiation with the Assessor.
· You must complete all questions unassisted by the Assessor or other personnel but may refer to reference material as needed. All questions must be answered correctly for a ‘Satisfactory’ assessment outcome to be awarded. 
· An oral examination may be allowed under certain circumstances, whereby your answers will be documented by another party. 
· Any written questions that are incomplete, or not answered satisfactorily will need to be completed again after further training support.
· If you answer a question incorrectly but modify your response, put your initials next to the written change (or the Assessor must initial a verbal change).

	Resources required

	Pen




	FOR THE ASSESSOR

	Instructions

	· Where oral examination has occurred, ensure that this is acknowledged in writing (e.g. FT001 and Assessor Comments)
· All questions must be satisfactorily demonstrated by the Participant for a Satisfactory determination (indicated by an Assessor tick to the right of the question).
· Assessors are to complete marking in pen of a different colour to the Participant.
· If the Participant verbally modifies their response, write in the modified response verbatim and put your initials next to the written change. 




	ASSESSOR COMMENTS

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	




NOTE

At times, you will be provided with a specific context to which you must respond, otherwise it is anticipated that you will use a workplace of your choosing (your own, or hypothetical) to provide the context to the task.

At all times, the responses in your assessment must reference Australian (Queensland or Federal) documentation, including legislation, regulations, codes of practice, standards and guidance publications.

	ACTIVITY 1  [bookmark: _Ref35349341]

	Access the National Construction Code (NCC) to:
a) Briefly explain what the General Requirements of buildings are.
b) Briefly explain what the Performance Requirements of buildings are.
c) Briefly explain the relationship between a building’s Performance Requirements and compliance options (e.g. performance solutions, deemed-to-satisfy solutions).



	a)  Briefly explain what the General Requirements of buildings are.

	General Requirements which cover other aspects of applying the NCC. This includes its interpretation, reference documents, the acceptance of design and construction (including related evidence of suitability/documentation) and the classification of buildings within the NCC.

	b) Briefly explain what the Performance Requirements of buildings are.

	Performance requirements typically comprise a set of criteria which stipulate how things should perform or the standards that they must achieve in a specific set of circumstances. This is as opposed to prescriptive specifications which set out in precise detail how something should be done.

	c) Briefly explain the relationship between a building’s Performance Requirements and compliance options (e.g. performance solutions, deemed-to-satisfy solutions).

	Compliance with the NCC's mandatory Performance Requirements is achieved by developing a Performance Solution, a DTS Solution, or a combination of the two. A Performance Solution uses any method other than the DTS Provisions to comply with the Performance Requirements.



	Satisfactory Outcome
	
	




	ACTIVITY 2  [bookmark: _Ref35349352]

	Provided in the table below are different building elements of Class 1 and Class 10 buildings. For each building element, provide one performance requirement according to the National Construction Code (NCC) Volume 2.
a) Structural stability and resistance.
b) Weatherproofing.
c) Automatic fire warning for occupants.
d) Personal hygiene and other facilities.
e) Movement to and within a building.



	a) Structural stability and resistance

	perform adequately under all reasonably expected design actions

	b) Weatherproofing

	For concrete, compressed fibre-cement and fibre-cement sheet flooring, the floor of the room must be water resistant

	c) Automatic fire warning for occupants

	 provided with a smoke alarm system complying with S20C3 within sole-occupancy units

	d) Personal hygiene and other facilities

	the disability or other particular needs of the occupants

	e) Movement to and within a building

	walking surfaces must have safe gradients



	Satisfactory Outcome
	
	




	ACTIVITY 3  [bookmark: _Ref128058640]

	Provided in the table below are different building elements of Class 1 and Class 10 buildings. Describe the how the verification method for each building element of the buildings must be implemented.



	a) Structural robustness

	 Deemed-to-Satisfy Solution

	b) Room space or height

	Performance solution



	Satisfactory Outcome
	
	




	ACTIVITY 4  [bookmark: _Ref128127326]

	Access and review the following documents included with this workbook regarding quality management systems of Cascade Peaks Construction:
Handout 2 (HO2) Cascade Peaks Construction Quality System – Beginning Construction
Handout 3 (HO3)Cascade Peaks Construction Quality System – Mandatory Inspections

Once you have accessed and reviewed the documents above, answer the following questions:
a) Briefly explain why proper procedures for demolition and temporary fencing is needed during construction. 
b) Briefly explain why mandatory inspections are needed during the construction of new buildings.
c) Identify two (2) tasks that should be done before demolition starts.
d) Identify two (2) characteristics that temporary fencing around a construction site should have.
e) Identify two (2) inspections that must be done by a building certifier.
f) Identify two (2) areas in a building that must be inspected for weatherproofing by a building certifier.



	a) Briefly explain why proper procedures for demolition and temporary fencing is needed during construction. 

	Temporary fencing / barrier systems are generally used to secure work sites. They also contribute to public safety by providing a physical barrier between people and demolition, excavation, construction and maintenance sites.

	b) Briefly explain why mandatory inspections are needed during the construction of new buildings.

	The objective of a building inspection is to determine whether the structure complies with building code requirements. Buildings are inspected to ensure that zoning bylaws, residents' health and safety, and building standards are followed. It is required for new construction, renovations, and other trades.

	c) Identify two (2) tasks that should be done before demolition starts.

	Obtain A Demolition Permit.
Hazardous materials diagnosis


	d) Identify two (2) characteristics that temporary fencing around a construction site should have.

	The gates should not project beyond the site when opened
Be difficult to climb to present trespassers


	e) Identify two (2) inspections that must be done by a building certifier.

	Footing and frame

	f) Identify two (2) areas in a building that must be inspected for weatherproofing by a building certifier.

	Wet area and external area



	Satisfactory Outcome
	
	




	ACTIVITY 5  [bookmark: _Ref128128349]

	Access and review: 
Handout 4 (HO4) Cascade Peak Construction’s Safety Policies and Procedures 

After reviewing the policies and procedures, provide the following information below:
a) Cascade Peaks Construction’s safety policy.
b) Cascade Peaks Construction’s field standard safety clothing and equipment policy.
c) Four (4) registers that Cascade Peaks Construction should keep regarding the safety of its workers.
d) Five (5) safety clothing that workers must wear regardless of their task.



	a) Cascade Peaks Construction’s safety policy.

	Cascade Peak Construction Pty Ltd is committed to creating a workplace environment that is conducive to safety as well as to productivity. To achieve this aim, management and employees will comply with all relevant legislation and safety regulations that are in force both in the office and in the client’s work environments.

	b) Cascade Peaks Construction’s field standard safety clothing and equipment policy.

	High visibility clothing to be worn.
Pedestrians to follow marked walkways.
Operators of forklifts and other vehicles to use designated lanes.
All materials and equipment to be stored in a safe manner in their allocated areas..
Report to the HSR all accidents or injuries of any nature and the damage to or loss or theft of any equipment.
Think before acting. If a situation has the potential to be hazardous extra care must be taken. Even party leaders can make the wrong choice of options. If you believe this to be the case, talk it over.
Ensure that all instructions shall be carried out in a tidy and safe manner on the site.
All manual lifting is to be conducted safely. Manual lifting of material where it is unreasonable for such to be conducted or to do so creates a danger of injury to persons or damage to equipment is forbidden.
Keep gear in first class condition. If an accident does occur it is much better to be cut with a sharp axe than a blunt one..
While working on public roads special care must be taken. Safety vests must be worn and “Men and Work” signs erected at both ends if the job.
Safety boots (steel caps) are mandatory. Some relaxation of this may be allowed in wet area.
There will be numerous work sites that have additional safety requirements.
Chainsaws are to be used by experienced personnel. Safety helmets and ear protection will be worn.
Whilst loose flowing clothing may be appropriate for our climate, industrial type clothes provide greater protection in hazardous situations. If hair is to be worn long it will be securely tied back from the face.
Personal protection. Sunscreen, insect repellent, medication (e.g. hay fever) to be used when necessary. Most important. If you are allergic to anything make sure that the person you are working with knows about it and what to do in case of emergency.
.


	c) Four (4) registers that Cascade Peaks Construction should keep regarding the safety of its workers.

	Phone/contact details – Staff Medical Advisors, Ambulance, Police, etc.
Accident: Minor and Serious
Inductions
Safety training courses attended

	d) Five (5) safety clothing that workers must wear regardless of their task.

	Steel Cap Footwear (boots) – at discretion of safety officer
Wide Brim Hat
UV protection sunscreen (supplied)
Long sleeve shirts buttoned or affixed at wrist.
Collared shirts 



	Satisfactory Outcome
	
	



	ACTIVITY 6  [bookmark: _Ref128131028]

	Consider the columns in the photo below and answer the following questions:
[image: ]

a) What kind of stress is being applied on the columns by the ceiling?
b) Describe the deformation that the columns are possibly undergoing due to the stress that the ceiling is applying on them.
c) Describe what would happen to the columns if the ceiling were too heavy to be supported.



	a) What kind of stress is being applied on the columns by the ceiling?

	compressive stress

	b) Describe the deformation that the columns are possibly undergoing due to the stress that the ceiling is applying on them.

	Bend

	c) [bookmark: _Ref128134604]Describe what would happen to the columns if the ceiling were too heavy to be supported.

	Break down



	Satisfactory Outcome
	
	




	ACTIVITY 7  [bookmark: _Ref128134618]

	The handrail of a staircase in a two-storey house located in a termite-risk area broke off while a resident was climbing down the stairs. The handrail was hollow and was infested with termites. Upon further inspection, most of the staircase was constructed from untreated timber, and the project plans made no mention of the fact that the house was made in a termite-risk area. 

Given the information above:
a) Identify two factors that contributed to the degradation of the house’s staircase.
b) Identify which Part from the NCC Volume 2 was not properly applied.
c) Briefly explain how the identified clause from the Building Code of Australia Volume 2 was not properly applied.
d) Identify which Australian standard was not properly applied.
e) Briefly explain how the identified Australian standard was not properly applied.
f) Identify one practice endorsed by Safe Work Australia was not properly applied.
g) Briefly explain how the identified practice endorsed by Safe Work Australia was not properly applied.
h) Identify what other defect the house would have considering the deviations of the construction from the code and standard.
i) Describe the extent of the work that needs to be done to rectify the termite infestation.



	a) Identify two (2) factors that contributed to the degradation of the house’s staircase.

	Wet air and lack of maintenance 

	b) Identify which Part from the NCC Volume 2 was not properly applied.

	H1P1

	c) Briefly explain how the identified Part from the NCC Volume 2 was not properly applied.

	Ignore the termite action.

	d) Identify which Australian standard was not properly applied.

	AS 3660.2-2000 

	e) Briefly explain how the identified Australian standard was not properly applied.

	Does not meet a minimum standard for termite management in and around existing buildings and structures as part of Australian Standard's 'Termite management' group of standards.

	f) Identify one practice endorsed by Safe Work Australia was not properly applied.

	Use untreated timber 

	g) Briefly explain how the identified practice endorsed by Safe Work Australia was not properly applied.

	Termite resistant materials
treated timber

	h) Identify what other defect the house would have considering the deviations of the construction from the code and standard.

	Structural reliability

	i) Describe the extent of the work that needs to be done to rectify the termite infestation.

	Replace the damaged timber instead of the treated timber and Choose a termite management system




	Satisfactory Outcome
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CPCCBC4001 
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PRACTICAL ASSESSMENT


	Participant name
	Dawei Yang




	FOR THE PARTICIPANT

	Instructions

	· The tasks outlined on the following pages will require performance of normal workplace activities, as a result of a structured activity set by an Observer in the workplace or a simulated activity set by your Assessor/Observer. 
· The timeframe for these tasks will be established by your Assessor/Observer, in consideration of location conditions and industry requirements.
· You must complete all tasks unassisted by the Assessor or other personnel, unless the steps note this assistance. 
· You must attempt all tasks (and itemised steps) for a ‘Satisfactory’ assessment outcome to be awarded.
· For any observation conducted that is incomplete, or without satisfactory performance, the observation will need to be completed again after further training support.




	FOR THE ASSESSOR/OBSERVER

	Instructions

	· The following observation record should be used to judge and record your observations of the Participant as they complete the task(s) set. You must record your observations of the Participant’s performance. 
· For each occasion, indicate the task performed and whether it was a simulation or workplace-based task. 
· Any simulated assessment must ensure the Participant still performs under workplace conditions which reflect industry standards.
· In the comments, provide clear detail regarding the task that the Participant was required to do (e.g. PPE used, materials handled, attachments connected, plant types).
· All steps must be satisfactorily demonstrated by the Participant for a ‘Satisfactory’ determination (indicated by an Assessor tick to the right of each itemised step, or an Observer tick to the right of each itemised step, and confirmation by an Assessor in the Assessor Comments).
· Where you have determined that one or more task steps have not been satisfactorily demonstrated, provide the Participant with additional support and outline details of such assistance in the Assessor/Observer Comments. Allow the Participant two (2) further opportunities to demonstrate the task again to allow an opportunity for a ‘Satisfactory’ assessment outcome to be achieved. 
· If after three (3) attempts the Assessor determines that the Participant cannot demonstrate the required steps, a ‘Not Satisfactory’ outcome is to be determined.





	TASK OUTCOME

	Task
	Date
	Task Type (Tick)
	Location
	Task outcome (Tick)

	
	
	
	
	Satisfactory
	Not Satisfactory

	Task 1
	Select Date.
	þ Workplace
 Simulation
	
	
	



	ASSESSOR COMMENTS: GENERAL

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	



	ASSESSOR COMMENTS: PRACTICAL TASK 1

	þ Individual student (as named on cover page)
 Multiple students [ All from Attendance Report,  Specific students involved – identify students]

	Task
	Provide detail 

	1.1A. 1.1B. 1.1C. 
	Specify () where building classifications, criteria requirements and performance solutions were documented:
¨ Workplace Quality document  Quality Assurance Template  Other (please specify): 


 Document attached as evidence


	1.2D. 
	Specify () who was consulted regarding compliance options: 
¨ Project management  Relevant tradesperson  Builder  Supplier 
 Other (please specify): 

	1.3C. 
	Specify existing building checked for compliance with active fire protection requirements:


þ Is checklist used attached as evidence





CPCCBC4001
Apply building codes and standards to the construction process for Class 1 and 10 buildings

	Practical Task 1 

	Description of task:
The participant must demonstrate the skills and knowledge to apply building codes and standards to the construction process one Class 1 or 10) building or structure project to a maximum of two storeys. Documented evidence of all criteria must be presented (template (HO1) available for use if required)The participant must also inspect one existing buildings for fire protection compliance using workplace or created document (See HO5 for information). Assessor and observer will be looking for evidence including:
· Classify building and document findings.
· Read the plans and specifications to determine the nature of the building, its use and arrangement.
· Read and correctly interpret relevant Parts of the NCC and related Australian Standards for the project.
· Determine and document the classification applicable to the building and all ancillary buildings and structures. (template available- HO1)
· Determine construction compliance requirements.
· Determine NCC Performance Requirements relevant to Class 1 and 10, up to two storeys, building projects.
· Determine range of criteria to ensure that construction methods comply with NCC Performance Requirements.
· Identify and document non-conforming construction methods against NCC Performance Requirements. (template available- HO1)
· Propose and discuss Performance Solution with design and building and construction professionals. Document consultation. (template available- HO1)
· Analyse and apply Assessment Methods to determine compliance with Performance Solution or Deem-to-Satisfy Solution (DTS). (template available- HO1)
· Meet the evidence of suitability requirements for building materials and products stated in the NCC.
· Complete documentation demonstrating how the project design and construction will meet NCC requirements (template available- HO1) including:
· energy efficiency
· damp and weatherproofing
· fire safety
· health and amenity
· structure
· safe movement and access
· ancillary provisions
· Determine fire protection requirements.
· Read the NCC and other legislative requirements for passive and active fire control elements in buildings.
· Write or obtain a checklist describing the level of fire resistance required for the construction of various buildings.
· Inspect one existing building for compliance with passive and active fire protection requirements.

These tasks may be simulated or real. The Participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. The Observer is to provide detailed comments on the tasks completed by the Participant (on the Observer Comments, overleaf). The Assessor is to verify the Observer’s comments, noting their findings in the Assessor Comments (on the back of the Practical Assessment cover page) and provide the assessment outcome.

	Resources required: 
Construction plans, drawings and specifications for one (1) building Class 1 or 10) building or structure project to a maximum of two storeys; workplace quality policies and procedures; technology to access building and related industry codes, standards and manufacturer product information and materials specifications; Technology to access the NCC and current relevant Acts and Regulations. PPE as required. Documentation of design and construction (suitability or evidence of suitability) (template available- (HO1).Fire protection checklist.

	Observer details

	Name of observer:
	Yanzhong Zhu

	Role of observer 
(Confirm suitability to sign)
	Builder 

	Email address of observer
	steve.zhu.au@hotmail.com

	Signature of observer:
	
	Date:
	30/09/2023



	When completing the task, did the Participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	1 Classify building

	[bookmark: _Ref128141140]Read the plans and specifications to determine the nature of the building and ancillary provisions, use and arrangement.
	þ
	[bookmark: _Ref128141144]Read and correctly interpret relevant Parts of the NCC and related Australian Standards for the project.
	þ
	[bookmark: _Ref128141148]Determine and document the classification applicable to the building and all ancillary buildings and structures. (attach evidence -template available- HO1)
	þ
	2 Determine construction compliance requirements

	[bookmark: _Ref128143424]Determine NCC Performance Requirements relevant to Class 1 and 10, up to two storeys, building projects. (attach evidence -template available- HO1)
	þ
	[bookmark: _Ref128143430]Determine range of criteria to ensure that construction methods comply with NCC Performance Requirements. (attach evidence -template available- HO1)
	þ
	[bookmark: _Ref128143438]Identify and document non-conforming construction methods against NCC Performance Requirements. (attach evidence -template available- HO1)
	þ
	[bookmark: _Ref128141784]Propose and discuss Performance Solution with design and building and construction professionals. Document consultation. (attach evidence -template available- HO1)
	þ
	[bookmark: _Ref128143579]Analyse and apply Assessment Methods to determine compliance with Performance Solution or Deem-to-Satisfy Solution (DTS). (attach evidence -template available- HO1)
	þ
	[bookmark: _Ref128143590]Meet the evidence of suitability requirements for building materials and products stated in the NCC.
	þ
	[bookmark: _Ref128143524]Complete documentation demonstrating how the project design and construction will meet NCC requirements for energy efficiency (attach evidence -template available- HO1).
	þ
	[bookmark: _Ref128143527]Complete documentation demonstrating how the project design and construction will meet NCC requirements for damp and weatherproofing (attach evidence -template available- HO1).
	þ
	[bookmark: _Ref128143529]Complete documentation demonstrating how the project design and construction will meet NCC requirements for fire safety (attach evidence -template available- HO1)
	þ
	[bookmark: _Ref128143531]Complete documentation demonstrating how the project design and construction will meet NCC requirements for health and amenity. (attach evidence -template available- HO1).
	þ
	[bookmark: _Ref128143533]Complete documentation demonstrating how the project design and construction will meet NCC requirements for structure. (attach evidence -template available- HO1).
	þ
	[bookmark: _Ref128143536]Complete documentation demonstrating how the project design and construction will meet NCC requirements for safe movement and access. (attach evidence -template available- HO1).
	þ
	[bookmark: _Ref128143539]Complete documentation demonstrating how the project design and construction will meet NCC requirements for ancillary provisions. (attach evidence -template available- HO1).
	þ
	3 Determine fire protection requirements.

	[bookmark: _Ref128143628]Read the NCC and other legislative requirements for passive and active fire control elements in buildings.
	þ
	[bookmark: _Ref128143542]Write or obtain a checklist describing the level of fire resistance required for the construction of various buildings.
	þ
	[bookmark: _Ref128142062]Inspect one existing building for compliance with passive and active fire protection requirements (attach checklist as evidence)
	þ




	Observer comments:
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