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	Participant name
	Lucy Muston 

	Date
	02/04/2025



	Building and construction project
	Registered Training Organisation (RTO) Facility 

	Project overview
	The RTO Facility is to be designed to accommodate both office and educational/training functions. The facility includes classrooms for training purposes, alongside office spaces for administrative operations, making it suitable for use by a Registered Training Organisation (RTO). 

	Building classification
	 Class 1 – 10 buildings, max two storeys
 Class 2 – 9 building, Type C only constructions

Specify class: Class 9b – Assembly Building (Educational Facility)

	Project site address
	878 Beaudesert Rd. Coopers Plains QLD 

	State/territory where project is undertaken
	QLD

	Construction plan documents reviewed
	Yes 



Building Legislation
List two (2) relevant legislations
	Building legislation
	Plans comply 
	Explanation

	Work Health and Safety Act 2011 (WHS Act)
	 Yes
	 No
	Ensures that all workplaces, including RTO facilities, provide a safe environment for workers, students, and visitors. It covers aspects such as safe building design, fire safety measures, and emergency evacuation plans, ensuring compliance with workplace health and safety regulations during both construction and operation.

	Disability (Access to Premises – Buildings) Standards 2010 (DDA Standards)
	 Yes
	 No
	Ensures that RTO facilities are designed to be accessible for people with disabilities. It mandates compliance with requirements such as ramps, lifts, accessible toilets, wide doorways, and tactile signage, ensuring equal access to education and training environments in line with the Disability Discrimination Act 1992.



Australian Standards
Provide two (2) relevant standards
	Australian Standards
	Plans comply 
	Explanation

	AS 3745:2010 (Planning for Emergencies in Facilities)
	 Yes
	 No
	Provides guidelines for developing emergency plans, procedures, and evacuation strategies for buildings, including RTO facilities. It ensures that the facility has proper emergency exits, fire safety measures, and trained personnel to manage emergencies such as fires, medical incidents, or natural disasters, enhancing the safety of students, staff, and visitors.

	AS/NZS 3000:2018 (Wiring Rules)
	 Yes
	 No
	Establishes safety standards for electrical installations in buildings, ensuring that all electrical systems in an RTO facility are designed and installed to prevent hazards such as electric shocks and fires. This standard outlines the requirements for circuit protection, grounding, and safe wiring practices, ensuring compliance with Australian electrical safety regulations.




NCC Requirements
Fire Safety x 1
	Requirements
	Plans comply 
	Explanation

	National Construction Code (NCC) Part E1 – Fire Fighting Equipment
	 Yes
	 No
	Requires that buildings, including RTO facilities, have appropriate fire protection measures in place. This includes the installation of fire extinguishers, fire hose reels, and sprinkler systems where required, ensuring that occupants have access to fire suppression equipment in case of an emergency. These provisions help to minimise fire risks and ensure compliance with Australian building safety regulations.




Health and amenity x 1
	Requirements
	Plans comply 
	Explanation

	National Construction Code (NCC) Part F2 – Sanitary and Other Facilities
	 Yes
	 No
	Outlines the health and amenity requirements for buildings, including RTO facilities. It mandates the provision of adequate toilet facilities, handwashing stations, and drinking water for all occupants. The number and accessibility of these facilities must meet specific standards to ensure the health, comfort, and wellbeing of students, staff, and visitors.







Safe movement and access x 1
	Requirements
	Plans comply 
	Explanation

	National Construction Code (NCC) Part D1 – Access and Egress
	 Yes
	 No
	Outlines requirements for safe movement and access within a building. It ensures that RTO facilities have sufficient and accessible pathways for entry, exit, and movement throughout the building. This includes provisions for accessible doorways, ramps, hallways, and stairways, as well as clearly marked emergency exits, to allow safe and efficient evacuation in case of an emergency, while also ensuring ease of access for people with disabilities.




Energy efficiency x 1
	Requirements
	Plans comply 
	Explanation

	National Construction Code (NCC) Part J – Energy Efficiency
	 Yes
	 No
	Sets requirements for the energy efficiency of buildings, including RTO facilities. This includes regulations on insulation, lighting, heating, cooling, ventilation, and the overall design of the building to reduce energy consumption. The aim is to ensure that the facility is environmentally sustainable, minimising energy use and operational costs while maintaining comfortable indoor conditions for occupants.
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