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RIICWM402E 
Supervise civil works contractors 

ASSESSMENT SUMMARY

The assessment activities for RIICWM402E Supervise civil works contractors cover all aspects of the unit of competency. For Apprentices/Trainees, this includes supervisor completion of the Apprentice/Trainee Record (ATR). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be fair, flexible, valid and reliable. If a Participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a Participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the Participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a Participant does not answer all questions or perform all tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. 

The Trainer/Assessor can provide the Participant with additional information on interpreting the assessment outcomes and guide the Participant’s options. If a Participant is still deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result as per the process in the Student Handbook. 

By signing below, the Participant acknowledges:
· They understand the assessment instructions and requirements, and consent to being assessed. 
· The work submitted is to be their own work – with the work of/with others needing to be clearly acknowledged and documented. 
· They consent to any photo/video recording of their work that occurs during assessment. 


	Participant name
	Brodie Page

	Participant signature
	



	Pre-requisite unit(s) to be achieved and authenticated prior to undertaking assessment

	 Not applicable 



	Task
	Date completed
	Assessment Results 

	Theory Exam
	Select Date.
	 Satisfactory 
	 Not Satisfactory

	Practical Assessment
	Select Date.
	 Satisfactory 
	 Not Satisfactory

	Outcome for RIICWM402E
	Select Date.
	 Competent
	 Not Yet Competent



	Evidence requirements checklist (ticked by assessor and evidence supplied to RTO)

	 Theory Exam
 Practical Assessment
	 Completed team WHS training need
 Completed job plan



	Assessor Name
	

	Assessor Signature
	


Theory Exam - RIICWM402E Supervise civil works contractors
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THEORY EXAM


	Participant name
	Brodie Page




	FOR THE PARTICIPANT

	Instructions

	· You will complete written questions as outlined on the following pages. You must attempt all questions and provide enough detail in your responses to demonstrate your knowledge.
· It is anticipated that you should complete this assessment within two (2) hours, but additional time may be allowed upon negotiation with the Assessor.
· You must complete all questions unassisted by the Assessor or other personnel but may refer to reference material as needed. All questions must be answered correctly for a ‘Satisfactory’ assessment outcome to be awarded. 
· An oral examination may be allowed under certain circumstances, whereby your answers will be documented by another party. 
· Any written questions that are incomplete, or not answered satisfactorily will need to be completed again after further training support.
· If you answer a question incorrectly but modify your response, put your initials next to the written change (or the Assessor must initial a verbal change).

	Resources required

	Pen




	FOR THE ASSESSOR

	Instructions

	· Where oral examination has occurred, ensure that this is acknowledged in writing (e.g. FT001 and Assessor Comments)
· All questions must be satisfactorily demonstrated by the Participant for a Satisfactory determination (indicated by an Assessor tick to the right of the question).
· Assessors are to complete marking in pen of a different colour to the Participant.
· If the Participant verbally modifies their response, write in the modified response verbatim and put your initials next to the written change. 


[bookmark: _Ref396827952]

	[bookmark: _Hlk82780839]ASSESSOR COMMENTS

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	




[bookmark: _Ref97533223]What preparation is required to determine a job plan for a contractor?

	[bookmark: _Hlk85785851]Answer
	Review project drawings, specifications, WHS documents, environmental requirements, site constraints, survey data, and program timelines. Confirm resource needs, risks, and required coordination with other crews.
	




[bookmark: _Ref97535021]How will you share emergency response information relevant to the site and various tasks with sub-contractors?

	Answer
	Through site inductions, pre‑start meetings, toolbox talks, posting information on site boards, and ensuring all contractors receive the Emergency Response Plan (ERP).
	




[bookmark: _Ref97535792]Which on-going risk management procedures do you follow and access when supervising civil work contractors and how do these link to legislative requirements?

	Answer
	Daily pre‑starts, SWMS reviews, site inspections, hazard reporting, and toolbox meetings. These procedures ensure compliance with WHS Act, WHS Regulations, Codes of Practice, and organisational safety systems.
	



[bookmark: _Ref97536472]What are (1) the objectives of the Environmental Management Plan (EMP) and (2) why should you read this EMP as part of planning the job?

	Answer
1.










2.
	Control environmental impacts (dust, noise, erosion, water quality, flora/fauna).

Ensures all site activities comply with environmental controls and legal obligations.
	




[bookmark: _Ref97537005]In the general principles of surveying, what is the importance of ‘working from the whole to the part’ (1) when surveying and (2) how this is achieved?

	Answer
1.







2.
	Ensures accuracy by establishing main control points before detailing smaller areas.

Achieved using primary benchmarks, control networks, and working outwards to fine set‑out points.
	



[bookmark: _Ref97537459]Why is it important to coordinate tasks with other work supervisors and schedule contractor activities?

	Answer
	To avoid clashes, ensure safe access, deliver efficient sequencing of works, and maintain project productivity.
	




[bookmark: _Ref97537789]What processes must you follow to acquire and confirm the acquisition of, required resources at your workplace?

	Answer
	Submit requisitions, review plant/ material schedules, confirm bookings with suppliers or plant hire, and verify deliveries/availability during pre‑start checks.
	




[bookmark: _Ref97538391]How do you communicate site safety requirements to ensure contractors wear PPE suited to the site and task?

	Answer
	During induction, pre‑starts, signage at access points, SWMS briefings, and ongoing supervision.
	




[bookmark: _Ref97538914]What is the ‘rule of thumb’ basis for matching a machine to a job?

	Answer
	Choose the machine that safely delivers the required productivity with appropriate capacity, reach, ground pressure, and suitability for site conditions.
	




[bookmark: _Ref97539430]Supervisors must have knowledge of factors affecting plant performance. What are four (4) factors that can affect plant performance and output and why must supervisors monitor each of these?

	Answer
1.



2.



3.



4.
	Ground conditions – affects traction and production.

Operator skill – impacts safety and efficiency.

Machine condition – reduces breakdowns and delays.

Weather – influences visibility, ground firmness, and safety.
	



[bookmark: _Ref97540244]How do you confirm that the contractor has a job plan available that meets task requirements?

	Answer
	Review their documentation, check alignment with project specifications and SWMS, and confirm understanding during pre‑start.
	




[bookmark: _Ref97541696]What methods can you apply to confirm contractors have communicated instructions to team members and others involved?

	Answer
	Observe pre‑start briefing, check sign‑on sheets, ask workers questions, and observe work practices matching instructions.
	




[bookmark: _Ref97544164]What is required when setting out for work tasks?

	Answer
	Accurate survey points, plans, appropriate instruments, control benchmarks, and clear marking of lines, levels, and offsets.
	




[bookmark: _Ref97544165]What is the importance of the survey pegs during the road set out?

	Answer
	They provide reference for alignment, levels, width, and earthworks cut/fill requirements.
	




[bookmark: _Ref97544497]What methods do you apply when monitoring civil works to ensure the required outcomes or met on a daily basis?

	Answer
	Daily inspections, checklists, progress photos, measurements, quality checks, and reviewing plant performance.
	




[bookmark: _Ref97545658]Name and explain the purpose for three (3) of the different test results the supervisor must be able to read and understand at different hold or witness points of a project.

	Answer
1.





2.





3.
	Compaction test (density/Moisture): Ensures subgrade/sub-base meets spec.

CBR test: Confirms ground strength for pavement design.

Concrete slump test: Confirms workability and compliance before pouring.
	




[bookmark: _Ref97546442]What is the purpose of road surface drainage and what are four (4) elements used to achieve this effectively?

	Answer
Purpose







Element

1.

2.

3.

4.
	Remove water quickly to protect pavement and prevent failures.

· Crossfall
· Table drains
· Culverts
· Subsoil drainage

	



[bookmark: _Ref97546666]What are the effects of inappropriate road drainage infrastructure?

	Answer
	Pavement failure, rutting, erosion, reduced road safety, and increased maintenance costs.
	




[bookmark: _Ref97547060]What are the three (3) main parts of roadway design and the importance of these features?

	Answer
1.







2.






3.
	Subgrade – provides foundation support.

Pavement layers – distribute loads.

Surface layer – provides smooth, safe driving and protection from weather.

	



[bookmark: _Ref97547690]What are four (4) events that might occur on a normal working day that may significantly affect progress of civil works tasks and force the use of contingency plans.

	Answer
1.





2.





3.





4.
	Heavy rain

Plant breakdown

Material supply delays

Unexpected ground conditions (rock/soft spots)
	




[bookmark: _Ref97547693]What are four (4) contingency plans that may be in place to support a civil construction operational plan?

	Answer
1.





2.





3.





4.
	Alternative suppliers

Backup plant availability

Wet‑weather work plans

Re‑sequencing tasks
	



[bookmark: _Ref97549194]What methods do you apply when monitoring worker and contractor performance for safety and compliance?

	Answer
	Inspections, SWMS checks, spot audits, observation of work practices, and safety reporting.
	




[bookmark: _Ref97550128]What is the relationship between waste management and environmental protection?

	Answer
	Correct waste handling prevents contamination, protects waterways, reduces environmental impact, and complies with environmental legislation.
	




[bookmark: _Ref97552476]Describe why supervisors access each of the following types of data.

	Answer

	Geological Data:

Understand ground conditions affecting excavation and stability.






Hydrological Data:

Plan drainage, manage groundwater, prevent flooding.






Meteorological Data:

Identify weather risks affecting safety, production, and material quality.
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PRACTICAL ASSESSMENT


	Participant name
	Brodie Page




	FOR THE PARTICIPANT

	Instructions

	· The tasks outlined on the following pages will require performance of normal workplace activities, as a result of a structured activity set by an Observer in the workplace or a simulated activity set by your Assessor/Observer. 
· The timeframe for these tasks will be established by your Assessor/Observer, in consideration of location conditions and industry requirements.
· You must complete all tasks unassisted by the Assessor or other personnel unless the steps note this assistance. 
· You must attempt all tasks (and itemised steps) for a ‘Satisfactory’ assessment outcome to be awarded.
· For any observation conducted that is incomplete, or without satisfactory performance, the observation will need to be completed again after further training support.




	FOR THE ASSESSOR/OBSERVER

	Instructions

	· The following observation record should be used to judge and record your observations of the Participant as they complete the task(s) set. You must record your observations of the Participant’s performance. 
· For each occasion, indicate the task performed and whether it was a simulation or workplace-based task. 
· Any simulated assessment must ensure the Participant still performs under workplace conditions which reflect industry standards.
· In the comments, provide clear detail regarding the task that the Participant was required to do (e.g. PPE used, materials handled, attachments connected, plant types).
· All steps must be satisfactorily demonstrated by the Participant for a ‘Satisfactory’ determination (indicated by an Assessor tick to the right of each itemised step, or an Observer tick to the right of each itemised step, and confirmation by an Assessor in the Assessor Comments).
· Where you have determined that one or more task steps have not been satisfactorily demonstrated, provide the Participant with additional support and outline details of such assistance in the Assessor/Observer Comments. Allow the Participant two (2) further opportunities to demonstrate the task again to allow an opportunity for a ‘Satisfactory’ assessment outcome to be achieved. 
· If after three (3) attempts the Assessor determines that the Participant cannot demonstrate the required steps, a ‘Not Satisfactory’ outcome is to be determined.





	TASK OUTCOME

	Task
	Date
	Task Type (Tick)
	Location
	Task outcome (Tick)

	
	
	
	
	Satisfactory
	Not Satisfactory

	Task 1
	Select Date.
	 Workplace
 Simulation
	
	
	

	Task 2 (Occasion 1)
	Select Date.
	 Workplace
 Simulation
	
	
	

	Task 2
(Occasion 2)
	Select Date.
	 Workplace
 Simulation
	
	
	



	ASSESSOR COMMENTS

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	



	ASSESSOR COMMENTS: PRACTICAL TASK 2: OCCASION 1

	 Individual student (as named on cover page)
 Multiple students [ All from Attendance Report,  Specific students involved – identify students]

	Task
	Provide detail 

	2.1.B. 
	Specify task to be completed:

 

	2.1.C. 
	Completed Task 1 meets these requirements: 



	2.1.E. 
	Specify tool and method applied to address potential risks, hazards and environmental issues and implement control measures.



	2.1.F. 
	PPE worn/applied (tick or specify):  Hi-viz  Helmet  Gloves  Safety boots
 Eye protection  Ear protection  Other (please specify): 

	2.1.G. 
	Specify method used to consult with contractors:



	2.1.J. 
	Specify method applied to confirm resources are available:



	2.2L. 
	Specify new potential hazards recognised and controlled:



	2.2N. 
	Specify what has been set out:



	2.3A. 
	Specify checks/measurements made:



	2.3D. 
	Communication applied (tick or specify):  Face to face  Marking on pegs  Stringlines 
 UHF  Hand signals  Whistles  Other (please specify): 

	2.3G. 
	Specify adjustments made:



	2.4D. 
	Outline recommendations made:





	ASSESSOR COMMENTS: PRACTICAL TASK 2: OCCASION 2

	 Individual student (as named on cover page)
 Multiple students [ All from Attendance Report,  Specific students involved – identify students]

	Task
	Provide detail 

	2.1.B. 
	Specify task to be completed:



	2.1.E. 
	Specify tool and method applied to address potential risks, hazards and environmental issues and implement control measures:



	2.1.F. 
	PPE worn/applied (tick or specify):  Hi-viz  Helmet  Gloves  Safety boots
 Eye protection  Ear protection  Other (please specify): 

	2.1.G. 
	Specify method used to consult with contractors:



	2.1.J. 
	Specify method applied to confirm resources are available:



	2.2L. 
	Specify new potential hazards recognised and controlled:



	2.2N. 
	Specify what has been set out:



	2.3A. 
	Specify checks/measurements made:



	2.3D. 
	Communication applied (tick or specify):  Face to face  Marking on pegs  Stringlines 
 UHF  Hand signals  Whistles  Other (please specify): 

	2.3G. 
	Specify adjustments made:



	2.4D. 
	Outline recommendations made:




	RIICWM402E
Supervise civil works contractors

	Practical Task 1

	Description of task:
The participant must demonstrate undertaking the role of a civil construction supervisor and prepare a job plan which is to be carried out as part of Practical Task 2. The participant must include documentation demonstrating collating of information. If they do not have adequate existing documentation, they will be required to develop a new template for use or one from another job which illustrates the type of information they require.

As part of this task, the participant is required to demonstrate the skills and knowledge to: 
· access, read and correctly interpret work documentation to ensure all work to be completed is compliant
· identify and address potential risks, hazards and environmental issues, and implement control measures including selecting and wearing site appropriate PPE
· consult with team members to confirm the task requirements 
· organise for the acquisition and availability of required resources
· implement a job plan that meets task requirements

Tasks are at the Assessor’s Discretion, but detail of tasks undertaken must be recorded in the Assessor’s Comments (on the back of the Practical Assessment cover page).

	Resources required: 
Work team, work site, organisational policies, standard operating procedures and plans, safety processes, hazard and risk assessment documents relevant to the area of work, Project plans and specifications, EMP, TMP, Engineering survey, Testing schedule requirements, relevant SDS for any chemicals used as part of the work task being assessed.



	When completing the task, did the Participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	1 Human resource requirements

	[bookmark: _Ref97618055]A clear and accurate overall number of workers required to undertake the construction task.
	

	[bookmark: _Ref97617715]Identify appropriate types of workers required for the task (e.g. skilled or unskilled labour, concreters, carpenters, road crews).
	

	2 Plant and machinery requirements

	[bookmark: _Ref97617718]Identify appropriate types of plant and machinery required to complete the task, and justification their selection.
	

	[bookmark: _Ref97617721][bookmark: _Ref387224637]Identify the plant and machinery requiring a trained or licensed operator and any legislative document or note providing this information.
	

	[bookmark: _Ref97617724]Identify how plant and equipment will be procured for the job and what procedures will be followed to undertake this (e.g. hire company, plant hired after requisition form submitted to the site engineer and accounts officer).
	

	3 Construction material requirements

	[bookmark: _Ref97617316]Interpret site plans and specifications to identify the types of construction materials to be used.
	

	[bookmark: _Ref97618081]Apply accurate calculations of material quantities to be used during the task showing areas, volume or tonnage and wastage factors from plan requirements and engineer requirements.
	

	[bookmark: _Ref97618083]Identify the total value of materials to be used.
	

	[bookmark: _Ref97618097]Document contingency planning in place regarding ordering materials from alternate suppliers.
	

	4 Sub-contractor support requirements

	[bookmark: _Ref97618106]Describe the requirement for all sub-contractor to undergo induction training prior to entering site.
	

	[bookmark: _Ref97618108]Identify key personnel that sub-contractors will refer to.
	

	[bookmark: _Ref97617744]Provide documentation from site including schedules or charts identifying:
· the use of sub-contractors over a given period of time
· plans of drawing of work to be completed by sub-contractors
· sub-contractor induction records
· organisational chart indicating who sub-contractors will report to.
	

	5 Waste disposal requirements

	[bookmark: _Ref97617747]Identify relevant state authority acts, regulations, codes of practice and standards relating to waste removal (e.g. Environmental Protection Act).
	

	[bookmark: _Ref97618154]Identify and explain how materials will be removed from site (e.g. Will they be taken to landfill, decontaminated).
	

	[bookmark: _Ref97617758]Describe any specific organisational requirements for waste disposal.(as applicable).
	

	6 Coordination requirements

	[bookmark: _Ref97618165]Identify and describe tasks that occur simultaneously on the job plan.
	

	[bookmark: _Ref97618167]Accurately identify the time required to undertake the main construction steps.
	

	[bookmark: _Ref97618169]Identify the persons required to monitor to different aspects of the project.
	

	7 Activity scheduling 

	[bookmark: _Ref97617323]Clearly identify the overall length of time assigned to the project and significant milestones from production schedules, construction sequence drawings, Gannt charts or similar.
	

	[bookmark: _Ref97618182]Sequence steps effectively with an efficient use of time.
	

	8. Materials delivery scheduling

	[bookmark: _Ref89848966]Clearly identify the key delivery dates for materials to be used.
	

	[bookmark: _Ref89848970]Identify the locations for site deliveries.
	

	[bookmark: _Ref89848978]Clearly explain the types of trucks, plant and machinery used during the materials delivery process.
	

	9. Risk assessment and management requirements

	[bookmark: _Ref97617976]Describe methods for prioritising risks onsite (e.g. using risks calculators, incident reports).
	

	[bookmark: _Ref97617981]Describe the processes involved with respect to deciding upon control measures.
	

	10. Work health and safety requirements

	1.10A  [bookmark: _Ref97617868]Identify appropriate safety personnel for the site and their roles in the safety system.
	

	[bookmark: _Ref97617988]Provide examples of how hazards may be identified on site through inspections, conducting on going risk assessments, checking reports.
	

	[bookmark: _Ref97617990]Explain the reporting requirements for hazards and incidents on site.
	

	[bookmark: _Ref97618224]Identify the requirements for all workers on site to undergo site specific inductions.
	

	[bookmark: _Ref97618226]Explain procedures for identifying non-hazardous and hazardous materials.
	

	[bookmark: _Ref97618227]Explain procedures for handling substances/ materials onsite (e.g. SDS).
	

	[bookmark: _Ref97618229]Explain the site evacuation procedure including meeting points using the site evacuation plans.
	

	[bookmark: _Ref97618235]Identify and explain the location of firefighting and first aid equipment.
	

	[bookmark: _Ref97618237]Identify and explain the roles of emergency personnel on site (e.g. Fire warden, Chief fire warden).
	

	11. Quality management requirements, including testing scheduling requirements

	[bookmark: _Ref97617888]Identify the tolerances applicable to the civil construction task from plans and specifications.
	

	[bookmark: _Ref97617890]Determine from specifications and schedule testing milestones, the types of testing required.
	

	[bookmark: _Ref97618250]Identify the personnel required to monitor and confirm testing.
	

	12. Traffic management requirements

	1.12A.  [bookmark: _Ref89848189]Identify exclusion zones, signage and barriers required for the project from the traffic management plan.
	

	1.12B.  [bookmark: _Ref89849058]Document the personnel required to implement and monitor the traffic management plan.
	

	13. Environmental requirements

	1.13A.  [bookmark: _Ref97617899]Identify and document how noise, erosion, water quality, waste disposal, flora and fauna and cultural heritage artefacts/ sites were intended to be controlled on site
	

	14. Task monitoring requirements

	1.14A.  [bookmark: _Ref89849075]Identify the persons required to monitor to different aspects of the project.
	

	1.14B.  [bookmark: _Ref89848199][bookmark: _Ref97618297]Provide production charts, toolbox meeting schedule, briefing note, emails, charts diagrams or work instruction requirements for addressing issues with safety/performance.
	

	15. Task performance monitoring requirements

	1.15A  [bookmark: _Ref97618303]Provide example documents including production charts, briefing note, emails, charts diagrams or work instruction indicating milestones or timeframes for the construction, organisation charts/diagrams or notes.
	

	16. Communication requirements

	1.16A  [bookmark: _Ref97618325]Identify how regularly toolbox meetings occur on site.
	

	1.16B  [bookmark: _Ref97618311]Explain the procedures for recording attendance and topics during toolbox meeting (agenda, sign on sheets).
	

	1.16C  [bookmark: _Ref97618313]Identify communication technology which may be used onsite.
	

	17. Reporting requirements

	1.17A  [bookmark: _Ref97617927]Document milestones and reporting requirements including reporting to who.
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	Practical Task 2 (2X)

	Description of task:
The participant must demonstrate undertaking the role of a civil construction supervisor, supervising contractors on two (2) occasions. Occasion 1 of this task will relate to the plan prepared in Practical Task 1. 

During this task, the participant the participant must display the skills and knowledge to effectively, safely and efficiently:
· prepare to supervise contractors of civil works
· confirm task initiation 
· confirm contractor has communicated instructions to team members and others involved during pre-start meeting
· set out tasks as required for the effective completion of the civil works
· while overseeing the execution of tasks:
· monitor task performance for safety effectiveness and efficiency
· implement adjustments to civil works practice and job plan as required
· oversee plant equipment and tools maintenance and confirm maintenance requirements are carried out and recorded according to manufacturer and site requirements
· report on the execution of tasks
· complete and submit written and verbal reports according to site requirements
· recommend improvements to civil works practice.

Tasks are at the Assessor’s Discretion, but detail of tasks undertaken must be recorded in the Assessor’s Comments (on the back of the Practical Assessment cover page).

	Resources required: 
Work team, work site, organisational policies, standard operating procedures and plans, safety processes, hazard and risk assessment documents relevant to the area of work, Project plans and specifications, EMP, TMP, Engineering survey, Testing schedule requirements, relevant SDS for any chemicals used as part of the work task being assessed, all materials, tools, plant or equipment required to complete the task, required PPE and relevant safety equipment.



	When completing the task, did the Participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	
	1st
Occasion
	2nd
Occasion

	1 Plan and prepare to supervise contractors of civil works

	2.1.A.  [bookmark: _Ref97620380]Identify the location of the site using appropriate project plans.
	
	

	2.1.B.  [bookmark: _Ref97556461]Determine the scope of the work task from plans, drawings and specifications.
	
	

	2.1.C.  [bookmark: _Ref97556995]Complete a job plan demonstrating ability to access, read and apply workplace documentation to confirm legislative, statutory and workplace compliance.
	
	

	2.1.D.  [bookmark: _Ref97620411]Confirm contractor has a job plan available that meets task and compliance requirements
	
	

	2.1.E.  [bookmark: _Ref97557249]Determine and address potential risks, hazards and environmental issues and implement control measures.
	
	

	2.1.F.  [bookmark: _Ref97557620]Select and wear PPE suited to site and tasks.
	
	

	2.1.G.  [bookmark: _Ref97557818]Consult contractors and team members regarding resource requirements for task.
	
	

	2.1.H.  [bookmark: _Ref97620467]Communicate with other supervisors/ team leaders to resolve potential coordination requirements.
	
	

	2.1.I.  [bookmark: _Ref97620487]Identify specific council, state or federal requirements for the site including those relating to finishes, quality, reporting and safety.
	
	

	2.1.J.  [bookmark: _Ref97557871]Confirm required resources including human resources are acquired and made available for task.
	
	

	2.1.K.  [bookmark: _Ref89848589]Explain any specific organisational, client and site requirements from site plans, specifications, geological, geotechnical data.
	
	

	2.1.L.  [bookmark: _Ref97620523]Clearly explain the meteorological data available for the site (rainfall, humidity, temperature and wind), and identify any issues in production (e.g. If a possibility of rain was evident), quality or safe work practices arising from the forecast.
	
	

	2.1.M.  [bookmark: _Ref89848672]Interpret site plans or environmental plans to clearly indicate the location of site wash down facilities.
	
	

	2 Confirm task initiation

	2.2A.  [bookmark: _Ref97620561]Facilitate a pre-start meeting with contractor and team.
	
	

	2.2B.  [bookmark: _Ref97620563]Monitor contractor participation in pre-start meeting to confirm contractor has communicated instructions to team members and others involved to workplace requirements.
	
	

	2.2C.  [bookmark: _Ref89850327]Discuss any possible construction problems (or lack of), regarding the type of rock found onsite.
	
	

	2.2D.  [bookmark: _Ref89850329]Discuss any possible construction problems (or lack of), regarding the type of soil types found onsite.
	
	

	2.2E.  [bookmark: _Ref97621764]Discuss weather conditions and recommend actions.
	
	

	2.2F.  [bookmark: _Ref97621767]Discuss site hydrological data and associated drainage requirements.
	
	

	2.2G.  [bookmark: _Ref89848669]Explain the log book, or scheduled servicing procedure for plant and machinery used on the site.
	
	

	2.2H.  [bookmark: _Ref89848670]Concisely explain how faulty or defective equipment will be reported and recorded onsite using example hazard identification forms.
	
	

	2.2I.  [bookmark: _Ref89848675]Explain any environmental hazards posed from the use of plant and machinery including control measures to be used to control these environmental hazards.
	
	

	2.2J.  [bookmark: _Ref89848678]Listen to and respond effectively to questions and queries.
	
	

	2.2K.  [bookmark: _Ref89848224]Ensure all workers understand the SWMS for the task and have signed their understanding.
	
	

	2.2L.  [bookmark: _Ref97616153]Walk the work area with contractors and the team, identifying new potential risks, hazards and environmental issues and suitable controls.
	
	

	2.2M.  [bookmark: _Ref89848361]Ensure signs and barriers have been installed to protect work area as required.
	
	

	2.2N.  [bookmark: _Ref89848692]Set out task correctly from engineers’ survey pegs using plans, drawings and specifications.
	
	

	3 Oversee execution of tasks

	2.3A.  [bookmark: _Ref97616380]Watch workers undertake tasks, checking that tolerances are met as required.
	
	

	2.3B.  [bookmark: _Ref97621301]Monitor workers for safety concerns, making sure manual handling procedures are followed and work activities are conducted safely.
	
	

	2.3C.  [bookmark: _Ref97621312]Watch plant and equipment used to confirm machinery is used safely and within machine capabilities and limitations.
	
	

	2.3D.  [bookmark: _Ref97616465]Clearly communicate with workers regarding task execution using approved and understood communication methods.
	
	

	2.3E.  [bookmark: _Ref97621332]Write notes in diary if safety or compliance issues arise.
	
	

	2.3F.  [bookmark: _Ref97621334]Write notes of measurements made, material quality, deliveries and docket checks.
	
	

	2.3G.  [bookmark: _Ref97616686]Organise and make adjustments to civil works practice and job plan as required and confirm required outcomes are achieved.
	
	

	2.3H.  [bookmark: _Ref97621359]Confirm personnel allocated has checked that log books have been filled out and scheduled servicing has been undertaken on plant and equipment.
	
	

	2.3I.  [bookmark: _Ref97621361]Confirm that faulty or defective equipment is reported and recorded according to site requirements.
	
	

	4 Report on execution of tasks

	2.4A.  [bookmark: _Ref97621374]Make verbal reports to relevant personnel regarding completion of stages, reaching milestones, testing required.
	
	

	2.4B.  [bookmark: _Ref97621378]Complete all diary entries clearly and legibly.
	
	

	2.4C.  [bookmark: _Ref97621381]Ensure all test results and checks are documented and stored according to site requirements.
	
	

	2.4D.  [bookmark: _Ref97616891]Make verbal or written recommendations regarding changes to task execution.
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