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CPCCBC4001A 
Apply building codes and standards to the construction process for low rise building projects
ASSESSMENT SUMMARY

The assessment activities for CPCCBC4001A Apply building codes and standards to the construction process for low rise building projects cover all aspects of the unit of competency required. To demonstrate competence in this unit, a participant must undertake all tasks and complete them satisfactorily and consistently. For Apprentices and Trainees, this includes employer completion of the Employer Record Book (ERB). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be equitable, fair and flexible. If a participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a participant does not answer some questions or perform some tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. The Trainer/Assessor is able to provide the participant with additional information on interpreting the assessment outcomes and provide guidance on the participant’s options. Should a participant still be deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result. 

By signing the cover page for each assessment item, the participant acknowledges they understand the assessment instructions and requirements and consent to being assessed. The participant also verifies and assures the RTO that the work submitted is their own work. 


	[bookmark: _Ref396827952]Participant Name
	Jessica Manley




	Task
	Assessment Results 

	Theory Exam
	 Satisfactory 
	 Not Yet Satisfactory

	Practical Assessment
	 Satisfactory 
	 Not Yet Satisfactory

	Outcome for Unit of Competency
	 Competent
	 Not Yet Competent




	Assessor Name
	

	Assessor Signature
	
	Unit Competence Determination Date
	Click here to enter a date.
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	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances, whereby the Participant’s answers will be documented by a party other than the Participant. This must be acknowledged in writing (e.g. FT001 and Assessor Comments)
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· Assessors are to complete marking in pen of a different colour to the Participant.
· If a Participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a Participant changes their response in writing, they must put their initials next to the written change.
· If a Participant changes their response verbally, this must be noted on the exam paper by the assessor.




	Participant name
	Jessica Manley

	
	

	Participant signature
	
	
	

	Date
	8/03/2021



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.




	Number of questions
	Number of questions answered correctly
	Task outcome (Tick)

	38
	
	Satisfactory
	Not Yet Satisfactory

	
	
	
	


	ASSESSOR COMMENTS

	


[bookmark: _Ref5882211]A Performance Solution must abide by which of the following? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Be assessed according to one or more of the Assessment Methods
	

	
		Go beyond the requirements of Deemed-to-Satisfy Provisions
	

	
		Comply with the Performance Requirements
	




[bookmark: _Ref5882213]True or False (Tick your response): The Performance Requirements of the National Construction Code can be achieved by using a Performance Solution, a Deemed-to-Satisfy Solution, or a combination of both.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref5882215]True or False (Tick your response): The term ‘Performance Solution’ in the NCC was formerly known as ‘Alternative Solution’.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref5882219]Where a Performance Solution has been proposed, which of the following documentation should be prepared and retained? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Details of the relevant Performance Requirements 
	

	
		Assessment Methods used to establish compliance with the relevant Performance requirements
	

	
		Details of any Expert Judgement relied upon
	

	
		Details of any tests of calculations used to determine compliance with the Performance Requirements
	

	
		Details of any Standards or other information which were relied upon
	





[bookmark: _Ref5950292]True or False (Tick your response): Where a Deemed-to-Satisfy solution has been proposed, all relevant plans/specifications should be retained.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref427235149]Identify the Volume and Parts of the NCC that outline the Assessment Methods used to determine whether a Performance Solution or a Deemed-to-Satisfy Solution complies with the Performance Requirements for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Volume 2 – part A2.2
	Volume 1- Part A2.2
	




[bookmark: _Ref536106146]Identify the Australian Standard that relates to artificial lighting needed for safe movement, as noted in the NCC.

	Answer
	AS/NZS1680.0
	



[bookmark: _Ref5782698]Identify the Volume and Parts of the NCC that outline the requirements for artificial lighting needed for safe movement for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Volume 2 – part 3.8.4.3
	Volume 1 – part F4.4 
	





[bookmark: _Ref5882620]Fill in the blanks for the statement below, referring to Volume 1 of the NCC with regards to lighting:

Where a Deemed-to-Satisfy Solution is proposed, Performance Requirements ____________ to ____________ are satisfied by complying with F4.12
F4.1
FP4.5
FP4.1

(i) ____________ to ____________; and part G6

(ii) For a building containing an occupiable outdoor area, ____________; and 
(iii) for farm buildings and farm sheds, ____________. 
Part H3

Where a Performance Solution is proposed, the relevant Performance Requirements must be determined in accordance with ____________ and ____________ as applicable. A2.4(3)
A2.2(3)


	Answer
	

	



[bookmark: _Ref422743346][bookmark: _Ref531682593]Fill in the blanks for the statement below, referring to Volume 2 of the NCC with regards to light:

Where an alternative light system is proposed as a Performance Requirement to that described in ____________, that proposal must comply with – P2.4.4
Part 3.8.4

(a) Performance Requirement ____________; and 
(b) the relevant Performance Requirements determined in accordance with ____________ and ____________ as applicable.A2.4(3)
A2.2(3)


	Answer
	

	



[bookmark: _Ref5882637]Identify the Australian Standard that relates to each of the listed types of fire fighting equipment, as noted in the NCC.

	Answer
	Equipment
	Australian Standard
	
	
	Fire hydrants
	AS 2419 
	

	
	Fire hose reels
	AS 2441
	

	
	Portable fire extinguishers
	AS 2444
	

	
	Smoke alarms
	AS 3786
	



[bookmark: _Ref5882646]For each of the listed types of fire fighting equipment, identify whether they are required by the NCC (if so, identify the relevant Part).

	Answer
	Equipment
	Volume 1
	Volume 2
	
	
	Fire hydrants
	EP1.3
	N/A
	

	
	Fire hose reels
	EP1.1
	N/A
	

	
	Portable fire extinguishers
	E1.6
	N/A
	

	
	Smoke alarms
	Spec E2.2a

	Part 3.7.5.2


	




[bookmark: _Ref531682022]Identify the applicable Act in your jurisdiction that outlines the requirements for smoke alarm installation in domestic dwellings. 
Briefly identify the requirements.

	Answer
	Act name and section(s)
	Requirements
	
	
	Fire and Emergency Services Act 1990 – 104RBA(5): Owner must install smoke alarm
	Each smoke alarm must be powered in a way prescribed by regulation, have been manufactured less than 10 years before is it installed, operate when tested and be interconnected to every other smoke alarm installed in the domestic dwelling.
	





[bookmark: _Ref5883662]Identify the applicable Act in your jurisdiction that outlines the requirements for testing smoke alarms in domestic dwellings. 
Briefly identify the requirements.

	Answer
	Act name and section(s)
	Requirements
	
	
	Fire and Emergency Services Act 1990 – 104RD: Testing smoke alarms 
	Within 30 days before the start of tenancy in a domestic dwelling, the lessor must test each smoke alarm in the dwelling in compliance with section 104RRA(3). Also during tenancy, the tenant must test each smoke alarm in the dwelling every 12 months,.
	




[bookmark: _Ref5952975]Identify the applicable Act in your jurisdiction that outlines what must occur if smoke alarm in a domestic dwelling does not operate upon testing and when any rectification must occur. Briefly identify the requirements.

	Answer
	Act name and section(s)
	Requirements
	
	
	Fire and Emergency Services Act 1990 – 104RC: Owner must replace smoke alarm
	If the smoke alarm in a domestic dwelling does not operate when tested, the owner of the dwelling must immediately replace the smoke alarm. 
	




[bookmark: _Ref5883528]In observation of NCC Volume 2, identify three (3) aspects which should be checked with regards to smoke alarms.

	Answer
	Three aspects which should be checked when having smoke alarms, is ensuring they comply with the AS 3786, they must be interconnected if there is more than one in the building, and be powered from the consumer mains source.
	




[bookmark: _Ref5883676]Must all smoke alarms be interconnected in domestic dwellings? Explain your response with reference to legislation.

	Answer
	Vol two, Part 3.7.5.6 (Fire Safety) - If there is more than one smoke alarm, they MUST be interconnected. Although this only applies within a single dwelling. This provides a common alarm, which will increase the likelihood of sleeping occupants becoming aware of the smoke/fire. 
	



[bookmark: _Ref5883539]Fill in the blanks for the definition of fire compartments, referring to Volume 1 of the NCC:

Fire compartment means – 
(a) The total space of a building; or
(b) When referred to in –
(i) The Performance Requirements – any part of a building separated from the remainder by ____________ to fire such as _____________ and/or ____________ having an appropriate resistance to the spread of fire with any ____________ adequately protected; orfloors
walls
barriers
openings

(ii) The Deemed-to-Satisfy Provisions – any part of a building separated from the remainder by ____________ and/or ____________ each having an ____________ not less than that required for a fire ____________ for that type of construction and where all ____________ in the ____________ construction are protected in accordance with the DtS Provisions of the relevant Part. wall
openings
FRL
floors
walls
separating


	Answer
	
	



[bookmark: _Ref5787153]Identify the Volume and Parts of the NCC that outline the requirements for fire compartmentation and separation for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Volume two – Part 3.7.2 and Part 3.7.4
	Volume one – Part C2
	



[bookmark: _Ref5885739]Fill in the blanks for the statement below, referring to Volume 1 of the NCC with regards to fire compartmentation and separation:

Where a Deemed-to-Satisfy Solution is proposed, Performance Requirements ____________ to ____________ are satisfied by complying with C2.14
C2.1
C1.14
C1.1
CP9
CP1

(i) ____________ to ____________, ____________ to ____________ and ____________ to ____________; and C3.1
Part G3
C3.17

(ii) in a building containing an atrium, ____________; and Part H1

(iii) for additional requirements for Class 9b buildings, ____________; and Part H3

(iv) for farm sheds, ____________. 
Where a Performance Solution is proposed, the relevant Performance Requirements must be determined in accordance with ____________ and ____________ as applicable. A2.4(3)
A2.2(3)


	Answer
	

	



[bookmark: _Ref5885741]Fill in the blanks for the statement below, referring to Volume 2 of the NCC with regards to fire separation:

Where an alternative fire separation design is proposed as a Performance Solution to that described in Part ____________ that proposal must comply with Performance Requirement ____________; and the relevant Performance Requirements determined in accordance with ____________ and ____________ as applicable. A2.4(3)
A2.2(3)
P2.3.1
3.7.2


	Answer
	

	



[bookmark: _Ref5885751]Identify the Australian Standard referenced in NCC Volume 1 with regards to compartmentation and separation for electricity supply systems.

	Answer
	AS/NZS 3013:2005
	




[bookmark: _Ref5886137]Identify the Volume and Parts of the NCC that outline the level of fire resistance required for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Volume 2 – Part 3.7
	Volume 1 – Part C1 – Spec C1.1
	




[bookmark: _Ref5951761]In a building’s specifications, an FRL is stated as being 90 / 60 / -. 
If exposed to a standard fire test, how many minutes can you expect this building element to last for the criteria listed below? 

	Answer
	Minutes
	Criteria
	
	
	No requirement
	Insulation
	

	
	60
	Integrity
	

	
	90
	Structural adequacy
	




[bookmark: _Ref5886138]Fill in the blanks: 
According to NCC Volume 1, an electricity substation located within a building must be separated from any other part of the building by construction having an FRL of no less than ____ / ____ / ____ and have any doorway in that construction protected with a self-closing fire door having an FRL of not less than ____ / ____ / ____. 120
120
120
-
30
120


	Answer
	

	



[bookmark: _Ref5886140]Fill in the blanks: According to NCC Volume 2, if an electrical wire or cable penetrates a separating wall, the service and building element at the penetration must be identical with a prototype assembly which has been tested and achieve an FRL of not less than ____ / ____ / ____. -
60
60


	Answer
	

	




[bookmark: _Ref5886711]Identify the applicable Act in your jurisdiction that outlines the occupier’s requirements for maintaining prescribed fire safety installations (e.g. fire doors). Briefly identify the requirements.

	Answer
	Act name and section(s)
	Requirements
	
	
	Fire and Emergency Services Act 1990 – 104D: Occupier of building to maintain prescribed fire safety installations
	The occupier of a building must maintain at all times every prescribed fire safety installation to a standard of safety and reliability in the event of a fire,
	




[bookmark: _Ref5958063]Identify the applicable Regulation in your jurisdiction that outlines the timeframes in which repair or corrective action must be taken when maintaining prescribed fire safety installations. Briefly identify the requirements. 

	Answer
	Regulation name and section(s)
	Requirements
	
	
	Building Fire Safety Regulation 2008 – Division 2: Obligations of persons maintaining prescribed fire safety installations
	The person must give the occupier of the building a notice about the defect in the approved form within 24 hours after the person carries out the maintenance of the installation.
	




[bookmark: _Ref5886716]NCC Volume 1 outlines that fire doors must be fitted with smoke seals and the assembly must be tested in accordance with Australian Standards. To which classes of building does this specification apply?

	Answer
	Class 5 or 6 building
	



[bookmark: _Ref5886719]Do all fire doors require tags? Explain your response with reference to legislation.

	Answer
	 Yes all fire doors need to be tagged in accordance with AS/NZS 1905.1-2005.
	


[bookmark: _Ref5886882]Match the building classifications and their descriptions by writing the appropriate letter next to each number in the centre column.

	Answer
	Classification
	Answers
	Description
	
	
	1
	Class 1
	1 - E
	A
	A non-habitable building or structure.
	

	
	2
	Class 2
	2 - H
	B
	A laboratory or a building in which a handicraft or process for the production, assembling, altering, repairing, packing, finishing or cleaning of goods or produce is carried on for trade, sale or gain.
	

	
	3
	Class 3
	3 - C
	C
	A residential building other than Class 1 or 2 which is a common place of long term transient living for a number of unrelated persons. 
	

	
	4
	Class 4
	4 - D
	D
	A dwelling in a building that is Class 5, 6, 7, 8 or 9 if it is the only dwelling in the building. 
	

	
	5
	Class 5
	5 - F
	E
	May be a single dwelling or a boarding house, guest hose or hostel with a floor area less than 300m2.
	

	
	6
	Class 6
	6 - G
	F
	An office building used for professional or commercial purposes, excluding buildings of Class 6, 7, 8 or 9.
	

	
	7
	Class 7
	7 - I
	G
	A shop or other building for the sale of goods by retail or the supply of services direct to the public.
	

	
	8
	Class 8
	8 - B
	H
	A building containing 2 or more sole-occupancy units, each being a separate dwelling. 
	

	
	9
	Class 9
	9 - J
	I
	A building which is a carpark or fore storage/display of goods or produce for sale by wholesale. 
	

	
	10
	Class 10
	10 - A
	J
	A building of a public nature.
	




[bookmark: _Ref5886883]What class of building would shops, restaurants and cafes belong to?

	Answer
	Class 6
	



[bookmark: _Ref5886885]What class of building would a general medical practitioner’s office belong to?

	Answer
	Class 5
	




[bookmark: _Ref423946303]True or False (Tick your response): At the design stage, it may not be clear who the final tenant will be (or how they will be using their tenancy), so as long as the design meets the minimum requirements of all the classifications, it could be used for any of the purposes.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref531681692]Where parts of a building have different purposes, the classification of Class 1 may apply to the whole building if not more than what percentage of the floor area is used for a purpose which is a different classification? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		5%
	

	
		10%
	

	
		25%
	

	
		50%
	




[bookmark: _Ref5965263]The NCC aims to ensure structures appropriately withstand normal forces. Match the terms and definitions below by writing the appropriate letter next to each number in the centre column.

	Answer
	Term
	Answers
	Definitions
	
	
	1
	Bending
	1 - B
	A
	A force which shortens or crushes.
	

	
	2
	Compression
	2 - A
	B
	A fore which stretches and squashes at the same time.
	

	
	3
	Shear
	3 - F
	C
	A force which tries to pull something apart.
	

	
	4
	Strain
	4 - E
	D
	Intensity of the internally distributed forces that resist a change in the form of a body.
	

	
	5
	Stress
	5 - D
	E
	Physical change in the dimensions of a structure that results from applying a load.
	

	
	6
	Tension
	6 - C
	F
	Created where two opposite forces try to cut, tear or rip something in two.
	





[bookmark: _Ref5965264]True or False (Tick your response): When a beam is loaded, the top is compressed and the bottom is in tension.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref5965265]True or False (Tick your response): When a cantilever is loaded, the top surface is in tension and the bottom is in compression.

	Answer
		True 
	
	
	
		False 
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	PRACTICAL ASSESSMENT INSTRUCTIONS

· The following practical assessment will require the Participant to complete work related activities.
· The Assessor will conduct observations of the Participant’s work to determine whether they display sufficient practical skills and knowledge. 
· Please fill in the details below – providing your name, signature and date of assessment.
· The Participant’s signature acknowledges that the Assessor provided clear instructions and the Participant understood what was required to complete this assessment.
· The Assessor may substitute a Practical Task with an alternate task of equal value.
· Alternate tasks must be fully documented by the assessor in the Assessor Comments area.





	Participant name
	Jessica Manley

	
	

	Participant signature
	
	
	

	Date
	8/03/2021



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.





	Task
	Task outcome (Tick)

	
	Satisfactory
	Not Yet Satisfactory

	Task 1 (Occasion 1)
		
	Task 1 (Occasion 2)
		

[bookmark: _GoBack]

	ASSESSOR COMMENTS

	


CPCCBC4001A
Apply building codes and standards to the construction process for low rise building projects

	Practical Task 1 (2X)

	Description of task:
On two (2) occasions, a suitable observer is to verify the participant’s ability to access, interpret and apply relevant building codes and standards. 
· Occasion 1: Construction classified as Class 1 and 10 construction
· Occasion 2: Construction classified in Classes 2 to 9 with a gross floor area not exceeding 2000 square metres, not including Type A or Type B construction

The participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. 

Evidence to be submitted may include: 
· Documented evidence of determining a compliant solution on a project including: 
· Correspondence such as letters, emails, and records of other communications
· Certifier reports, instructions
· Other compliance documentation for a project including: 
· Council or private certifier inspection reports 
· Structural inspection certificates 
· Occupation certificates

The observer is to provide detailed comments on the tasks completed by the participant. The assessor is to verify the observer’s comments in the Assessor Comments section, and provide the Practical Assessment outcome on the front cover of this document.

	Resources required: 
Drawings and specifications, National Construction Code, Australian Standards, Relevant legislation.

	Assessment of task

	Name of participant:
	Jessica Manley

	Name of observer:
	Khyle Glover

	Role of observer 
(Confirm suitability to sign)
	Estimating Manager – superior group

	Email address of observer
	Khyle@superiorgroup.com.au

	Signature of observer:
	
	Date:
	8/03/2021
	When completing the task, did the participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	
	1st
Occasion
	2nd
Occasion

	1 Access and interpret codes and standards

	1.A.  [bookmark: _Ref531596182][bookmark: _Ref5621987]Identify relevant performance requirements from the National Construction Code that apply to individual projects described as low rise.
		
	1.B.  [bookmark: _Ref531596194]Determine requirements of relevant National Construction Code deemed-to-satisfy (DTS) provisions.
		
	1.C.  [bookmark: _Ref5621994]Access and interpret requirements of relevant Australian standards referenced in the National Construction Code. 
		
	2 Classify buildings

	1.2A.  [bookmark: _Ref531596197][bookmark: _Ref5621997]Determine the nature of building according to its use and arrangement.
		
	1.2B.  [bookmark: _Ref5622001]Apply National Construction Code criteria to determine the defined classification. 
		
	1.2C.  [bookmark: _Ref5622021]Identify and interpret National Construction Code requirements for multiple classification.
		
	3 Solutions for compliance

	1.3A.  [bookmark: _Ref5622025]Determine range of criteria to ensure that construction methods comply with National Construction Code performance requirements. 
		
	1.3B.  [bookmark: _Ref531596223][bookmark: _Ref5622028]In accordance with company policy and procedures, discuss and propose alternative solutions to a design or construction problem that complied with National Construction Code requirements, considering basic design principles and the behaviour of materials and structures under stress, strain, compression, bending or combined actions.
		
	1.3C.  [bookmark: _Ref5622031]Identify and document performance-based solutions in accordance with National Construction Code requirements.
		
	1.3D.  [bookmark: _Ref5622034]Analyse and apply assessment methods referenced in the National Construction Code to determine whether a building solution complied with performance requirements or DTS provision. 
		
	1.3E.  [bookmark: _Ref5622037]Identify and complete relevant documentation in accordance with National Construction Code requirements. 
		
	1.3F.  [bookmark: _Ref535842459]Effectively communicate using the following methods:
· Language/concepts appropriate to cultural differences
· Non-verbal communication
		
	4 Fire protection requirements 

	1.4A.  [bookmark: _Ref531596228]Identify and apply passive and active fire control elements for low rise buildings, as required by the National Construction Code and other legislation (including WHS requirements). 
		
	1.4B.  [bookmark: _Ref5622050]Determine level of fire resistance required for the construction of various low rise buildings.
		
	1.4C.  [bookmark: _Ref5622053]Check existing buildings for compliance with passive and active fire protection requirements, in accordance with National Construction Code requirements.
		
	The Participant’s performance was:  Satisfactory     Not Satisfactory



	OBSERVER COMMENTS

	 - Jess did very well in determining the relevant codes.
- Jess impressed me with her ability to interpret the document/plans provided.
- Overall, Jess did an outstanding job.
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