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1Cost Estimation Sheet

	Participant name
	Abbie Heaslip

	Date
	25/09/2024



Details of Building and Construction Project
	Name of project
	Southern Queensland Correctional Precinct – Stage 2

	Type of project
	 Residential building
 Commercial building

	State/Territory
	Qld

	Plans accessed for material estimates
	GBA-DWG-AR-AD-120 GROUND FLOOR - SETOUT PLAN
GBA-DWG-AR-DU-140 ROOF PLAN




Identify internal linings, external cladding and roof materials from plans and specification
	Item
	Description 

	Internal linings
	Blockwork/ precast concrete

	External cladding
	Blockwork/ precast concrete. Fibre cement linings are located on the wet area /
Plumbing side of the wall

	Roofing materials
	MR01-CB01 Econoclad metal roof sheeting




Opinion of costs - for one (1) room identify costs of three (3) materials needed.
	Item
	Description (including size, thickness)
	Cost per Unit
	Quantity
	Total cost
	Construction method

	1
	PNT01 (2.4m2 x 4.2m2) 
	$30/m2
	6.6m2
	$198
	Painting

	2
	FV10 (2.4m x 4.2m)
	$58.62/m2
	6.6m2
	$386.9
	Vinyl flooring, to achieve slip resistant. Fixed in accordance with the manufacturer's recommendation

	3
	Paint to Doors:
PNT22 
to Room Entry Door
(Type PD10)
	$30/m2
	2m2
	$60
	Painting




Identify two (2) Prime Cost (PC) items and two Provisional Sum items
	Prime Cost items
	Provisional Sum items

	Bathroom Fixtures
	Earthworks

	Cabinetry
	Services Connections
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