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	Items
	Size
	Thickness (mm)
	Quantity (pcs)

	
	Height (mm)
	Width (mm)
	
	

	Category 1: Doors 

	Entry 
	2400
	1500
	40
	1

	Garage
	2400
	720
	40
	2

	Garage 
	2400
	5210
	40
	1

	Media room 
	2400
	820
	35
	1

	Bathroom
	2400
	820
	35
	1

	Living room
	2500
	6000
	35
	1

	Pantry
	2400
	820
	35
	1

	Laundry
	2400
	720
	35
	1

	Study
	2400
	820
	35
	1

	Study
	2400
	1000
	35
	1

	Bedroom 4
	2400
	820
	35
	1

	Bedroom 4
	2400
	720
	35
	1

	Bathroom
	2400
	720
	35
	1

	Bedroom 3
	2400
	3000
	35
	1

	Bedroom 3
	2400
	1200
	35
	1

	Bedroom 2
	2400
	820
	35
	1

	Bedroom 2
	2400
	2450
	35
	1

	Master bedroom
	2400
	820
	35
	1

	Wardrobe
	2400
	820
	35
	1

	Ensuite
	2400
	820
	35
	1

	Category 2: Windows
	
	
	
	

	Entry
	600
	3000
	3
	2

	Dining
	2700
	900
	3
	1

	Laundry
	1200
	600
	3
	1

	Study
	1200
	600
	3
	2

	Stair area
	1200
	900
	3
	1

	Stair area
	1200
	700
	3
	1

	Stair area
	2400
	900
	3
	5

	Master bedroom
	600
	900
	3
	1

	Master bedroom
	600
	1500
	3
	1

	Master bedroom
	2400
	900
	3
	1

	Master bedroom
	2400
	1500
	3
	1

	Ward robe
	300
	3000
	3
	1

	Ensuite
	2400
	600
	3
	1

	Bedroom 2
	600
	900
	3
	2

	Bedroom 2
	600
	1500
	3
	1

	Bedroom 3
	600
	1500
	3
	1

	Bath
	600
	1200
	3
	1

	Bedroom 4
	1200
	600
	3
	2

	Bedroom 4
	1200
	1800
	3
	1

	Roof skylight
	700
	1140
	3
	1



The above materials are sourced from QLD supplier (name kept in confidentiality please)
Safety: The doors and windows meet safety standards and have features such as sturdy locks, tempered glass, and proper installation techniques to enhance security.
Fire resistance rating: The external doors and windows with fire-resistant properties or ones that meet fire resistance regulations to help prevent the spread of fire.
Suitability: The doors and windows are suitable for the intended purpose and the architectural style of the building. Consider factors such as design, material, and functionality to ensure they match the requirements.
Durability: The doors and windows made from high-quality materials that can withstand environmental factors like humidity, temperature changes, and potential wear and tear over time. This helps ensure their long-term performance.
Serviceability: The Doors and windows are easy to maintain and repair if necessary. The suppliers offers warranty or after-sales services for the products.
Cost-effectiveness: The overall cost of the doors and windows, including their initial purchase price, installation costs, maintenance expenses, and potential energy savings and providing long-term benefits and value.
Short-term degradation: We have assess any potential short-term degradation issues, such as color fading, warping, or structural integrity concerns. The product had good reviews and recommendations to minimize the risk of immediate deterioration.
Long-term degradation: The expected lifespan of the doors and windows, as well as any potential long-term degradation, such as corrosion or deterioration of seals and insulation is minimal. By selecting the high-quality materials and well-known brands can help mitigate these issues.
Availability: These were readily available for the date and time required for our Project

If the above were not available, consideration to obtain these would be undertaken:
Research other suppliers who would have these
Look for custom solutions if possible – but be wary of the expenses involved
Reach out to other contractors or builders with a similar experience
Alternate materials eg) wooden doors instead of aluminium or fiberglass or composite doors
Custom fabrication
Modification of existing if possible eg) additional security features or fire-resistant coatings
Consult with engineers who can advice on suitable alternatives based on building regulations
Evaluate any given alternatives to the above mentioned criteria including safety, fire-resistance rating, durability etc

Relevant docs assessed and reviewed are attached and also includes https://awa.associationonline.com.au/documents/item/2124
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