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Handout 1 - Compliance Review

	Participant name
	Michael Trott

	Date
	17/12/23



	Building and construction project
	RTO Facility

	Project overview
	Office Refurb

	Building classification
	 Class 1 – 10 buildings, max two storeys
 Class 2 – 9 building, Type C only constructions

Specify class: class 5

	Project site address
	878 Beaudesert Road, Coopers plains

	State/territory where project is undertaken
	QLD

	Construction plan documents reviewed
	Sections/Elevations/Floor plans/site plan



Building Regulations
List relevant regulations
	Building regulations
	Plans comply 
	Explanation

	Example: Smoke alarms
	 Yes
	 No
	Smoke alarm locations shown in floor plans - photoelectric (AS 3786-2014) hardwired and interconnected.

	Plumbing and drainage act 2022
	 Yes
	 No
	Shown in plumbing layout (AS/NZS.3500)

	Structural timber sizes
	 Yes
	 No
	Shown in section a (AS1684)

	Wet areas
	 Yes
	 No
	Shown in floor plans (AS3740)

	Mechanical ventilation
	 Yes
	 No
	Shown in floor plans (AS1668.1)

	
	 Yes
	 No
	

	
	 Yes
	 No
	



Building Standards
Provide relevant standards
	Building Standards
	Plans comply 
	Explanation

	AS1684
	 Yes
	 No
	Structural timber sizes

	AS/NZS.3500
	 Yes
	 No
	Plumbing and drainage works installation

	AS3740
	 Yes
	 No
	Wet area compliance

	AS1668.1
	 Yes
	 No
	Mechanical ventilation compliance

	AS3786
	 Yes
	 No
	Smoke alarm installation

	AS1562.1
	 Yes
	 No
	Roof installation



NCC Requirements
Fire Safety
	Requirements
	Plans comply 
	Explanation

	Smoke alarms connected to mains power installed in accordance with AS-3786 and NCC PART 3.7.2
	 Yes
	 No
	Electrical layout shows smoke detectors

	Lighting to assist evacuation 3.7.2.5
	 Yes
	 No
	Electrical layout shows emergency exit light wired to mains power

	
	 Yes
	 No
	

	
	 Yes
	 No
	

	
	 Yes
	 No
	

	
	 Yes
	 No
	



Health and amenity
	Requirements
	Plans comply 
	Explanation

	There should be a clear space of 1.2m between the closest pan within the sanitary compartment and the doorway p3.8.3.3
	 Yes
	 No
	Door way opening has clear 1.2m space away from toilet components

	 Artificial lighting provided in sanitary compartments with no windows NCC3.8.4.3
 , 

	 Yes
	 No
	As shown in Electrical layout

	Provide mechanical ventilation NCC 3.8.5
	 Yes
	 No
	Not shown in electrical layout

	
	 Yes
	 No
	

	
	 Yes
	 No
	

	
	 Yes
	 No
	




Safe movement and access
	Requirements
	Plans comply 
	Explanation

	
	 Yes
	 No
	

	
	 Yes
	 No
	

	
	 Yes
	 No
	

	
	 Yes
	 No
	

	
	 Yes
	 No
	

	
	 Yes
	 No
	



Energy efficiency
	Requirements
	Plans comply 
	Explanation

	External windows and door to be fitted with a seal NCC 3.12.33
	 Yes
	 No
	As shown in floor plans

	
	 Yes
	 No
	

	
	 Yes
	 No
	

	
	 Yes
	 No
	

	
	 Yes
	 No
	

	
	 Yes
	 No
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