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CPCCBC4014 
Prepare simple building sketches and drawings 

ASSESSMENT SUMMARY

The assessment activities for CPCCBC4014 Prepare simple building sketches and drawings cover all aspects of the unit of competency. For Apprentices/Trainees, this includes supervisor completion of the Apprentice/Trainee Record (ATR). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be fair, flexible, valid and reliable. If a Participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a Participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the Participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a Participant does not answer all questions or perform all tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. 

The Trainer/Assessor can provide the Participant with additional information on interpreting the assessment outcomes and guide the Participant’s options. If a Participant is still deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result as per the process in the Student Handbook. 

By signing below, the Participant acknowledges:
· They understand the assessment instructions and requirements, and consent to being assessed. 
· The work submitted is to be their own work – with the work of/with others needing to be clearly acknowledged and documented. 
· They consent to any photo/video recording of their work that occurs during assessment. 

	Participant name
	Abbie Heaslip

	Participant signature
	


	Pre-requisite unit(s) to be achieved and authenticated prior to undertaking assessment

	 Not applicable 



	Task
	Date completed
	Assessment Results 

	Theory Exam
	9/10/2024
	 Satisfactory 
	 Not Satisfactory

	Practical Assessment
	Select Date.
	 Satisfactory 
	 Not Satisfactory

	Outcome for CPCCBC4014
	Select Date.
	 Competent
	 Not Yet Competent



	Evidence requirements checklist (ticked by assessor and evidence supplied to RTO)

	 Theory Exam
 Practical Assessment
 Compliance review
	 Planning sheet
 Sketch/drawing of 1 structural component
 Sketch/drawing of 1 non-structural component



	Assessor name
	

	Assessor signature
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THEORY EXAM


	Participant name
	Abbie Heaslip




	FOR THE PARTICIPANT

	Instructions

	· You will complete written questions as outlined on the following pages. You must attempt all questions and provide enough detail in your responses to demonstrate your knowledge.
· It is anticipated that you should complete this assessment within two (2) hours, but additional time may be allowed upon negotiation with the Assessor.
· You must complete all questions unassisted by the Assessor or other personnel but may refer to reference material as needed. All questions must be answered correctly for a ‘Satisfactory’ assessment outcome to be awarded. 
· An oral examination may be allowed under certain circumstances, whereby your answers will be documented by another party. 
· Any written questions that are incomplete, or not answered satisfactorily will need to be completed again after further training support.
· If you answer a question incorrectly but modify your response, put your initials next to the written change (or the Assessor must initial a verbal change).

	Resources required

	Pen




	FOR THE ASSESSOR

	Instructions

	· Where oral examination has occurred, ensure that this is acknowledged in writing (e.g. FT001 and Assessor Comments)
· All questions must be satisfactorily demonstrated by the Participant for a Satisfactory determination (indicated by an Assessor tick to the right of the question).
· Assessors are to complete marking in pen of a different colour to the Participant.
· If the Participant verbally modifies their response, write in the modified response verbatim and put your initials next to the written change. 


[bookmark: _Ref396827952]

	[bookmark: _Hlk82780839]ASSESSOR COMMENTS

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	




[bookmark: _Ref128478397]Describe each of the following types of plans and explain what they are used for.

	Answer
	Type of plan
	Description
	Use
	

	
	Presentation drawings
	Presentation drawings include tones and hatches to represent different materials. They are diagrams and are not intended to appear realistic. Basic presentation drawings typically include people, vehicles and trees.
	Presentation drawings are used to explain a scheme and to highlight its features. They describe the design and are generally shown to clients during the design process.
	

	
	Isometric drawings
	An isometric drawing is a three-dimensional (3D) drawing set out using 30-degree angles. In an isometric drawing, the foreshortening of the axes is equal. Therefore, the final image produced is not distorted.
	Isometric drawings provide a 3D representation of an object, building, or design on a 2D surface.
	

	
	Orthographic drawings
	Orthographic drawings are two-dimensional (2D). In each of these drawings, the object (e.g. house) is viewed along parallel lines that are perpendicular to the plane of the drawing (e.g. top view, front view and side view).
	Orthographic drawings show an object from every angle to help the builders and contractors plan the construction.
	

	
	Perspective drawings
	Perspective drawings approximate the flat surface of an object (e.g. a house or a building) as the eye perceives it.
	Perspective drawing accurately depicts spatial depth or perspective and accurately depicts a 3D object onto a 2D plane.
	




[bookmark: _Ref130992849]A client doesn’t understand where or how two (2) wall inserts would look beside a window in the designated living room. What type of drawing could you draw to assist in their understanding?

	[bookmark: _Hlk85785851]Answer
	Presentation drawing
	




[bookmark: _Ref130993108]What type of drawing would you need to present to builders or contractors to give a visual aid of all angles of the building?

	Answer
	Orthographic drawings
	




[bookmark: _Ref130993266]What type of drawings are used to demonstrate landscape features such as trees, rocks and shrubs? 

	Answer
	Presentation drawings
	




[bookmark: _Ref130993728]What type of information can you interpret from a site plan? 

	Answer
	A site plan is a drawing that provides an overview of the entire property. It shows all site elements considered in building construction and gives an idea of the entire scope of work involved in the project. A site plan can be used for purposes such as identifying adjacent roads, identifying the location of the project site, determining structures to be retained or demolished, and determining the building layout and orientation. 

	



[bookmark: _Ref130975341]What is building information modelling (BIM)?

	Answer
	· Building Information Modelling (BIM) is a 3D model-based process that utilises tools and technologies to create and manage digital representations of physical and functional characteristics of structures/ buildings and places
· Used to design, document, analyse, review and generate visualisations
· BIM is used for real-time collaboration

	




[bookmark: _Ref130890045]Explain how the NCC is relevant to construction drawings.

	Answer
	Building Information Modelling (BIM) is a 3D model-based process that utilises tools and technologies to create and manage digital representations of physical and functional characteristics of structures/ buildings and places
Used to design, document, analyse, review and generate visualisations
BIM is used for real-time collaboration
	




[bookmark: _Ref130890248]Discuss the importance of complying with standards during a building and construction project.

	Answer
	Complying with standards is one way to achieve compliance with government minimum requirements set out in the NCC. In addition, standards serve as concrete examples of best practices that can then be used to model what needs to be done in a building and construction project. They serve as thresholds that the project must meet to achieve safety, sustainability and proper functionality. These standards are used to assess the completed building, so referring to them during construction means greater chances of passing these assessments.
As construction personnel tasked with preparing simple building sketches and drawings, you need to know and understand the relevant standards
	



[bookmark: _Ref130994354]Why is it important to confirm that construction plan information complies with building and construction regulations.

	Answer
	Failure to do so can cause delays to the project, safety issues, construction issues, possible fines and the possibility of the construction plans being rejected by the building authorities. 

	




[bookmark: _Ref131053198]When selecting information from plans to present to others, what will determine the format of the information you wish to present?

	Answer
	What is the most appropriate way to present the drawings and sketches so the intended audience can properly understand the information?
Does the intended audience have a preferred mode of presentation?


	




[bookmark: _Ref131054043]What is involved when inspecting drawing equipment for serviceability?

	Answer
	When inspecting drawing equipment for serviceability, you are checking that the equipment or tool you plan to use fits for purpose and has no faults or issues.
The process involves:
Checking for faults or jams
Checking maintenance logs to determine the last time it was serviced
Check f all software to be used is up to date
Conduct a test or pre-start check
And document any identified faults or issues
	




[bookmark: _Ref131054548]Listed below are common drawing conventions. Provide a brief explanation of each.

	Answer
	Drawing convention
	Explanation
	

	
	Sheet layout
	Sheet layout refers to arranging all drawings in the drawing sheet, including the title block (covered in the subsequent discussions). When drawn, the sheet layout for all types of plans (i.e. house plans, floor plans, site plans and elevations) should comply with the AS 1100, Part 3 Architectural Drawing. The standard outlines where things should be located on the page and how different design elements should be drawn, abbreviated and annotated.
	

	
	Title Block
	A title block is an important element of any drawing or plan and provides vital information to assist in reading and understanding the document. Every drawing sheet will have a title block. Usually, you will find the title block on the bottom right-hand corner of the drawing sheet or, sometimes, at the top right corner, depending on the architect or building designer.
	

	
	Line types
	Line types serve the purpose of conveying certain information or differentiating between various components within a drawing. If all lines on a sketch or drawing use the same thickness, it would be hard to interpret their function and what they refer to. Line types further describe the relationships between space and the objects represented and hidden conditions. The different line types include: Solid, dotted, solid with a shaded fill or hatch, dashed or curved.
	

	
	Symbols
	Symbols refer to icons commonly used in building and construction to convey information, such as the location of components and others, to the end-users. They often refer to fixtures, placements and important elements, such as electrical and gas outlets. Most symbols are universal, so it is easy for builders to recognise where fixtures are located by referring to the symbol legend on the drawings.
	

	
	Dimensions
	Dimensions are numerical values expressed in units of measurement, which are important in defining an object's size and other measurements, including length, width, height and thickness. 
In construction drawings, the metric system is usually used (unless otherwise indicated) since Australia uses the metric system. Thus, you can see in the plans that the units metres (m) and millimetres (mm) are typically used to define the dimensions.
	

	
	Dimension lines
	Dimension lines indicate the main object's measurements and are often characterised by light, fine solid lines with terminators on each end, which can be arrows, slashes and thick.
	

	
	Abbreviations
	Abbreviations are shortened forms of common construction terminologies that can be used to represent key information in your drawings. Abbreviations are an important part of any drawing as they keep drawings clear and make them easier to read. By simplifying notations using abbreviations, drawings will not be cluttered with information that would otherwise make them hard to read and may even cause issues locating important information.
	



[bookmark: _Ref131056132]Explain what is learned and confirmed by reading AS 1100.101.

	Answer
	This standard is titled Technical drawing, Part 101: General principles. It covers the basic principles of technical drawing practices, basic use of abbreviations, materials, sizes and layout of drawing sheets, requirements for distinct uniform letters, numerals and symbols, recommended scales and their applications. Additionally, it provides the standards for technical drawings, diagrams, charts, tables, and the specifications for scaling, ratios, technical drawing principles and conventions to assist building professionals in creating quality sketches and drawings.
















	




[bookmark: _Ref131056529]Provide a brief explanation for the following building and construction methods.

	Answer
	Methods
	Explanation
	

	
	Solid brick construction
	Masonary construction that utilises layers, referred to as wythes, of brick with header bricks to hold them together.
	

	
	Brick veneer construction
	Where a wooden or steel frame is concealed with a single layer of bricks as the exterior layer.
	

	
	Framing
	Fitting together separate structural pieces or components to give a structure support and shape.
	

	
	Post and beam construction
	Using heavy timbers instead of dimensional lumber. 
Connections in this method are usually made with plates or bolts.
	




[bookmark: _Ref131056986]Define the following construction terminology.

	Answer
	Term
	Definition
	

	
	Nogging
	This is a horizontal piece of timber fixed between studs in a framed wall.
	

	
	Pilot hole
	This is a hole drilled to receive a nail or a screw.
	

	
	Masonry
	This means brick, concrete, stone, artificial stone or terra cotta laid in mortar.
	

	
	Admixture
	These are materials added to mortar or concrete to achieve modifications to the normal properties of the basic material.
	




[bookmark: _Ref131058922]Discuss what different types of information you must gather to create effective sectional drawings and sketches from building plans. 

	Answer
	To produce effective sectional drawings and sketches, you need to gather information from the building plans schedules, methodologies and photographs, such as measurements, line types, scales and dimensions. This will ensure that accurate information is transferred to the drawings and sketches.
	



[bookmark: _Ref131059321]What type of information might you need to effectively draw bracing details for a wall adjacent to ceiling joists?

	Answer
	For wall bracing adjacent to ceiling joists, you need to know the location of the wall studs, ceiling joists and the truss bottom, measurements of long blocks, the overall layout and position, etc. You can use solid lines to outline these. You can project these orthographically, although it is much better to use isometric projection since it gives you a better grasp of the details
	




[bookmark: _Ref131059730]Discuss the importance of adding labels to the drawing discussed in Q17. 

	Answer
	Labels are important to the drawing to provide a textual description of important parts of the drawing, such as the measurement for long blocks. Additionally, the label specifies the ceiling joist or truss bottom chord's layout or position against the wall bracing top plate.
	




[bookmark: _Ref131060368]Why should the drawing be created ‘to scale’?

	Answer
	Scales are especially significant in illustrating the drawing so that the object's details are captured and that the object fits in the drawing sheet. When objects are scaled up, one can see and examine the intricate details of a component better.
	




[bookmark: _Ref131060863]When using symbols and abbreviations, how can you ensure that each reader of the plans understand what they mean?

	Answer
	Most symbols and abbreviations are universal, so it is easy for builders to recognise and understand what where key things are. Other uncommon symbols and abbreviations are in a separate sheet's ‘Legend’ portion to briefly describe what they are and when they are used.
	




[bookmark: _Ref131063017]Discuss the sheet layout and information included to present elevation drawings to the local council for approval.

	Answer
	Elevation drawings must illustrate all sides of a building to give a complete and final picture of the building structure. They must also contain all the necessary information to be submitted to the local council for approval. The information must be clearly labelled and include precise and accurate measurements of the building structure. 
For every sheet you make, you need to include information such as the following:
Dimensions
Scale
Title Block
Notes
Section Number
Type of View

	




[bookmark: _Ref128474348]What format would you produce construction plans to present to each of the following recipients?

	Answer
	Recipients
	Format (hard copy/ digital)
	

	
	Client
	PDF files or a video animation or powerpoint
	

	
	Builder/ Contractor
	Hardcopy prints
	

	
	Local Council
	Online Submission
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PRACTICAL ASSESSMENT


	Participant name
	Abbie Heaslip




	FOR THE PARTICIPANT

	Instructions

	· The tasks outlined on the following pages will require performance of normal workplace activities, as a result of a structured activity set by an Observer in the workplace or a simulated activity set by your Assessor/Observer. 
· The timeframe for these tasks will be established by your Assessor/Observer, in consideration of location conditions and industry requirements.
· You must complete all tasks unassisted by the Assessor or other personnel, unless the steps note this assistance. 
· You must attempt all tasks (and itemised steps) for a ‘Satisfactory’ assessment outcome to be awarded.
· For any observation conducted that is incomplete, or without satisfactory performance, the observation will need to be completed again after further training support.




	FOR THE ASSESSOR/OBSERVER

	Instructions

	· The following observation record should be used to judge and record your observations of the Participant as they complete the task(s) set. You must record your observations of the Participant’s performance. 
· For each occasion, indicate the task performed and whether it was a simulation or workplace-based task. 
· Any simulated assessment must ensure the Participant still performs under workplace conditions which reflect industry standards.
· In the comments, provide clear detail regarding the task that the Participant was required to do (e.g. PPE used, materials handled, attachments connected, plant types).
· All steps must be satisfactorily demonstrated by the Participant for a ‘Satisfactory’ determination (indicated by an Assessor tick to the right of each itemised step, or an Observer tick to the right of each itemised step, and confirmation by an Assessor in the Assessor Comments).
· Where you have determined that one or more task steps have not been satisfactorily demonstrated, provide the Participant with additional support and outline details of such assistance in the Assessor/Observer Comments. Allow the Participant two (2) further opportunities to demonstrate the task again to allow an opportunity for a ‘Satisfactory’ assessment outcome to be achieved. 
· If after three (3) attempts the Assessor determines that the Participant cannot demonstrate the required steps, a ‘Not Satisfactory’ outcome is to be determined.





	TASK OUTCOME

	Task
	Date
	Task Type (Tick)
	Location
	Task outcome (Tick)

	
	
	
	
	Satisfactory
	Not Satisfactory

	Task 1 (Occasion 1)
	Select Date.
	 Workplace
 Simulation
	
	
	

	Task 1 (Occasion 2)
	Select Date.
	 Workplace
 Simulation
	
	
	



	ASSESSOR COMMENTS: GENERAL

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	



	ASSESSOR COMMENTS: PRACTICAL TASK 1: OCCASION 1 Structural component

	 Individual student (as named on cover page)
 Multiple students [ All from Attendance Report,  Specific students involved – identify students]

	Task
	Provide detail 

	1.2B. 1.2C. 
1.3B. 
	Specify Standard drawing conventions applied: 
When assisting in the preparation of the detail structural drawings, Abbie applied drawing conventions such as scales (1:25), and dimension lines.

	1.3C. 
	Specify form created for presentation:
These drawings were presented as hard copies to the engineering team



	ASSESSOR COMMENTS: PRACTICAL TASK 1: OCCASION 2  Non-structural component

	 Individual student (as named on cover page)
 Multiple students [ All from Attendance Report,  Specific students involved – identify students]

	Task
	Details

	1.2B. 1.2C. 
1.3A. 1.3B. 
	Specify Standard drawing conventions applied: 
When assisting in the preparation of the elevation drawings, Abbie applied drawing conventions such as scales (1:100), and dimensions

	1.3C. 
	Specify form created for presentation:
These drawings were presented as hard copies to the engineering team. 




CPCCBC4014
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	Practical Task 1 (2X)

	Description of task:
The participant must demonstrate the skills and knowledge to produce and prepare two (2) simple sketches of different components of the fabric of a building from a set of construction plans (HO3- CSTC RTO facility plans). The sketches must be of one (1) structural component (Occasion 1- typical wall detail) and one (1) non-structural component (Occasion 2 – shower base detail). During the demonstration, the assessor will be checking for evidence of:
· Prepare to make sketches and drawings.
· Determine the relevant information from construction plans that is required for sketching or drawing. (Template available for use- HO2-Planning sheet))
· Check construction plan information against building and construction regulations, standards and codes for compliance, including safety and the environment. (Template available for use- HO1-Compliance review)
· Consider the intended audience and purpose of drawings to determine appropriate presentation method. (Template available for use- HO2-Planning sheet))
· Determine the most suitable format for the information and select and check availability of all materials, tools and equipment and check for serviceability before use. (Template available for use- HO2-Planning sheet))
· Create simple sketches and drawings.
· Determine and record measurements, information and details required for drawing and sketches. (Template available for use- HO2-Planning sheet)
· [bookmark: _Hlk135296544]Using all the gathered information create two-dimensional and three-dimensional sketches/drawings of one structural section of a typical wall detail and one non-structural sectional drawing of the shower base detail using standard drawing convention.
· Clearly identify and label the elements and components in the sectional drawings.
· Notate and process drawings.
· Include all essential information to the drawings using dimension lines, symbols and abbreviations following standard drawing conventions.
· Include drawing and job tile, date, scale and sheet number in the title block.
· Produce clear and descriptive completed drawings in an appropriate form for presentation.
· Submit completed drawings with name and date attached to assessor as evidence.

These tasks may be simulated or real. The Participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. The Observer is to provide detailed comments on the tasks completed by the Participant (on the Observer Comments, overleaf). The Assessor is to verify the Observer’s comments, noting their findings in the Assessor Comments (on the back of the Practical Assessment cover page) and provide the assessment outcome.

	Resources required: 
Construction plans and specifications; Access to current building and construction codes and standards, the NCC, workplace procedures and other quality documentation; Hand drawing materials, tools and equipment; PC, applications and software to access drawings and other relevant information.

	Observer details

	Name of observer:
	Ryan Murphy

	Role of observer 
(Confirm suitability to sign)
	Senior Contracts Administrator

	Email address of observer
	Ryan.murphy@jhg.com.au

	Signature of observer:
	
	Date:
	5/11/2024



	When completing the task, did the Participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	
	1st
Occasion
	2nd
Occasion

	1 Prepare to make sketches and drawings.

	[bookmark: _Ref131077206]Determine the relevant information from construction plans required for sketching or drawing. (Template available for use- HO2-Planning sheet))
		
	[bookmark: _Ref131077214]Check construction plan information against building and construction regulations, standards and codes for compliance, including safety and the environment. (Template available for use- HO1-Compliance review)
		
	[bookmark: _Ref131077320]Consider the intended audience and purpose of drawings to determine appropriate presentation method. (Template available for use- HO2-Planning sheet))
		
	[bookmark: _Ref131077328]Determine the most suitable format for the information and select and check availability of all materials, tools and equipment and check for serviceability before use. (Template available for use- HO2-Planning sheet))
		
	2 Create simple sketches and drawings.

	[bookmark: _Ref131077335]Determine and record measurements, information and details required for drawing and sketches. (Template available for use- HO2-Planning sheet)
		
	[bookmark: _Ref131074589]Using all the gathered information create two-dimensional and three-dimensional sketches/drawings of one structural section of a typical wall detail (Occasion 1)and one non-structural sectional drawing of the shower base detail (Occasion 2) using standard drawing convention.
		
	[bookmark: _Ref131074591]Clearly identify and label the elements and components in the sectional drawings.
		
	3 Notate and process drawings.

	[bookmark: _Ref131074746]Include all essential information to the drawings using dimension lines, symbols and abbreviations following standard drawing conventions.
		
	[bookmark: _Ref131074748]Include drawing and job tile, date, scale and sheet number in the title block.
		
	[bookmark: _Ref131074782]Produce clear and descriptive completed drawings in an appropriate form for presentation.
		
	[bookmark: _Ref131077438]Submit completed drawings with name and date attached to assessor as evidence.
		




	Observer comments:

	Abbie has demonstrated her ability to understand and prepare plans and drawings. She is able to identify the regulations and codes of practice required and if the plans comply.
She has displayed this through both structural and no-structural components and plans in both real-time and simulation experiences. Overall, Abbie has showed her ability and understanding in the preparing plans and sketches.
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