PRACTICAL ASSESSMENT 2

Communication of unsatisfactory work to concrete sub-contractor:
Good morning Scott,
Yesterday your guys poured the ground slab for ‘Townhouse 3’, unfortunately the step down in the concrete for the bathroom was not installed as you can see in the picture below:
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The slab will need to be cut and jackhammered down to below the intended RL and then filled up with self levelling contcrete to the RL that it is meant to be. As the installation of the set downs is part of your contract this will need to be done at your expense. Please don’t hesitate to get in contact with me if you have any questions or concerns.
Thanks
Matt Cumiskey





Material delivery for commercial build of townhouses:

Deliveries to 10-18 Robertson Street Carina Monday 12th October 2020
	Delivery for:
	Supplier:
	Description:
	Qty/Units:
	Delivery received by:
	Notes:

	East electrical
	MM Electrical
	21mm conduit
	5 x 50 3.6m lengths
	Matt
	1 pack of 50 was taken to each townhouse

	Pete’s Plasters
	USG Boral
	2400x1200 gyprock
	70 sheets
	Matt
	Sheets for townhouse 3

	Tony’s Tiling
	Beaumont 
	Bathroom floor tiles
	6 boxes of tiles
	Matt
	Bathroom floor tiles for main bathroom and ensuite for Townhouse 1
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