CONTRACTOR LIST



	Relevant construction works/services
	Description/scope

	Demolition labour
	Demolish existing kitchen and make good
Dismantling the existing storage, slab platform including supporting walls, wall tiles, flooring, sink etc. at all levels as required carefully and disposing off and clearing away the debris
Slabs to be chased to allow for new plumbing



	Kitchen Labour
	Installation of supply mentioned above

	Butlers Pantry Labour
	Installation of supply mentioned above

	Laundry Labour
	Installation of supply mentioned above

	Plumbing
	Installation of supply mentioned above
Slabs to be chased to allow for new plumbing
Plumbing cap off and reconnections
Plumbing dis-connections to existing serviceable connection points and connections
Water dis-connection and connections from pre-tapped water main


	Electrical
	Installation of supply mentioned above
Electricity cap off and reconnections
Electricity dis-connections to existing serviceable connection points and connections
Duct work for bench mount exhaust to run through back of drawers and wall to external wall and motor
Cooktop downdraft ventilation system

	Building / Carpentry Labour
	Labour for scopes of work described excluding the installation of above fixtures
New stud plasterboard wall to be build
New fixed glass window to existing opening
Enclose wall above and below to match existing 
Window tint to be discussed with client
New doors to match switch opening with screens
New doors to match triple slider with screens
New Laundry door location cavity slider to match existing
Tambour door in kitchen
New Laundry window to suit existing opening width over dishwasher


	Tiling Labour
	Installation of supply mentioned above

	Butlers Pantry - Fixed Glass Window Labour
	Installation of supply mentioned above

	French Doors - Triple Slider Labour
	Installation of supply mentioned above

	Dining Room Slider - Reverse Opening Labour
	Installation of supply mentioned above

	Removal of Debris
	Labour and clean-up



