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CPCCBC4053 
Apply building codes and standards to the construction process for Class 2 to 9 Type C buildings 

ASSESSMENT SUMMARY

The assessment activities for CPCCBC4053 Apply building codes and standards to the construction process for Class 2 to 9 Type C buildings cover all aspects of the unit of competency. For Apprentices/Trainees, this includes supervisor completion of the Apprentice/Trainee Record (ATR). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be fair, flexible, valid and reliable. If a Participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a Participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the Participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a Participant does not answer all questions or perform all tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. 

The Trainer/Assessor can provide the Participant with additional information on interpreting the assessment outcomes and guide the Participant’s options. If a Participant is still deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result as per the process in the Student Handbook. 

By signing below, the Participant acknowledges:
· They understand the assessment instructions and requirements, and consent to being assessed. 
· The work submitted is to be their own work – with the work of/with others needing to be clearly acknowledged and documented. 
· They consent to any photo/video recording of their work that occurs during assessment. 

	Participant name
	Dawei Yang

	Participant signature
	


	Pre-requisite unit(s) to be achieved and authenticated prior to undertaking assessment

	 Not applicable 



	Task
	Date completed
	Assessment Results 

	Theory Exam
	Select Date.
	 Satisfactory 
	 Not Satisfactory

	Workbook 
	Select Date.
	 Satisfactory 
	 Not Satisfactory

	Practical Assessment
	Select Date.
	 Satisfactory 
	 Not Satisfactory

	Outcome for CPCCBC4053
	Select Date.
	 Competent
	 Not Yet Competent



	Evidence requirements checklist (ticked by assessor and evidence supplied to RTO)

	 Theory Exam
 Workbook
 Practical Assessment
	 Documentation of design and construction (suitability or evidence of suitability)
 Fire protection inspection checklist



	Assessor name
	

	Assessor signature
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THEORY EXAM


	Participant name
	Dawei Yang




	FOR THE PARTICIPANT

	Instructions

	· You will complete written questions as outlined on the following pages. You must attempt all questions and provide enough detail in your responses to demonstrate your knowledge.
· It is anticipated that you should complete this assessment within two (2) hours, but additional time may be allowed upon negotiation with the Assessor.
· You must complete all questions unassisted by the Assessor or other personnel but may refer to reference material as needed. All questions must be answered correctly for a ‘Satisfactory’ assessment outcome to be awarded. 
· An oral examination may be allowed under certain circumstances, whereby your answers will be documented by another party. 
· Any written questions that are incomplete, or not answered satisfactorily will need to be completed again after further training support.
· If you answer a question incorrectly but modify your response, put your initials next to the written change (or the Assessor must initial a verbal change).

	Resources required

	Pen




	FOR THE ASSESSOR

	Instructions

	· Where oral examination has occurred, ensure that this is acknowledged in writing (e.g. FT001 and Assessor Comments)
· All questions must be satisfactorily demonstrated by the Participant for a Satisfactory determination (indicated by an Assessor tick to the right of the question).
· Assessors are to complete marking in pen of a different colour to the Participant.
· If the Participant verbally modifies their response, write in the modified response verbatim and put your initials next to the written change. 


[bookmark: _Ref396827952]

	[bookmark: _Hlk82780839]ASSESSOR COMMENTS

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	




[bookmark: _Ref127186634]Provide a brief description of the given classes of buildings according to the National Construction Code (NCC). 

	Answer
	Assessment method
	Description
	

	
	Class 2 building
	A building containing two or more sole-occupancy units. Each unit must be a separate dwelling. 
	

	
	Class 3 building
	Class 3 buildings are residential buildings other than Class 1 or 2. These are long-term or transient living accommodations for unrelated people. These include the following:
boarding house, guest house, a hostel or backpackers larger than the limits of a Class 1b building
dormitory-style accommodation or workers’ quarters, e.g. fruit-pickers
healthcare facilities like accommodations for children, elderly or people with disability which must not be considered under Class 9
residential parts of motels, hotels, schools, hospitals, or jails
	

	
	Class 4 building
	A Class 4 building is the only dwelling or residence within any Class 5, 6, 7, 8 or 9 buildings.
	

	
	Class 5 building
	An office building used for professional or commercial purposes, except for buildings of Class 6, 7, 8 or 9. Examples include: 
law office
office for general medical practitioners
	

	
	Assessment method
	Description
	

	
	Class 6 building
	Buildings that directly sell goods by retail or supply services to the public, such as:
restaurants or cafés
markets, shopping centres and malls
public laundry
hairdressers and barbershops
	

	
	Class 7a building
	Car-parks
	

	
	Class 7b building
	The following buildings are classified under Class 7b:
warehouses
storage buildings
buildings used to display or produce wholesale goods 
	

	
	Class 8 building
	These are process-type buildings such as:
buildings used for production, assembling, altering, repairing, finishing, packing or cleaning of goods or produce
laboratories (classified as such because of their high potential for fire hazard)
	





[bookmark: _Ref128984255]Discuss Class 9 buildings according to the NCC, including the difference between the three (3) Class 9 sub-classifications.

	Answer
	
	


	
	Buildings of public nature

	Class 9a
	Healthcare buildings in which occupants are either: 
· undergoing or have undergone medical treatment; or
· in need of physical assistance in the evacuation during emergencies.

	Class 9b
	Assembly buildings used for social, theatrical, political, religious, or civil purposes. The following are examples of Class 9b buildings:
· schools
· universities
· childcare centres
· pre-schools
· sporting facilities
· night clubs
· public transport buildings

	Class 9c
	An aged care building. An aged care building is defined as a residential accommodation for elderly people who are:
· provided with personal care services; and
· need 24-hour staff assistance to evacuate the building in an emergency.




[bookmark: _Ref128115391]A client is showing you the plans for a group of four (4) dwellings over two (2) storeys, above a common basement or carpark. Determine what classification would be assigned to this building. Explain your answer.

	Answer
	Class two building Class 2 buildings may also be single storey attached
dwellings with a common space below. For example,
2 dwellings above a common basement or carpark 
	




[bookmark: _Ref128115393]Another client would like to build a new doctors surgery. Determine what classification would be assigned to this. Explain your answer.

	Answer
	Class three  These are long-term or transient living accommodations for unrelated people. 
	



[bookmark: _Ref128119881]Explain why the plans for a warehouse that contains a caretakers residence may have more than one classification.

	Answer
	a building can be used for different purposes, multiple classifications are allowed. 
	




[bookmark: _Ref128990469]What dictates how buildings must be constructed in Australia and how may this differ in your State or Territory?

	Answer
	State/Territory Legislation
	




[bookmark: _Ref127183513]Explain why it is important to understand references the NCC makes to Australian Standards.

	Answer
	The NCC is considered a performance-based code. It requires you to comply with the minimum level of health, safety, amenity, and sustainability set in the Performance Requirements
	




[bookmark: _Ref128991786]Clarify the purpose of compliance with AS 3600.

	Answer
	specifies minimum requirements for the design and construction of concrete building structures and members that contain reinforcing steel or tendons, or both. Known as the AS 3600 Concrete code, also sets out requirements for plain concrete and pedestal footings.
	




[bookmark: _Ref128995884]Provide a brief explanation of the listed NCC compliance assessment methods used to determine compliance using a Performance Solution pathway.

	Answer
	Assessment method
	Description
	

	
	Evidence of suitability
	This is also known as ‘documentary evidence.’ This entails showing evidence that the use of material, plumbing and drainage product or form of construction or design meets the Performance Requirements or a DTS Provision
	

	
	Verification methods
	.Verification Methods include quantifiable or predetermined acceptable criteria that must be achieved by the given compliance option. 
	

	
	Comparison with DTS Provisions
	This method applies to Performance Solutions. It involves doing a comparative analysis to determine whether Performance Solutions provide the superior or same level of health, safety, amenity, or sustainability as using the DTS provisions.
	

	
	Expert Judgement
	An expert can either be a person or an organisation with the necessary skills and experience to make a judgement concerning NCC compliance. 
	



[bookmark: _Ref127263388]Discuss the listed levels found in the NCC Performance Hierarchy.

	Answer
	Performance Hierarchy
	Description
	

	
	Objectives
	something that one's efforts or actions are intended to attain or accomplish; purpose; goal; target
	

	
	Functional statements
	describe conditions in the building that help satisfy the objectives.
	

	
	Performance requirements
	 the minimum level that buildings, building elements and plumbing and drainage systems must meet
	

	
	Building Solutions
	provides a tailored solution to meet the intended objective of the Performance Requirements
	




[bookmark: _Ref127278250][bookmark: _Ref129067815]Why may you need to use a combination of Performance Solutions and Deemed-to-Satisfy (DtS) solutions to comply with the Performance Requirements of the NCC?

	Answer
	A combination of the two solutions can be used when satisfying a single Performance Requirement. This is possible when Performance Requirements cover several elements within a building. The Assessment Method to be used depends on which compliance option was applied. 
	




[bookmark: _Ref129066894]Discuss the workplace policies and procedures that should be held on-site.

	Answer
	code of conduct.
mobile phone policy.
non-smoking policy.
drug and alcohol policy.
health and safety policy.
anti-discrimination and harassment policy.
	




[bookmark: _Ref129067939]Describe the basic principles of structural design and how these align with large span structures.

	Answer
	a principle of structures is that they be designed to maintain a state of equilibrium; resisting external loads without moving.Structures having spans more than 20 meters are considered long-span structures. Trusses, folding plates, shell structures, frames, tent structures, and tensile structures are the most prevalent forms of long-span structures.
	




[bookmark: _Ref127274757]What type of information is determined from the working drawings and specifications when organising the excavation for a shopping centre with underground parking?

	Answer
	earthworks
erosion and sediment controls
concrete works
fencing
building works
roads
electrical systems
water reticulation systems
	




[bookmark: _Ref127253785]Discuss compressive and tensile stresses on buildings.

	Answer
	Tension forces are pulling forces that tend to elongate or stretch the material, while compression forces are pushing forces that tend to compress or shorten the material.
	




[bookmark: _Ref129070306]Briefly clarify the meaning of ‘water ingress’ when related to waterproofing a building.

	Answer
	Water ingress is when water makes its way into a building. 

	




[bookmark: _Ref129071735]What do you check for to confirm product compliance with NCC requirements?

	Answer
	Compliance with the NCC's mandatory Performance Requirements is achieved by developing a Performance Solution, a DTS Solution, or a combination of the two.
	




[bookmark: _Ref129071897]Where do you record checks that you have made on products and materials that have arrived on-site?

	Answer
	Material inspection report
	




[bookmark: _Ref129075029]What are some indications that a construction company is abiding by environmental protection laws?

	Answer
	All construction job undertake CEMP  
	



[bookmark: _Ref129075323]Explain your understanding of the following concepts relating to sustainability.

	Answer
	Concept
	Explanation 
	

	
	Ecological footprint
	The ecological footprint (EF) estimates the biologically productive land and sea area needed to provide the renewable resources that a population consumes and to absorb the wastes it generates
	

	
	Renewable energy
	Renewable energy is energy derived from natural sources that are replenished at a higher rate than they are consumed.
	




[bookmark: _Ref128122622]Provide the six (6) bushfire attack level ratings that AS 3959 uses to establish the requirements for construction. Explain each rating.

	Answer
1.



2.



3.



4.



5.



6.
	
BAL-Low



 BAL-12.5



19



29


40



FZ

	



[bookmark: _Ref128122625]Complete the table below by identifying the type of fire-resisting construction (i.e. Type A, Type B, or Type C) given the following class of building and number of storeys each class of building has.

	Answer
	Rise in Storeys
	Class of building:
2,3,9
	Class of building:
5,6,7,8
	

	
	4 or more
	A
	A
	

	
	3
	A
	B
	

	
	2
	B
	C
	

	
	1
	C
	C
	




[bookmark: _Ref128129905]Respond to each of the following regarding zero-energy building.

	Answer
	
	Zero energy building
	

	
	Definition
	a zero energy building produces enough renewable energy to meet its own annual energy consumption requirements, thereby reducing the use of nonrenewable energy in the building sector. 
	

	
	One (1) technique used in zero energy building
	Solar power
	

	
	The procedure in implementing the technique you have identified
	Install solar panel on the rood
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WORKBOOK


	Participant name
	Dawei Yang




	FOR THE PARTICIPANT

	Instructions

	· You will complete written activities as outlined on the following pages. You must attempt all questions and provide enough detail in your responses to demonstrate your knowledge.
· The timeframe for these tasks will be established by your Assessor or Training Plan, but additional time may be allowed upon negotiation with the Assessor.
· You must complete all questions unassisted by the Assessor or other personnel but may refer to reference material as needed. All questions must be answered correctly for a ‘Satisfactory’ assessment outcome to be awarded. 
· An oral examination may be allowed under certain circumstances, whereby your answers will be documented by another party. 
· Any written questions that are incomplete, or not answered satisfactorily will need to be completed again after further training support.
· If you answer a question incorrectly but modify your response, put your initials next to the written change (or the Assessor must initial a verbal change).

	Resources required

	Pen




	FOR THE ASSESSOR

	Instructions

	· Where oral examination has occurred, ensure that this is acknowledged in writing (e.g. FT001 and Assessor Comments)
· All questions must be satisfactorily demonstrated by the Participant for a Satisfactory determination (indicated by an Assessor tick to the right of the question).
· Assessors are to complete marking in pen of a different colour to the Participant.
· If the Participant verbally modifies their response, write in the modified response verbatim and put your initials next to the written change. 




	ASSESSOR COMMENTS

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	




NOTE

At times, you will be provided with a specific business context to which you must respond, otherwise it is anticipated that you will use a workplace of your choosing (your own, or hypothetical) to provide the context to the task.

At all times, the responses in your assessment must reference Australian (Queensland or Federal) documentation, including legislation, regulations, codes of practice, standards and guidance publications.

	ACTIVITY 1  [bookmark: _Ref35349341]

	Access the National Construction Code (NCC) to:
a) Determine where to locate the technical building requirements for Class 2 to 9 buildings.
b) What is stated in Volume One Amendment 1 – Queensland Part B1 Structural provisions?
c) What is stated in Volume One Amendment 1 – NSW Section A6.6 Class 6 buildings?



	a) Determine where to locate the technical building requirements for Class 2 to 9 buildings.

	The classification of a building or part of a building is determined by the purpose for which it is designed, constructed or adapted to be used.

	b) What is stated in Volume One Amendment 1 – Queensland Part B1 Structural provisions?

	Deemed-to-Satisfy Provisions

	c) What is stated in Volume One Amendment 1 – NSW Section A6.6 Class 6 buildings?

	A Class 6 building is a shop or other building used for the sale of goods by retail or the supply of services direct to the public, including—
(1) an eating room, café, restaurant, milk or soft-drink bar; or
(2) a dining room, bar area that is not an assembly building, shop or kiosk part of a hotel or motel; or
(3) a hairdresser's or barber's shop, public laundry, or undertaker's establishment; or
(4) market or sale room, showroom, or service station.





	Satisfactory Outcome
	
	




	ACTIVITY 2  [bookmark: _Ref128995624]

	Access the National Construction Code (NCC) Volume One Amendment 1 - Section A Governing Requirements - Part A2 Compliance with the NCC and respond to the following:
a) What does this Part explain?
b) What methods are available to achieve the Performance requirements?
c) How is a performance solution shown to comply with the relevant Performance Requirements? 



	a) What does this Part explain?

	This Part explains the possible methods of demonstrating compliance with the NCC. It explains the various compliance pathways within the NCC and the appropriate steps that must be taken for each of these pathways.

	b) What methods are available to achieve the Performance requirements?

	A Performance Solution.
(2)
A Deemed-to-Satisfy Solution.
(3)
A combination of (1) and (2).

	c) How is a performance solution shown to comply with the relevant Performance Requirements?

	(a)Evidence of suitability in accordance with Part A5 that shows the use of a material, product, plumbing and drainage product, form of construction or design meets the relevant Performance Requirements.
(b)A Verification Method including the following:
(i)The Verification Methods provided in the NCC.
(ii)Other Verification Methods, accepted by the appropriate authority that show compliance with the relevant Performance Requirements.
(c)Expert Judgement.
(d)Comparison with the Deemed-to-Satisfy Provisions.





	Satisfactory Outcome
	
	




	ACTIVITY 3  [bookmark: _Ref128134618]

	Some occupants of a brick apartment building have complained about plaster damage, mould build up, damaged skirting and floorboards. The issue seems to affect rooms beside or including bathrooms.

Given the information above:
a) Identify factors that may have contributed to the damage issue.
b) Identify which Part from the NCC Volume 1 Amendment 1 was not properly applied.
c) Briefly explain how the identified Part from the NCC Volume 1 was not properly applied.
d) Identify which Australian standard was not properly applied.
e) Briefly explain how the identified Australian standard was not properly applied.
f) Identify what other defect the building may have considering the deviations of the construction from the code and standard.
g) Describe the extent of the work that needs to be done to rectify the issue.



	a) Identify what contributed to the degradation issue.

	 water, craftsmanship, or structural integrity of the building

	b) Identify which Part from the NCC Volume 1 Amendment 1 was not properly applied.

	Part A5 Documentation of design and construction

	c) Briefly explain how the identified Part from the NCC Volume 1 was not properly applied.

	(1)
The form of evidence used must be appropriate to the use of the material, product, plumbing product, form of construction or design to which it relates.

(2)
Any copy of documentary evidence submitted must be a complete copy of the original certificate, report or document.

	d) Identify which Australian standard was not properly applied.

	Water proof

	e) Briefly explain how the identified Australian standard was not properly applied.

	E-poxy is not applied as underlay

	f) Identify what other defect the building may have considering the deviations of the construction from the code and standard.

	All the external timber should select waterproofing one 

	g) Describe the extent of the work that needs to be done to rectify the issue.

	Confirm all external timber are processed by waterproofing 




	Satisfactory Outcome
	
	




	ACTIVITY 4  [bookmark: _Ref129007825]

	Access the NCC via the internet to locate the requirements applicable to a building development in the Brisbane area, containing 6 sole-occupancy units, two (2) on each level, each being a separate dwelling. 
This building includes one (1) basement level designated for car parking. 
The proposed building structure requires reinforced concrete floors and columns.
Document your findings or where in the NCC the information can be located. 




Building Description
	Classification

	2

	Rise in Storeys

	3

	Number of Storeys

	4

	Type of construction

	concrete

	Climate Zone and description

	Climate zone 5 - warm temperate.


Fire resistance and stability
	Locate fire resistance information

	A

	Compartmentation and fire separation

	FRL90 

	Fire hazard properties of materials, assemblies, fixtures and linings

	Doors windows curtains 



Material requirements
	Reinforced concrete requirements relative to Australian Standards

	 AS 2870 and AS 3600. 

	Glazing requirements specifically for windows, sliding doors with frames and balconies.

	AS 1288:2021 



	Satisfactory Outcome
	
	



	ACTIVITY 5  [bookmark: _Ref127273569]

	The building discussed in ACTIVITY 2 includes one (1) basement level designated for car parking. 
Provide information required for 
· Bored piling to retain the soil and enable basement walls.
· Work Health and Safety
· Water proofing
· Water ingress

Document your findings or where the information can be located. 



	Bored piling to retain soil and enable basement walls 

	The soil conditions of your site: Is the soil cohesive (clayey) or non-cohesive (gravel/sand), is very high strength rock present.
How deep your basement needs to be: Is it a single level basement for a residential application or a multi-level basement car park for a high-rise office building.
Weather you basement is above or below the water table: Is your lowest basement level significantly lower than the expected water table level of the area? Is the basement close to the shoreline?
Proximity of the basement to site boundary or neighbouring structure: Does a structure exist close by which may run the risk of being undermined depending on the basement wall construction type chosen?

	Work Health and Safety

	All the on site stuff follow WHS policy

	Water proofing

	Performanve solution

	Water ingress

	DTS solution



	Satisfactory Outcome
	
	



	ACTIVITY 6  [bookmark: _Ref129073248]

	A newly-built hotel needed to have its second-storey elevator lobby renovated, so customers had to take the stairs to get to the second storey of the hotel. On more than one occasion, people with visual impairment have had trouble finding the first step of the stairway, with some even misjudging the first step and falling over. No serious injury has happened yet, but the hotel manager decided something had to be done with the lack of indication of the first step of the stairway. An investigation was made after the third person tripped over the first step, and the investigation revealed that no research on who could possibly use the stairs was done. Respond to the following:
a) Identify one factor that contributed to the failure of the people with visual impairment to find the stairs of the hotel.
b) Identify which clause from the NCC Volume 1 was not properly applied.
c) Briefly explain how the clause from the NCC Volume 1 was not properly applied.
d) Identify which Australian standard was not properly applied.
e) Describe the extent of work that needs to be done to rectify the breach.



	a) Identify one factor that contributed to the failure of the people with visual impairment to find the stairs of the hotel.

	t the lack of indication

	b) Identify which clause from the Building Code of Australia Volume 1 was not properly applied.

	Section D

	c) Briefly explain how the identified clause from the Building Code of Australia Volume 1 was not properly applied.

	a ramp complying with AS 1428.1 or a passenger lift need not be provided to serve a storey or level other than the entrance storey in


	d) Identify which Australian standard was not properly applied.

	 AS 1428.1 

	e) Describe the extent of work that needs to be done to rectify the breach.

	Install ramp



	Satisfactory Outcome
	
	




Workbook - CPCCBC4053 Apply building codes and standards to the construction process for Class 2 to 9 Type C buildings

	Workbook - CPCCBC4053 Apply building codes and standards to the construction process for Class 2 to 9 Type C buildings


CPCCBC4053 
Apply building codes and standards to the construction process for Class 2 to 9 Type C buildings

PRACTICAL ASSESSMENT


	Participant name
	Dawei Yang




	FOR THE PARTICIPANT

	Instructions

	· The tasks outlined on the following pages will require performance of normal workplace activities, as a result of a structured activity set by an Observer in the workplace or a simulated activity set by your Assessor/Observer. 
· The timeframe for these tasks will be established by your Assessor/Observer, in consideration of location conditions and industry requirements.
· You must complete all tasks unassisted by the Assessor or other personnel, unless the steps note this assistance. 
· You must attempt all tasks (and itemised steps) for a ‘Satisfactory’ assessment outcome to be awarded.
· For any observation conducted that is incomplete, or without satisfactory performance, the observation will need to be completed again after further training support.




	FOR THE ASSESSOR/OBSERVER

	Instructions

	· The following observation record should be used to judge and record your observations of the Participant as they complete the task(s) set. You must record your observations of the Participant’s performance. 
· For each occasion, indicate the task performed and whether it was a simulation or workplace-based task. 
· Any simulated assessment must ensure the Participant still performs under workplace conditions which reflect industry standards.
· In the comments, provide clear detail regarding the task that the Participant was required to do (e.g. PPE used, materials handled, attachments connected, plant types).
· All steps must be satisfactorily demonstrated by the Participant for a ‘Satisfactory’ determination (indicated by an Assessor tick to the right of each itemised step, or an Observer tick to the right of each itemised step, and confirmation by an Assessor in the Assessor Comments).
· Where you have determined that one or more task steps have not been satisfactorily demonstrated, provide the Participant with additional support and outline details of such assistance in the Assessor/Observer Comments. Allow the Participant two (2) further opportunities to demonstrate the task again to allow an opportunity for a ‘Satisfactory’ assessment outcome to be achieved. 
· If after three (3) attempts the Assessor determines that the Participant cannot demonstrate the required steps, a ‘Not Satisfactory’ outcome is to be determined.





	TASK OUTCOME

	Task
	Date
	Task Type (Tick)
	Location
	Task outcome (Tick)

	
	
	
	
	Satisfactory
	Not Satisfactory

	Task 1 (Occasion 1)
	Select Date.
	 Workplace
 Simulation
	
	
	

	Task 1 (Occasion 2)
	Select Date.
	 Workplace
 Simulation
	
	
	



	ASSESSOR COMMENTS: GENERAL

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	



	ASSESSOR COMMENTS: PRACTICAL TASK 1: OCCASION 1- Class 2, 3 or 9

	þ Individual student (as named on cover page)
 Multiple students [ All from Attendance Report,  Specific students involved – identify students]

	Task
	Provide detail 

	1.1A. 1.1B. 1.1C. 1.1D. 
	Specify () where building classifications, criteria requirements and performance solutions were documented:
þ Workplace Quality document  Quality Assurance Template  Other (please specify):



 Document attached as evidence

	1.2D. 
	Specify () who was consulted regarding compliance options: 
 Project management  Relevant tradesperson þ Builder  Supplier 
 Other (please specify): 

	1.3C. 
	Specify building checked for compliance with active fire protection requirements:



 Is checklist used attached as evidence





	ASSESSOR COMMENTS: PRACTICAL TASK 1: OCCASION 2 - Class 5 to 8

	þ Individual student (as named on cover page)
 Multiple students [ All from Attendance Report,  Specific students involved – identify students]

	Task
	Details

	1.1A. 1.1B. 1.1C. 1.1D. 
	Specify () where building classifications, criteria requirements and performance solutions were documented:
þ Workplace Quality document  Quality Assurance Template  Other (please specify):



 Document attached as evidence

	1.2D. 
	Specify () who was consulted regarding compliance options: 
 Project management  Relevant tradesperson þ Builder  Supplier 
 Other (please specify): 

	1.3C. 
	Specify building checked for compliance with active fire protection requirements:



 Is checklist used attached as evidence





CPCCBC4053
Apply building codes and standards to the construction process for Class 2 to 9 Type C buildings

	Practical Task 1 (2X)

	Description of task:
The participant must demonstrate the skills and knowledge to apply building codes and standards to the construction process for Class 2 to 9 Type C buildings. 
· Occasion 1 - Class 2, 3 or 9
· Occasion 2 - Class 5 to 8
Documented evidence of all criteria must be presented (template (HO1) available for use if required) The participant must also inspect one existing buildings for fire protection compliance using workplace or created document (See HO2 for information). Assessor and observer will be looking for evidence including:
· Classify building and document findings.
· Read the plans and specifications to determine the nature of the building, its use and arrangement.
· Read and correctly interpret relevant Parts of the NCC and related Australian Standards for the project.
· Determine and document the classifications applicable to the building. (template available- HO1)
· Identify and interpret multiple classifications from NCC.
· Determine construction compliance requirements.
· Determine NCC Performance Requirements relevant to Class 2 to 9 Type C building projects.
· Determine range of criteria to ensure that construction methods comply with NCC Performance Requirements.
· Identify and document faults or non-conforming construction methods against NCC Performance Requirements. (template available- HO1) 
· Propose Performance Solution during discussion with design and building professional.
· Analyse and apply Assessment Methods to determine compliance with Performance Solution or Deem-to-Satisfy Solution (DTS). (template available- HO1)
· Meet the evidence of suitability requirements for building materials and products stated in the NCC.
· Complete documentation demonstrating how the project design and construction will meet NCC requirements (template available- HO1) including:
· Structure
· Access and egress
· Services and equipment
· Health and amenities
· Ancillary provisions
· Energy efficiency
· Determine fire protection requirements.
· Read the NCC and other legislative requirements for passive and active fire control elements in buildings.
· Write or obtain a checklist describing the level of fire resistance required for the construction of various buildings.
· Inspect one building for compliance with passive and active fire protection requirements.

These tasks may be simulated or real. The Participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. The Observer is to provide detailed comments on the tasks completed by the Participant (on the Observer Comments, overleaf). The Assessor is to verify the Observer’s comments, noting their findings in the Assessor Comments (on the back of the Practical Assessment cover page) and provide the assessment outcome.

	Resources required: 
Construction plans, drawings and specifications of two Type C building projects- one(1) Class 2, 3 or 9 and one (1) Class 5 to 8.; workplace quality policies and procedures; technology to access building and related industry codes, standards and manufacturer product information and materials specifications; Technology to access the NCC and current relevant Acts and Regulations. PPE as required. Documentation of design and construction (suitability or evidence of suitability) (template available- (HO1)). Fire protection checklist (HO2).

	Observer details

	Name of observer:
	Yanzhong Zhu

	Role of observer 
(Confirm suitability to sign)
	Builder

	Email address of observer
	steve.zhu.au@hotmail.com

	Signature of observer:
	
	Date:
	18/11/2023



	When completing the task, did the Participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	
	1st
Occasion
	2nd
Occasion

	1 Classify buildings.

	[bookmark: _Ref129077872]Read the plans and specifications to determine the nature of the building, its use and arrangement.
	þ	
	[bookmark: _Ref129077875]Read and correctly interpret relevant Parts of the NCC and related Australian Standards for the project.
	þ	
	[bookmark: _Ref129077878]Determine and document the classifications applicable to the building. (template available- HO1)
	þ	
	[bookmark: _Ref129077882]Identify and interpret multiple classifications from NCC.
	þ	
	2 Determine construction compliance requirements from NCC.

	[bookmark: _Ref129079891]Determine NCC Performance Requirements relevant to Class 2 to 9 Type C building projects.
· Occasion 1- Class 2, 3 or 9
· Occasion 2 - Class 5 to 8
	þ	
	[bookmark: _Ref129079900]Determine range of criteria to ensure that construction methods comply with NCC Performance Requirements.
	þ	
	[bookmark: _Ref129079909]Identify and document faults or non-conforming construction methods against NCC Performance Requirements. (template available- HO1) 
	þ	
	[bookmark: _Ref129078432]Propose Performance Solution during discussion with design and building professional. 
	þ	
	[bookmark: _Ref129079927]Analyse and apply Assessment Methods to determine compliance with Performance Solution or Deem-to-Satisfy Solution (DTS). (template available- HO1)
	þ	
	[bookmark: _Ref129079933]Meet the evidence of suitability requirements for building materials and products stated in the NCC.
	þ	
	[bookmark: _Ref129079940]Complete documentation demonstrating how the project design and construction will meet NCC requirements for structure. (template available- HO1)
	þ	
	[bookmark: _Ref129079955]Complete documentation demonstrating how the project design and construction will meet NCC requirements for access and egress. (template available- HO1)
	þ	
	[bookmark: _Ref129079957]Complete documentation demonstrating how the project design and construction will meet NCC requirements for services and equipment. (template available- HO1)
	þ	
	[bookmark: _Ref129079961]Complete documentation demonstrating how the project design and construction will meet NCC requirements for health and amenities. (template available- HO1)
	þ	
	[bookmark: _Ref129079963]Complete documentation demonstrating how the project design and construction will meet NCC requirements for ancillary provisions. (template available- HO1)
	þ	
	[bookmark: _Ref129079964]Complete documentation demonstrating how the project design and construction will meet NCC requirements for  energy efficiency. (template available- HO1)
	þ	
	[bookmark: _Ref129080153]Complete documentation demonstrating how the project design and construction will meet NCC requirements for fire protection. (template available- HO1)
	þ	
	3 Determine fire protection requirements.

	[bookmark: _Ref129079972]Read the NCC and other legislative requirements for passive and active fire control elements in buildings.
	þ	
	[bookmark: _Ref129079978]Write or obtain a checklist describing the level of fire resistance required for the construction of various buildings.
	¨	
	[bookmark: _Ref129078721]Inspect one building for compliance with passive and active fire protection requirements.
	þ	




	Observer comments:
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