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CPCCBC4014A 
Prepare simple building sketches and drawings


	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances. 
Answers will be documented and FT003 (Oral examination declaration form) must be completed.
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· If a participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a participant changes their response in writing, they must put their initials next to the written change.
· If a participant changes their response verbally, this must be noted on the exam paper by the assessor.
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	ASSESSOR COMMENTS

	


Identify three (3) two-dimensional drawings/sketches that may be used to clarify or communicate ideas to clients or other parties. For each drawing/sketch, identify four (4) key features that may be shown. 

	Answer
	Drawing/sketch type
	Key features
	
	
	Concept sketch
	Getting thoughts on paper
Planning any special or critical areas.
	

	
	Floor plans
	Layout / arrangement of the rooms
House interior
	

	
	Orthographic drawings
	Representing 3 D view on paper in 2D format
Ceiling and floors

	




[bookmark: _Ref1652804]Name two (2) advantages of a three-dimensional sketch/drawing. 

	Answer
	3D provides more realistic picture of space

They can be developed using different softwares
Gives understanding of the scale
	



[bookmark: _Ref1652809]Name one (1) individual you might contact to establish the scope and standard of the job being undertaken. 

	Answer
	Client, supervisor

	



[bookmark: _Ref1652872]You need to inspect the relevant area to take measurements for your drawings/sketches. Identify two (2) safety requirements you would need to observe on site. 

	Answer
	Induction and PPE

	



[bookmark: _Ref1629720]Identify two (2) types of tools/equipment you would use when inspecting the area to take measurements. 

	Answer
	Measuring wheel
Spirit level
	



[bookmark: _Ref1629725]Identify two (2) types of tools/equipment you might need when completing sketches/drawings. 

	Answer
	HB Pencil, rubber and bio.
Clip board and paper
Computer, digital camera
	



[bookmark: _Ref415490119]What action should be taken if any of the tools/equipment identified in Q5. and Q6. are found to be defective? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Report, Record
	

	
		Stop, Report, Record
	

	
		Stop, Tag, Report, Record
	

	
		Stop, Fix, Report, Record
	




[bookmark: _Ref875165]True or False (Tick your response): It is best practice to double check measurements before recording them.

	Answer
		True 
	
	
	
		False 
	
	



[bookmark: _Ref1653135]Explain the purpose of the scale on sketches/drawings. 

	Answer
	Buildings are drawn in proportion (reduce or enlarged) to the actual measurement of the object which is known as the scale of the drawing

If the drawing is 1:10 the object is drawn a tenth of its actual size.

	



[bookmark: _Ref1653139]You have measured a wall that is 2.4m high. Using a scale of 1:100, what size will this be drawn? Provide your answer in mm. Show your workings.

	Answer
	1 m = 1000 mm
2.4m = 2400 mm

Scale 1:100 means 2.4m (2400mm) high wall will be drawn 24 mm on drawing.
	



[bookmark: _Ref1653143]Explain the purpose of a key or legend on sketches/drawings. 

	Answer
	Key or legends explains the meaning of symbol used in sketches/drawings
	



[bookmark: _Ref1653145]Which of the following are true about drawing contours? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Equally spaced contour lines indicate uniform slope
	

	
		Closely spaced contour lines indicate flat surface
	

	
		Closely spaced contour lines indicate steep ground
	

	
		Concentric closed contours with decreasing values toward the centre indicate a pond
	

	
		Concentric closed contours with decreasing values toward the centre indicate a hill
	



[bookmark: _Ref427235149]Identify the Volume and Parts of the NCC that relate to metal sheet roof cladding for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Volume 2 and Part 3.5.1.0 – 3.5.5.0
	Volume 1 and Part B1.4 and F 1.5
	




[bookmark: _Ref531355745]Which Australian Standard is referenced in the NCC with regards to the requirements for the design and installation of metal sheet roof cladding?

	Answer
	AS1562
	



[bookmark: _Ref427733304]Sketch the following standard design symbols.

	Answer
	Item
	Sketch
	
	
	Compass (North)
		

	
	Sink with one bowl
		

	
	Stairs
		

	
	Toilet
		





[bookmark: _Ref427219196]Explain the meaning of the abbreviations in the table below.

	Answer
	Abbreviation
	Meaning
	
	
	BK
	Brick
	

	
	CBD / CPD
	Cupboard
	

	
	DP
	Down pipe
	

	
	INSUL
	Insulation
	

	
	KIT
	Kitchen
	

	
	MSB
	Main switch board
	

	
	PBD
	Plasterboard
	

	
	RWT
	Rain water tank
	

	
	SHR
	Shower
	

	
	TEL
	Telephone
	

	
	WC
	Water closet
	




[bookmark: _Ref1653550]True or False (Tick your response): The dashed/chain lines on the section view shown below represent the portions that have been in contact with the cutting plane. 

[image: ][image: ]

Source: https://www.mcvts.net/cms/lib/NJ01911694/Centricity/Domain/131/Section_Views.pdf

	Answer
		True 
	
	
	
		False 
	
	



[bookmark: _Ref1653558]Explain the use of hatching lines for sectional drawings.

	Answer
	Hatching lines are thin lines normally drawn 45 to the horizontal left or right. The hatching lines represent the material type in contact with the cutting plane, as illustrated by the key/legend.
	



[bookmark: _Ref1653570]True or False (Tick your response): In an offset sectional drawing, the cutting plane does not travel in a straight line.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref1653501]Which of the following information should be included in the title block for a sketch/drawing? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Client details
	

	
		Contact details for person who prepared drawings
	

	
		Date drawing was completed
	

	
		Drawing number
	

	
		Drawing title
	

	
		Job number
	

	
		Project name and address
	

	
		Revisions / Amendments (if applicable)
	

	
		Scale
	




[bookmark: _Ref1653504]True or False (Tick your response): Amendments usually have to be signed or initialled by both the builder and the client to show they both agree.

	Answer
		True 
	
	
	
		False 
	
	



[bookmark: _Ref1653930]Explain why it is good practice to have a single repository for sketches/drawings.

	Answer
	a reference or centre point to check that the sketches/drawings being used are the most current and approved. 

	



[bookmark: _Ref355889][bookmark: _Ref1653905]Name the Regulation and identify the section that outlines the requirement for structure designers to produce a safety report. 
Briefly describe the requirements. 

	Answer
	Section of Act
	Requirements
	
	
	NSW WHS Regulation 2017 Part 6.2 Section 295
	The designer of a structure or any part of a structure that is to be constructed must give the person conducting a business or undertaking who commissioned the design a written report that specifies the hazards relating to the design of the structure that, so far as the designer is reasonably aware:
(a)  
       create a risk to the health or safety of persons who are to carry out any construction work on the structure or part, and
(b)  
are associated only with the particular design and not with other designs of the same type of structure.
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