Incident investigation form


	Incident details

	Name of person involved in the incident: Joseph Blogs
	Date of incident: 23.01.2020

	Location of incident: 14th floor CBUS building 1 William Street Brisbane Q 4000

	Incident investigation team: Chris Tauri Acer Services Site Supervisor

	Robert Young Acer Services HSR
	Cullum Murray Multiplex WHSO

	Benjamin Dover Bright Spark Electrical HSR
	Shelly Shores Multiplex WHS Assistant

	What task was being performed at the time of the incident?

	Installing air-con ducting to the underside of the suspended slab

	What happened? (e.g. ‘employee tripped over box’ or ‘forklift hit wall’)

	Elevated work platform unexpectedly raised up crushing the operator between the handrail of the machine and the slab.

	What factors contributed to the incident?

	Environment:
	Equipment/materials:

	· Noise
	· Layout / design
	· Wrong equipment for the job
	· Equipment failure

	· Lighting
	· Dust / fume
	· Inadequate maintenance
	· Material / equipment too heavy / awkward

	· Vibration
	· Slip / trip hazard
	X Inadequate guarding
	· Inadequate training provided

	· Damaged / unstable floor
	· Other
	· Other

	Work systems:
	People:

	· Hazard not identified 
	· No / inadequate risk assessment conducted 
	X Procedure not followed / no procedure exists
	· Drugs / alcohol

	· No / inadequate safe work procedure 
	· No / inadequate controls implemented 
	· Fatigue
	· Time / production pressures

	· Hazard not reported 
	· Inadequate training / supervision 
	· Change of routine
	· Distraction / personal issues / stress 

	· Other
	· Lack of communication
	· Other

	Corrective actions:

	Contributing factor

(from above list)
	What are we going to do to fix the problem?
	Who
	When
	Completion date

	Standard Operating Procedure of machine was not followed.
	Re-training
	Robert Young
	30.03.2020
	1.04.2020

	Inadequate guarding
	Have approached plant supplier to address
	Robert Young

	30.03.2020
	ongoing

	
	
	
	
	

	
	
	
	
	


	Issue fixed? Yes

	Name
	Signature
	Date

	Person involved in incident: Joseph Blogs
	
	

	Manager: Jay Matsen (Acer Services)
	
	24.01.2020



Incident investigation process guide
1. Establish the facts of the incident, including:

· What happened?
· When and where did it happen?
· What task was being done?
· Who was involved?
· Were there any witnesses?

2. Gather all necessary background information, for example:

· maintenance records
· safe work procedures
· instructions manuals
· training records.

3. Consider all the potential contributing factors: 

· Environment: Did environmental conditions (e.g. light, noise, floor surfaces) contribute to the incident?
· Equipment /materials: Did anything about the equipment, materials, tools etc (e.g. equipment failures, missing guards) contribute to the incident?
· Work systems: Was there something about the system that contributed (e.g. hazard not identified, known hazard not addressed)?
· People: Was there something the workers, supervisors or contractors did that contributed to the incident (e.g. poor communication, being tired or rushing to finish on time)?
4. Determine the primary cause/s of the incident, that is, those which if they hadn’t occurred then the incident wouldn’t have occurred. Ask yourself “Would the incident have happened if….?”
5. Identify the root cause / system failures that underlie the primary cause/s and contributing factors. 
One simple technique for identifying the root cause is the ‘Five Whys’. This technique involves asking yourself ‘Why did this happen?’ and continuing to ask ‘Why’ for each response until you reach a conclusion that does not generate another ‘why’ and the underlying cause becomes apparent. 

6. The final and most import step in any investigation is to take action to fix all the factors that contributed to the incident, starting with the primary cause/s and working through each of the contributing and underlying causes.
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