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BSBOHS201A 
Participate in OHS processes
ASSESSMENT SUMMARY

The assessment activities for BSBOHS201A Participate in OHS processes cover all aspects of the unit of competency required. To demonstrate competence in this unit, a participant must undertake all tasks and complete them satisfactorily and consistently. For Apprentices and Trainees, this includes employer completion of the Employer Record Book (ERB). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be equitable, fair and flexible. If a participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a participant does not answer some questions or perform some tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. The Trainer/Assessor is able to provide the participant with additional information on interpreting the assessment outcomes and provide guidance on the participant’s options. Should a participant still be deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result. 

By signing the cover page for each assessment item, the participant acknowledges they understand the assessment instructions and requirements and consent to being assessed. The participant also verifies and assures the RTO that the work submitted is their own work. 


	Participant Name
	




	Task
	Assessment Results 

	Theory Exam
	 Satisfactory 
	 Not Yet Satisfactory

	Practical Assessment
	 Satisfactory 
	 Not Yet Satisfactory

	Outcome for Unit of Competency
	 Competent
	 Not Yet Competent




	Assessor Name
	

	Assessor Signature
	
	Unit Competence Determination Date
	Click here to enter a date.
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BSBOHS201A 
Participate in OHS processes

	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances, whereby the Participant’s answers will be documented by a party other than the Participant. This must be acknowledged in writing (e.g. FT001 and Assessor Comments)
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· Assessors are to complete marking in pen of a different colour to the Participant.
· If a Participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a Participant changes their response in writing, they must put their initials next to the written change.
· If a Participant changes their response verbally, this must be noted on the exam paper by the assessor.




	Participant name
	JIE DONG

	
	

	Participant signature
	
	
	

	Date
	3/07/2021



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.




	Number of questions
	Number of questions answered correctly
	Task outcome (Tick)

	24
	
	Satisfactory
	Not Yet Satisfactory

	
	
	
	


	ASSESSOR COMMENTS

	


Match the terms and definitions by writing the appropriate letter next to each number in the centre column.

	Answer
	Terms
	Answers
	Definition
	
	
	1
	PRA
	1 - F
	A
	Outline the requirements of the work to be undertaken.
	

	
	2
	JSA
	2 - E
	B
	Outline what to do in the event of fires and other accidents
	

	
	3
	Plans and specifications
	3 - A
	C
	Contains important information about hazardous materials or chemicals.
	

	
	4
	Manufacturer specifications
	4 - D
	D
	Outlines how tools and equipment should be used (e.g. lubricant levels, maintenance requirements).
	

	
	5
	SDS
	5 - C
	E
	Identifies hazards and potential hazards that may be encountered while working.
	

	
	6
	Emergency procedures
	6 - B
	F
	A personal assessment of risk
	




[bookmark: _Ref424210309][bookmark: _Ref412796746]For each of the hazards identified below, describe the injuries/damage they may cause (i.e. to fellow workers, other people and/or animals) and suggest a suitable control measure.

	Answer
	Hazard
	Injuries or damage
	Control measure
	
	
	Hazardous chemical
	Respiratory damage, skin rashes, chemical burns
	Firstly, once this hazard is recognised, it should be reported immediately to my supervisor, site/project manager or Health&Safety representative, using the report form supplied by my organisation. Secondly, following control measures: Changing process to minimize contact with hazardous chemicals; Isolating or enclosing the process; Use of wet methods to reduce generation of dusts or other particulates; General dilution ventilation; Using fume hoods. Finally, implementing the hierarchy of control: Eliminating the hazard, Substituting the hazard, Isolating the hazard, Control the hazard by engineering means, Control the hazard by administrative means and Providing & using Personal Protective Equipment (PPE)
	

	
	Noise
	Hearing damage, headaches, fatigue
	Firstly, once this hazard is recognised, it should be reported immediately to my supervisor, site/project manager or Health&Safety representative, using the report form supplied by my organisation. Secondly, following control measures: Elimination, removing the source of the noise completely; Substitution, employing alternate construction techniques; Isolation; Equipment selection; Engineering Controls; Quiet work practices; Administrative control. Finally, implementing the hierarchy of control: Eliminating the hazard, Substituting the hazard, Isolating the hazard, Control the hazard by engineering means, Control the hazard by administrative means and Providing & using Personal Protective Equipment (PPE) 
	

	
	Manual handling
	Strains, sprains
	Firstly, once this hazard is recognised, it should be reported immediately to my supervisor, site/project manager or Health&Safety representative, using the report form supplied by my organisation. Secondly, following control measures: Avoiding the need for manual handling; reducing the load risk by using lighter weights or more stable containers; reorganising the activity or environment to further reduce the impact on the individual(s); utilising mechanical lifting aids or equipment.  Finally, implementing the hierarchy of control: Eliminating the hazard, Substituting the hazard, Isolating the hazard, Control the hazard by engineering means, Control the hazard by administrative means and Providing & using Personal Protective Equipment (PPE) 
	




[bookmark: _Ref415045277]Who should you speak to if you find problems (e.g. hazards, accidents and emergencies)?

	Answer
	I should speak immediately t my supervisor, site/project manager or Health & Safety Representative
	


[bookmark: _Ref406591713]What action should be taken if plant, tools and/or equipment are found to be defective? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Report, Record
	

	
		Stop, Report, Record
	

	
		Stop, Tag, Report, Record
	

	
		Stop, Fix, Report, Record
	




[bookmark: _Ref424211517]Which legislation relates to safety in the workplace? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Occupational Health and Safety Act 2015 
	

	
		Work Health and Safety Act 2011 
	

	
		Safety Act 1900 
	

	
		Safety and Health Act 2011 
	




[bookmark: _Ref424211632]True or False (Tick your response): Employers are required by legislation to implement safety measures which are reasonably practicable.

	Answer
		True 
	
	
	
		False 
	
	




[bookmark: _Ref424211634]True or False (Tick your response): Workers are required by legislation to follow reasonable employer directives (e.g. to undertake first aid and/or fire safety training).

	Answer
		True 
	
	
	
		False 
	
	





[bookmark: _Ref424213216]The following symbols appear under the heading ‘Required PPE’ on an SDS. What do the symbols represent?

	Answer
	Symbol
	Meaning
	
	
	
[image: ]

	PROTECTIVE CLOTHING REQUIRED/OVERALLS MUST BE WORN
	

	
	
[image: ]

	SAFETY GLOVES REQUIRED/HAND PROTECTION MUST BE WORN 
	

	
	
[image: ]

	GOGGLES REQUIRED/EYE PROTECTION MUST BE WORN 
	

	
	
[image: ]

	RESPIRATOR REQUIRED/BREATHING PROTECTION MUST BE WORN 
	




[bookmark: _Ref408209094]Describe the meaning and use of the signs displayed below.

	Answer
	Sign
	Meaning
	
	
	[image: First aid.jpg]
	Location of First Aid Kit
	

	
	[image: Do Not Enter Saftety Sign]
	Warns off unauthorised persons from entering area
	

	
	[image: https://encrypted-tbn3.gstatic.com/images?q=tbn:ANd9GcRfZQGVU3BvP46nBERPIeqexiKuKX8OHW4dEmTYE6j-oAKUgPPkHw]
	Location of Fire Fighting Facilities
	





Refer to the Risk Matrix below when responding to Q10. to Q12. 

	Matrix
	A:
Death or permanent disability
	B:
Serious injury
	C:
Lost time injury
	D:
Casualty Treatment
	E:
First Aid

	1: Very Likely
	E
	E
	H
	H
	M

	2: Likely
	E
	H
	H
	M
	M

	3: Possible
	H
	H
	M
	M
	L

	4: Unlikely
	H
	M
	M
	L
	L

	5: Very Unlikely
	M
	M
	L
	L
	L



	E: Extreme
	H: High
	M: Medium
	L: Low




[bookmark: _Ref408921283]Which rating is designated for the highest risk and which rating is used for the lowest risk?

	Answer
	Highest Risk:  E: Extreme in red color (1. Very Likely + Consequence A) – Left top corner.
Lowest Risk:   L: Low in green color (5. Very Unlikely + Consequence E – Right bottom corner

	



[bookmark: _Ref408921265]What is the risk rating for the following circumstances: An event which is possible and would require low-level hospital treatment.

	Answer
	M: Medium in yellow color - (3. Possible + Consequence D)
	



[bookmark: _Ref408921287][bookmark: _Ref412797660]What are the factors that would lead to a risk rating of E: Extreme?

	Answer
	Risk is measured in terms of the seriousness of the possible consequences of the hazard and the likelihood that those consequences will occur. Therefore, the most serious consequence of the hazard and the highest likelihood that the consequence occurred would lead to the E: Extreme risk rating in the Risk Matrix  
	



[bookmark: _Ref424212548]When should safety checks be undertaken on machinery and equipment? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Before operation
	

	
		After operation
	

	
		Both before and after operation
	



[bookmark: _Ref408921427]Order the elements of the hierarchy of control, from 1 to 6 (i.e. most effective to least effective).


	Answer
	Label (1 – 6)
	Element
	
	
	3
	Isolate the hazard
	

	
	6
	Provide and use Personal Protective Equipment (PPE)
	

	
	1
	Eliminate the hazard
	

	
	4
	Control the hazard by engineering means
	

	
	5
	Control the hazard by administrative means
	

	
	2
	Substitute the hazard
	




[bookmark: _Ref408921430]Why is elimination the best method of hazard control and PPE considered the least effective?

	Answer
	Elimination is the process of physical removing the hazard or getting rid of the hazard from the workplace. It is the most effective way to control a risk because the hazard is no longer present. It is the preferred way to control a hazard and should be used whenever possible.
PPE does not control the hazard at the source. It only replies on human behaviour and supervision and, used on their own, tend to be least effective in minimising risks. It does not eliminate the hazard and will present the wearer with the maximum health risk if the equipment fails.
	



[bookmark: _Ref408921432]If you were to replace a flammable solvent with a water-based solvent, what category of control measure would that be under the hierarchy of control?

	Answer
	It is the 2nd category of control measure – “Substitute the hazard”
	


[bookmark: _Ref401921251][bookmark: _Ref401900343]

[bookmark: _Ref401922320]In the diagram below a person is lifting a tool box.
Filling in the table, indicate how each body part should be used/placed. 
[image: lifting]F. Hands
E. Knees
D. Shoulders
C. Feet
B. Back
A. Neck

	Answer
	Area of body (Letter)
	How it should be placed
	
	
	D
	Level
	

	
	A
	Upright
	

	
	F
	Good grip
	

	
	B
	Natural curve
	

	
	E
	Bent
	

	
	C
	Flat, facing load
	




[bookmark: _Ref415049799][bookmark: _Ref421093133]In a medical emergency, what is the first step in the DRSABCD action plan that you need to follow?

	Answer
	Danger checked. Check for any danger in the immediate vicinity.
	



[bookmark: _Ref421092991]In the event of a fire emergency, what should you do? 
Fill in the table below to explain the acronym R.A.C.E.

	Answer
	Letter
	Meaning
	
	
	R
	Remove people from immediate danger
	

	
	A
	Alert people of emergency
	

	
	C
	Confine fire and smoke
	

	
	E
	Evacuate to the assembly area
	



[bookmark: _Ref414952615]What should you do as part of the clean up process? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Store all plant, tools and equipment without cleaning
	

	
		Maintain plant, tools and equipment
	

	
		Dispose of materials that cannot be reused or recycled
	

	
		Report faults in logbook and/or site records
	

	
		Clean all plant, tools and equipment before storage
	




[bookmark: _Ref408921186]Read the scenario below and complete the Hazard Report Form.

SCENARIO
Today at 10:45am a delivery truck reversed into a car park (located at 54 Standish Street, Salisbury) to deliver gardening materials. There was nobody in the car park to guide the driver and he backed into a number of drums of diesel located to the left of the photograph (below).  One drum was pierced and its contents erupted from the container. 

The marked area on the photo represents the diesel spill, measuring 3m x 4m.











HAZARD REPORT FORM

	GENERAL

	Date
	10:45am on 3rd July 2021

	Submitted by
	JIE DONG

	HAZARD DETAILS

	Location
	A Car Part located at 54 Standish Street, Salisbury, QLD 4107

	Description of issue
	A delivery truck for gardening materials reversed into the car park located at 54 Standish St, Salisbury Qld 4107 at 10:45am today on 3rd July 2021. As there was nobody in the car park to guide the driver and he backed into a number of drums of diesel located to the left of the photograph – please find the picture in the attached. One drum was pierced, and its contents erupted from the container. The marked area of the diesel spillages is measuring 3m x 4m. 

	Risk class
	  Extreme
	  High
	  Medium
	  Low

	CONTROL MEASURES

	Corrective action required 
	Action 1: reporting this issue immediately to the car park owner. If the car park is public, then ringing Brisbane City Council immediately to report this issue. Action 2: trying to stop the spill. finding properly qualified and equipped personal should safely stop the leak or spill of the diesel as soon as possible. Action 3, containing and recovering the spill. If the spill or leak cannot be stopped, catching the flowing liquid using whatever is available. Action 4, using barrier systems (eg: water filled barrier system) and warning signs to surround the spill area to avoid any person walks by to enter the spill area. Action 5, extinguishing any open flames in the spill area of the diesel fuel. Action 6, Removing the rest of drums of diesel to the safe area. This accident has showed that the current location to keep those drums of diesel is very dangerous and the current storage location leads to this hazard easily. Action 7, the police and fire service may also need to be involved if those above actions cannot be taken completely to stop the diesel spill 

	Person to action
	Car park owner, Brisbane City Council (if it is a public car parking), Truck driver
	When
	  Immediately
  Within 24 hours
  Within 7 days



	Answer
	
	


[bookmark: _Ref412803069]Who would you submit a hazard report form to?

	Answer
	Car Park Owner, Brisbane City Council, Police, Fire Services
	



[bookmark: _Ref412803089]Who would approve proposed risk controls and organise the required resources for implementation of the risk control?

	Answer
	Brisbane City Council, Police, Fire Services, Car Park Owner
	



[bookmark: _Ref424215038]Identify one (1) way you can assess if risk controls have been effective.

	Answer
	Cleaning all spilled diesel and removing the rest of drums of diesel to the safe and proper storge areas 
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