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ASSESSMENT SUMMARY

The assessment activities for CPCCBC4014A Prepare simple building sketches and drawings cover all aspects of the unit of competency required. To demonstrate competence in this unit, a participant must undertake all tasks and complete them satisfactorily and consistently. For Apprentices and Trainees, this includes employer completion of the Employer Record Book (ERB). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be equitable, fair and flexible. If a participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a participant does not answer some questions or perform some tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. The Trainer/Assessor is able to provide the participant with additional information on interpreting the assessment outcomes and provide guidance on the participant’s options. Should a participant still be deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result. 

By signing the cover page for each assessment item, the participant acknowledges they understand the assessment instructions and requirements and consent to being assessed. The participant also verifies and assures the RTO that the work submitted is their own work. 


	Participant Name
	




	Task
	Assessment Results 

	Theory Exam
	 Satisfactory 
	 Not Yet Satisfactory

	Practical Assessment
	 Satisfactory 
	 Not Yet Satisfactory

	Outcome for Unit of Competency
	 Competent
	 Not Yet Competent




	Assessor Name
	

	Assessor Signature
	
	Unit Competence Determination Date
	Click here to enter a date.
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	THEORY EXAM INSTRUCTIONS

· This exam will occur under standard assessment conditions.
· An oral examination may be allowed under certain circumstances, whereby the Participant’s answers will be documented by a party other than the Participant. This must be acknowledged in writing (e.g. FT001 and Assessor Comments)
· Participants must provide enough detail in their responses to demonstrate their knowledge and skills.
· Please fill in the details below, providing your name, signature and date of assessment.
· Your signature acknowledges that this is your own work.
· Assessors are to complete marking in pen of a different colour to the Participant.
· If a Participant initially answers a question incorrectly but modifies their response, they must follow the instructions below:
· If a Participant changes their response in writing, they must put their initials next to the written change.
· If a Participant changes their response verbally, this must be noted on the exam paper by the assessor.




	Participant name
	Carly Dyson

	
	

	Participant signature
	
	
	

	Date
	7/06/2021



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.




	Number of questions
	Number of questions answered correctly
	Task outcome (Tick)

	23
	
	Satisfactory
	Not Yet Satisfactory

	
	
	
	


	ASSESSOR COMMENTS

	


Q1.  Identify three (3) two-dimensional drawings/sketches that may be used to clarify or communicate ideas to clients or other parties. For each drawing/sketch, identify four (4) key features that may be shown. 

	Answer
	Drawing/sketch type
	Key features
	
	
	Floor Plan
	Relationship between rooms
Spaces and features viewed from above
Room dimensions
Door and window dimensions

	

	
	Sectional View
	Vertical view through the middle of structure
Material weights / dimensions for internal structure
Material types to be used
Visibility of how to assemble internal structure

	

	
	Land boundary / Contour Plan
	Boundaries
Levels of property
Adjoining properties
Position of proposed building on property
	




Q2.  [bookmark: _Ref1652804]Name two (2) advantages of a three-dimensional sketch/drawing. 

	Answer
	Provide a more realistic picture of space
Improves accuracy

	



Q3.  [bookmark: _Ref1652809]Name one (1) individual you might contact to establish the scope and standard of the job being undertaken. 

	Answer
	Client
	



Q4.  [bookmark: _Ref1652872]You need to inspect the relevant area to take measurements for your drawings/sketches. Identify two (2) safety requirements you would need to observe on site. 

	Answer
	Relevant PPE

	



Q5.  [bookmark: _Ref1629720]Identify two (2) types of tools/equipment you would use when inspecting the area to take measurements. 

	Answer
	Spirit level
Gradient of digital level
	



Q6.  [bookmark: _Ref1629725]Identify two (2) types of tools/equipment you might need when completing sketches/drawings. 

	Answer
	Pencils
Rubber
	



Q7.  [bookmark: _Ref415490119]What action should be taken if any of the tools/equipment identified in Q5. and Q6. are found to be defective? Tick your response.

	Answer
	Choice
	Possible Answers
	
	
		Report, Record
	

	
		Stop, Report, Record
	

	
		Stop, Tag, Report, Record
	

	
		Stop, Fix, Report, Record
	




Q8.  [bookmark: _Ref875165]True or False (Tick your response): It is best practice to double check measurements before recording them.

	Answer
		True 
	
	
	
		False 
	
	



Q9.  [bookmark: _Ref1653135]Explain the purpose of the scale on sketches/drawings. 

	Answer
	Scale allows an understanding of the relationship between a drawing and reality. Scale shows that relative sizes are correctly represented. 
	



Q10.  [bookmark: _Ref1653139]You have measured a wall that is 2.4m high. Using a scale of 1:100, what size will this be drawn? Provide your answer in mm. Show your workings.

	Answer
	2.4m = 240cm = 2400mm
2400mm / 100 = 24mm
The wall would be drawn as 24mm
	



Q11.  [bookmark: _Ref1653143]Explain the purpose of a key or legend on sketches/drawings. 

	Answer
	To identify symbols and abbreviations used
	



Q12.  [bookmark: _Ref1653145]Which of the following are true about drawing contours? 
Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Equally spaced contour lines indicate uniform slope
	

	
		Closely spaced contour lines indicate flat surface
	

	
		Closely spaced contour lines indicate steep ground
	

	
		Concentric closed contours with decreasing values toward the centre indicate a pond
	

	
		Concentric closed contours with decreasing values toward the centre indicate a hill
	



Q13.  [bookmark: _Ref427235149]Identify the Volume and Parts of the NCC that relate to metal sheet roof cladding for Classes 1 and 10, and Classes 2 to 9.

	Answer
	Classes 1 and 10
	Classes 2 to 9
	
	
	Volume 2 
Part 3.5
	Volume 2 
Part 3.5
	




Q14.  [bookmark: _Ref531355745]Which Australian Standard is referenced in the NCC with regards to the requirements for the design and installation of metal sheet roof cladding?

	Answer
	AS1562.1:
	



Q15.  [bookmark: _Ref427733304]Sketch the following standard design symbols.

	Answer
	Item
	Sketch
	
	
	Compass (North)
		

	
	Sink with one bowl
		

	
	Stairs
		

	
	Toilet
		





Q16.  [bookmark: _Ref427219196]Explain the meaning of the abbreviations in the table below.

	Answer
	Abbreviation
	Meaning
	
	
	BK
	Brick
	

	
	CBD / CPD
	Cupboard
	

	
	DP
	Downpipe
	

	
	INSUL
	Insulation
	

	
	KIT
	Kitchen
	

	
	MSB
	Main Switchboard
	

	
	PBD
	Plasterboard
	

	
	RWT
	Rain Water Tank
	

	
	SHR
	Shower
	

	
	TEL
	Telephone
	

	
	WC
	Water Closet
	




Q17.  [bookmark: _Ref1653550]True or False (Tick your response): The dashed/chain lines on the section view shown below represent the portions that have been in contact with the cutting plane. 

[image: ][image: ]

Source: https://www.mcvts.net/cms/lib/NJ01911694/Centricity/Domain/131/Section_Views.pdf

	Answer
		True 
	
	
	
		False 
	
	



Q18.  [bookmark: _Ref1653558]Explain the use of hatching lines for sectional drawings.

	Answer
	Hatching lines represent the material type in contact with the cutting plane
	



Q19.  [bookmark: _Ref1653570]True or False (Tick your response): In an offset sectional drawing, the cutting plane does not travel in a straight line.

	Answer
		True 
	
	
	
		False 
	
	




Q20.  [bookmark: _Ref1653501]Which of the following information should be included in the title block for a sketch/drawing? Tick all that apply.

	Answer
	Choice
	Possible Answers
	
	
		Client details
	

	
		Contact details for person who prepared drawings
	

	
		Date drawing was completed
	

	
		Drawing number
	

	
		Drawing title
	

	
		Job number
	

	
		Project name and address
	

	
		Revisions / Amendments (if applicable)
	

	
		Scale
	




Q21.  [bookmark: _Ref1653504]True or False (Tick your response): Amendments usually have to be signed or initialled by both the builder and the client to show they both agree.

	Answer
		True 
	
	
	
		False 
	
	



Q22.  [bookmark: _Ref1653930]Explain why it is good practice to have a single repository for sketches/drawings.

	Answer
	To ensure that records are kept current and the most recent version is available.
	



Q23.  [bookmark: _Ref355889][bookmark: _Ref1653905]Name the Regulation and identify the section that outlines the requirement for structure designers to produce a safety report. 
Briefly describe the requirements. 

	Answer
	Section of Act
	Requirements
	
	
	Work Health and Safety Act  
Section 22
	The designer must give adequate information to each person who is provided with the design for the purpose of giving effect to it concerning— 
(a) each purpose for which the plant, substance or structure was designed; and 
(b) the results of any calculations, analysis, testing or examination mentioned in subsection (3), including, in relation to a substance, any hazardous properties of the substance identified by testing; and 
(c) any conditions necessary to ensure that the plant, substance or structure is without risks to health and safety when used for a purpose for which it was designed or when carrying out any activity mentioned in subsection (2)(a) to (e)
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	PRACTICAL ASSESSMENT INSTRUCTIONS

· The following practical assessment will require the Participant to complete work related activities.
· The Assessor will conduct observations of the Participant’s work to determine whether they display sufficient practical skills and knowledge. 
· Please fill in the details below – providing your name, signature and date of assessment.
· The Participant’s signature acknowledges that the Assessor provided clear instructions and the Participant understood what was required to complete this assessment.
· The Assessor may substitute a Practical Task with an alternate task of equal value.
· Alternate tasks must be fully documented by the assessor in the Assessor Comments area.





	Participant name
	

	
	

	Participant signature
	
	
	

	Date
	Click here to enter a date.



	Assessor name
	

	
	

	Assessor signature
	
	
	

	Date
	Click here to enter a date.





	Task
	Task outcome (Tick)

	
	Satisfactory
	Not Yet Satisfactory

	Task 1 (Occasion 1)
		
	Task 1 (Occasion 2)
		



	ASSESSOR COMMENTS

	


CPCCBC4014A
Prepare simple building sketches and drawings

	Practical Task 1 (2X)

	Description of task:
On two (2) occasions, a suitable observer is to verify the participant’s ability to produce sketches and drawings for a small work project (Note: The participant is not required to demonstrate complex drafting skills). Sketches and drawings may be simplified versions taken from architectural drawings, designed to capture design concepts or options. They may be used for estimating purposes and to show measurements and other requirements for building and construction works. Standard drawing conventions and features must be implemented (including direction, scale, key, contours, symbols and abbreviations). 

The participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. Evidence to be submitted may include: 
· Building sketches from projects the candidate has worked on

The observer is to provide detailed comments on the tasks completed by the participant. The assessor is to verify the observer’s comments in the Assessor Comments section, and provide the Practical Assessment outcome on the front cover of this document.

	Resources required: 
Computer, digital camera, pen and paper.

	Assessment of task

	Name of participant:
	

	Name of observer:
	

	Role of observer 
(Confirm suitability to sign)
	

	Email address of observer
	

	Signature of observer:
	
	Date:
	Click here to enter a date.
	When completing the task, did the participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	
	1st
Occasion
	2nd
Occasion

	1.A.  [bookmark: _Ref1568136]Identify and record types of drawings required and key features, in compliance with the cope and standard of the job. 
		
	1.B.  [bookmark: _Ref1568169]Identify and follow WHS requirements on site and statutory/authority requirements. 
		
	1.C.  [bookmark: _Ref1568174]Gather and check tools and equipment required for inspection, measurement and producing drawings. 
		
	1.D.  [bookmark: _Ref1568177]Inspect relevant area, taking and recording required measurements. 
		
	1.E.  [bookmark: _Ref1568181]Create simple 2D and 3D sketches and drawings, using standard drawing conventions and incorporating relevant codes and standards.
		
	1.F.  [bookmark: _Ref1568184]Create sectional drawings of simple structural elements, using standard drawing conventions. 
		
	1.G.  [bookmark: _Ref1568188]Record essential information on the drawings with symbols and abbreviations, according to standard drawing conventions.
		
	1.H.  [bookmark: _Ref1568191]Label, date and process drawings according to organisational administration and quality procedures. 
		
	1.I.  [bookmark: _Ref1568436]Effectively communicate using the following methods:
· Using language/concepts appropriate to cultural differences
· Non-verbal communication 
		
	The participant’s performance was:  Satisfactory     Not Satisfactory



	OBSERVER COMMENTS

	





CSTC Pty Ltd_RTO#0699_v1-3_02/10/2019	Page 3 of 4
image2.jpg




image3.jpg
W




image4.jpg
|





image5.jpg




image6.jpg




image7.png




image8.png




image1.png




