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RISK REGISTER
	Record number
	Date of entry
	Hazard
	Location
	People exposed
	Possible injuries/ damage
	Control measures
	Risk assessment

	1
	14/02/2022
	Mobile plant collision with persons
	Site entry - Gate 1
	Workers, visitors, pedestrians 
	· Bruising
· Fractures
· Sprains
· Lacerations 
· Permanent impairment
· Crushing injuries
· Death
	· Spotter
· Exclusion zones
· Close sidewalk and provide alternative walkway for pedestrians
· Install “Watch for trucks” signage
· Vehicle Movement plan displayed & communicated during inductions
· Traffic control 
	Inherent Risk – High

Residual Risk - Low

	2
	16/02/2022
	Objects falling off scaffold onto workers below
	Perimeter scaffold
	Workers, visitors, pedestrians
	· Head injuries
· Bruising
· Fractures  
· Lacerations
· Damage to equipment & vehicles
	· Designated PPE free zones (site compound)
· Wrap scaffold in containment screening 
· Weekly formal inspections of scaffold
· Daily informal inspections of scaffold (general walk of the scaffold to identify gaps in containment screening)
· Store all objects in the centre of the deck/structure
· Exclusion zones
· Tether tools

	Inherent Risk – High

Residual Risk - Low



RISK MATRIX
	Matrix
	A:
Death or permanent disability
	B:
Serious injury
	C:
Lost time injury
	D:
Casualty Treatment
	E:
First Aid

	1: Very Likely
	E
	E
	H
	H
	M

	2: Likely
	E
	H
	H
	M
	M

	3: Possible
	H
	H
	M
	M
	L

	4: Unlikely
	H
	M
	M
	L
	L

	5: Very Unlikely
	M
	M
	L
	L
	L



	E: Extreme
	H: High
	M: Medium
	L: Low
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