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	EMERGENCY RESPONSE, FIRST AID AND EMERGENCY EQUIPMENT RISK ASSESSMENT



	Project Name:
	Rockpool Pelican Waters

	Date of Assessment
	13/09/2022
	Job No:
	22065

	Assessed by:
	

	
	Clinton Guest

	
	



EMERGENCY RESPONSE REQUIREMENTS
The following emergency response requirements have been assessed as applicable for this site.

Applicable emergency responses shall be made relevant for the activities being undertaken on this site considering the high risk activities as identified in the Project Risk Assessment.
	Ref
	Category

	1
	Evacuate workplace

	2
	Unplanned fire event at 

	3
	First aid treatment

	4
	
Medical Assistance

	5
	Electric Shock

	6
	Substance Spill

	7
	Bomb threat

	8
	Explosion

	9
	Severe storm

	10
	Mobile plant rollover

	11
	Non responsive tower crane operator

	12
	First aid box retrieval

	13
	EWP or arrested fall retrieval

	14
	Collapsed structure 

	
	Mobile plant collision



FIRST AID KITS
The following table shall be used in determining the type of kit(s) to be supplied for the project:

	Assessment Factors
	Comments

	Size and Layout of the workplace
	4000 M2

	Nature of Hazards and Severity of Risks
	High Risk Work Site

	Max distance to First Aid
	24m vertically -100m max 

	Ambulance Access
	Located at project entrance

	Patient retrieval
	Stretcher via scaffold – Vertical stretcher (lift shaft)

	Number and Distribution of Employees on site
	95 Max

	Shifts / Overtime worked
	Single shifts - 6:30am – 600pm, 6 day weeks

	Are any Employees Isolated?
	Crane operator

	Can members of the public be involved?
	Yes - During plant access and exit to site, Scaffold erection, crane erection

	Location of the Workplace
	90 Spitfire Banks Drive, Pelican Waters

	Nearest Hospital:
	Caloundra Hospital – 5.6KM – 10 Minutes

	Nearest Medical Centre:
Include opening / closing times and coverage outside of these times.
	OCHRE Medical Centre Caloundra – 6.1KM – 11 Min 

	Time to Medical Service
	11 minutes

	Stretcher Required?
	Yes

	First Aid Room needed?
	Yes

	Number of First Aiders needed?
	4 plus subcontractor first aid assistant

	Level of first Aider required?
	Occupational First Aid



Based upon the above assessment, the following F.A. kit type is required: 
One McNab type C kit x 30 workers – Max numbers 95 workers and a total of 4 kits located strategically i.e. first aid room, hoist & every third level 

Depending on job progression and projected numbers. Preempting of site numbers to be monitored and first aid provisions provided.

	TYPE A (REMOTE)
	
	TYPE  B (LARGE)
	
	TYPE C (MEDIUM)
	
	TYPE D (SMALL)
	



Based upon the type of activities undertaken, specify any additional requirements in addition to the minimum kit quantities:

	ITEM
	TYPE A
REMOTE
	TYPE B
LARGE
	TYPE C
MEDIUM
	TYPE D
SMALL

	
	MIN. STOCK LEVEL
	STOCK REQD
	MIN. STOCK LEVEL
	STOCK REQD
	MIN. STOCK LEVEL
	STOCK REQD
	MIN. STOCK LEVEL
	STOCK REQD

	BASE-LINE KIT ITEMS 
	
	
	
	
	
	
	
	

	First Aid Treatment Report 
	!
	
	1
	
	3
	
	1
	

	Basic First Aid Notes/Pamphlet 
	1
	
	1
	
	1
	
	1
	

	Notepad & Pencil 
	1
	
	1
	
	1
	
	1
	

	Sterile eye pads 
	5
	
	5
	
	3
	
	0
	

	Adhesive dressing strips (Bandaids) 
	100
	
	100
	
	50
	
	50
	

	Non-Adherent Sterile Wound Covering -7.5x10cm  
	2
	
	5
	
	2
	
	0
	

	Non-Adherent Sterile Wound Covering -5x7cm 
	2
	
	5
	
	2
	
	0
	

	Triangular Bandages 
	5
	
	8
	
	4
	
	1
	

	Assorted Safety pins (pkt 12, various sizes) 
	1
	
	1
	
	1
	
	1
	

	Small sterile un-medicated wound dressing (#13) 
	3
	
	3
	
	1
	
	0
	

	Medium sterile un-medicated wound dressing (#14) 
	3
	
	3
	
	1
	
	0
	

	Large sterile un-medicated wound dressing (#15) 
	3
	
	8
	
	4
	
	1
	

	Adhesive dressing tape, 25mm 
	1
	
	1
	
	1
	
	1
	

	Crepe Bandages 
	
	
	
	
	
	
	
	

	Crepe Bandages (7.5cm) 
	2
	
	2
	
	1
	
	1
	

	Crepe Bandages (10cm) 
	2
	
	2
	
	1
	
	1
	

	Gauze Bandages: 
	
	
	
	
	
	
	
	

	- 5cm 
	3
	
	3
	
	1
	
	1
	

	- 10cm 
	3
	
	3
	
	1
	
	2
	

	Disposable Gloves (pairs) 
	5
	
	5
	
	3
	
	0
	

	Safety Glasses 
	1
	
	1
	
	1
	
	0
	

	Magnifying glass
	1
	
	0
	
	0
	
	0
	

	Forceps (Blunt/ Pointed)
	2
	
	0
	
	0
	
	0
	

	Scissors, blunt nosed 
	1
	
	1
	
	1
	
	1
	

	Antiseptic (alcohol prep) swabs, Pkt of 10 (eg: Mediprep) 
	1
	
	1
	
	1
	
	0
	

	Eye wash, Saline single use ampoules 
	5
	
	5
	
	3
	
	1
	

	Disposable Resuscitation  Face-shield 
	1
	
	1
	
	1
	
	0
	

	Rescue Blanket, Silver space 
	1
	
	1
	
	1
	
	0
	

	Plastic Bags that can be sealed, for amputated parts: 
	
	
	
	
	
	
	
	

	- Medium 
	2
	
	2
	
	1
	
	1
	

	- Large 
	2
	
	2
	
	1
	
	1
	

	Basic Dressing Pack 
	2
	
	2
	
	1
	
	0
	

	EYE MODULE
	
	
	
	
	
	
	
	

	Guidance Note - eye injuries 
	1
	
	1
	
	1
	
	0
	

	Once only use container - eye wash 
	2
	
	2
	
	1
	
	0
	

	Additional sterile eye pads 
	3
	
	3
	
	1
	
	0
	

	Additional adhesive tape 
	1
	
	1
	
	1
	
	0
	

	BURNS MODULE
	
	
	
	
	
	
	
	

	Guidance Notes - burn injuries 
	1
	
	1
	
	1
	
	0
	

	Assorted size burns dressings 
	5
	
	5
	
	2
	
	0
	

	Clean Sheeting (for covering burns) 
	1
	
	1
	
	1
	
	0
	

	Burn Gel (Med)
	1
	
	0
	
	0
	
	0
	

	REMOTE LOCATIONS MODULE
	
	
	
	
	
	
	
	

	Emergency Reference manual 
	1
	
	1
	
	1
	
	0
	

	10cm crepe bandages (for snake bites) 
	4
	
	4
	
	2
	
	0
	

	Non-Adherent Sterile Wound Covering -7.5x10 (pack 100) 
	1
	
	0
	
	0
	
	0
	

	 Resuscitation  Face-shield ( O2 compatible)
	1
	
	0
	
	0
	
	0
	

	Torch / flashlight 
	1
	
	1
	
	1
	
	0
	

	Sharps Container 
	1
	
	1
	
	0
	
	0
	

	Sam splint
	2
	
	0
	
	0
	
	0
	

	Single use cool pack
	1
	
	0
	
	0
	
	0
	

	SOS/  Carry sheet
	1
	
	0
	
	0
	
	0
	

	large clean sheeting (for covering burns) 
	1
	
	1
	
	1
	
	0
	

	Large combine Dressing 
	1
	
	1
	
	0
	
	0
	

	OTHER FIRST AID ITEMS
	
	
	
	
	
	
	
	

	Disposable splinter probes 
	5
	
	5
	
	3
	
	0
	

	Single Use icepacks 
	1
	
	1
	
	1
	
	0
	

	1 way valve resuscitation mask 
	1
	
	1
	
	1
	
	0
	

	Other items (please specify item & number)
	
	
	
	
	
	
	
	



EMERGENCY EQUIPMENT
The following emergency equipment is required for the project.  The location of this equipment shall be included onto the Site Plan and inspected on a weekly basis.

	

Equipment Type
	Symbol
	Type(s) Required
	Quantity / Location / Comments

	First Aid Kit
	
	Refer Above:
2 x type c first aid kits required for each stage

Stages 1, 2, 3, 4
	Stage 1- under 30 workers -- First aid room
Stage 2 – 30-50 workers – First aid room & upper working level including hoist
Stage 3 – 50 to 70 Workers -- First aid room & every third working level including hoist
Stage 4 – 70 to 95 workers-- First aid room & every third working level including hoist


	Emergency Siren
	[image: ]
	Transistor megaphone
	Located in Site management office

	Portable Fire Extinguishers
	[image: File:PublicInformationSymbol FireExtinguisher.svg]
	Dry powder type
	Located in relevant areas  in near proximity to electrical boards and hot works

	Chemical 
Spill Kit
	
	Bin type
	Located in substance storage area

	Chemical Resistant Gloves
	
	EN388/ 4121
	Located in spill kit & site management office

	Defibrillator
	[image: https://www.seton.net.au/media/catalog/product/cache/1/small_image/250x250/9df78eab33525d08d6e5fb8d27136e95/f/i/file_89_4.jpg]
	Automated
	Located in first aid room

	Stretcher
	
	Foldable
	Located in first aid room

	Other – specify:
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