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Materials List

	Company Name:
	N/A
	Address:
	Southern Queensland Correctional Precinct
	Email:
	N/A

	
	
	
	
	Contact No.
	N/A

	Building Project:
	Southern Queensland Correctional Precinct
	Address:
	N/A


	Category
	Material
	Description
	Supplier
	Quantity

	Foundation
	Reinforced Concrete
	High-strength concrete mix complying
	Holcim Australia
	250 m³

	
	Steel Reinforcement
	Reinforcing bars (Grade 500) for slabs and columns.
	InfraBuild Steel Centre
	12 tonnes

	
	Formwork Panels
	Pre-fabricated plywood formwork panels for concrete pouring.
	Dincel Construction System
	75 panels

	
	Waterproof Membrane
	Durable membrane for foundation moisture protection.
	Ardex Australia
	500 m²

	Structure
	Structural Steel
	Hot-rolled steel beams and columns
	BlueScope Steel
	15 tonnes

	
	Fire-Resistant Linings
	Fire-rated plasterboard for walls (FRL 120/120/120).
	Gyprock Trade
	450 sheets (1200x2400 mm)

	
	Concrete Columns
	Precast concrete columns for structural load-bearing.
	CSR Concrete Solutions
	30 columns

	Framing
	Timber Framing
	Treated pine framing for non-load-bearing walls
	Bunnings Trade
	200 linear meters

	
	Steel Framing
	Lightweight steel framing for internal partitions.
	Studco Building Systems
	150 lengths

	
	Insulation Panels
	Thermal and acoustic insulation for wall cavities.
	Bradford Insulation
	600 m²
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