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[bookmark: _Toc505596889][bookmark: _Toc435518296]Introduction
[bookmark: _Toc505596890]This Scope of Works relates to construction works at palm beach Job the site is located at lot 8 Rees Court Palm Beach QLD

The contract used may be the Australian Standard amended Subcontract Agreement: -

Hutchinson Lump Sum Subcontract Agreement (Minor Works)
All information and documentation has been provided by the Main Contractor in good faith. To the best of the Main Contractor’s knowledge, these documents describe the condition of the site. The Subcontractor is to thoroughly examine the site and will be fully responsible for work and costs associated with the site conditions.
Project Description
The project is a
. Two story Domestic dwelling 

Estimated project value for applicable allowances is.
$420000
Key project dates are:-
· Commencement on Site: 27/06/2022
· Practical Completion: 08/07/2022

Site Location: lot 8 Rees court Palm Beach QLD
[bookmark: _Toc505596891]Scope of Works
The Subcontract Works outlined in this document includes, but is not limited to the provision of all ……….
The Subcontract Works includes all related items as contained within the Project Documentation and to the satisfaction of: -
all legislation, 
The National Construction Code, 
The Building Code (where required under the Code)
The Australian Standards, 
Codes of Practice,
The Main Contractor’s Quality Manual / Handbook 
The Main Contractor’s Work Health and Safety Management Plan
The Main Contractor’s Subcontractor Health and Safety Requirements
The Main Contractor’s Environmental Management Plan
The Main Contractor’s Traffic Management Plan
The Main Contractor’s Industrial Relations Management Plan (where required under by the Code)
The Main Contractor’s Construction Management Plan

The details in this Scope of Works document form part of the Project Documentation, which includes (but is not limited to): -
the Subcontract Terms and Conditions,
Specifications,
Schedules,
Drawings,
The Principal Contractor’s Construction Program. 

Where ambiguities, discrepancies or inconsistencies exist between the Subcontract documents (subcontract terms and conditions, drawings, specifications, and the scope of works), the Subcontract document Order of Precedence within the Subcontract shall prevail. In addition, the Subcontractor has allowed within the Subcontract sum (at the time of tender acceptance) for the requirements of the Main Contractor’s Quality Manual and Quality Handbook as a minimum. The Subcontractor must notify the Main Contractor immediately upon discovery of any ambiguities, discrepancies or inconsistencies.
[bookmark: _Toc505596892]Detailed Description of the Work Elements
The Subcontract Works include but are not limited to the following:
1. Blockwork works as detailed and described as follows: -
a. Instillation of 7335 120mm x 280mm bricks 
b. The bricks shall be regular in size and free of defects
c. Instillation of ¼” to 5/8” thick mortar 
d. Instillation of any required scaffold up to 3m. (above 3m supplied by PCBU)
e. All work is to be carried out in accordance with the Work health safety act 2011 and other relevant legislation

2. The supply and installation of blockwork shall include, but not be limited to: -
a. All masonry work shall be carried out by qualified and competent workers
b. All bricks shall be laid true to lines and levels with joint of uniform thickness
c. All walls to be plump and in accordance with Australian standard AS/NZS 4456
d. Before use bricks shall be cleaned and scrubbed of any dirt/fungus etc to ensure the quality of finished product
e. Sand shall be screened once and washed once immediately before use
f. Mortar shall be used within 30 minutes of mixing, No re tempering of mortar will be aloud.





[bookmark: _Toc505596893]Works by Others
The following works DO NOT form part of this Scope of Works:
1. {Note any items excluded from Trade}
1. Reinforcement supply by the Main Contractor.
1. Concrete corefill supply by the Main Contractor 
1. Pressed Metal Door Frames (PMDF) supplied by the Main Contractor
1. Waterproofing 
1. 

[bookmark: _Toc505596894]Trade Inclusions (Generic to all Work Elements)
The Subcontract Works include but are not limited to the following:
1. The provision of all necessary tools, equipment, machinery and the like for the works under the Subcontract. 
1. Provide portable power generators for the supply of temporary site power where the site connection to the local authority power grid has not been completed or has been interrupted.
1. Assist in any dewatering or other rectification necessary following any inclement weather. Provide equipment (wet vacuum), clothing (brooms, squeegees, gum boots, etc.) required to allow for the rectification to be carried out in an efficient manner. 
1. Provide all scaffolding (other than scaffolding to the perimeter of the building), mobile scaffolding, work platforms, scissor lifts or the like, to provide access to heights and areas for the execution of the Subcontract works.
1. The Subcontractor Sum allows for costs associated with resolution and modifications in construction for all buildability issues.
1. The Subcontractor is to obtain, complete and submit all notices required by the various authorities when necessary and pay all fees in connection therewith, and shall submit for approval all necessary drawings and obtain all consents required to permit the execution of the works. 
1. The Subcontractor is responsible for the fire rating and acoustic rating of all penetrations, seals, and control joints associated with the Subcontract Works in accordance with the Main Contractor’s Quality Handbook Topic 14 and approved Fire Compartmentation Plan. At commencement of Works, submit for review a proposed Fire Penetration Register prepared by a Passive Fire QBCC Licensee / Certifier, showing details of the penetrations and the tested systems, together with test data and marking plans that uniquely identify each penetration.  Provide only a DTS NCC Section C system or DTS tested system / solution. Once approved by the certifier, ensure that all As-Built penetrations in fire rated building elements a) comply with test data, b) are recorded in the Certifier approved Subcontractor’s Fire Penetration Register, and c) that the installer’s Form 16 reflects this Register. Include with the Register photos of each penetration showing its identification label (and Fire Certifier’s QBCC licence number on the photo and Form 16), and marked up drawings identifying the positions of the installations.  
1. The Subcontractor is responsible for providing, monitoring and maintaining adequate protection of all works until Practical Completion of works having regard to the likely effect of all following trades and the sequencing of works.  The Subcontractor will be responsible for the rectification of any items damaged by following trades as a result of deficient protection.
1. The Main Contractor shall provide: -
a. Temporary site power  - 240v Single phase power boards,
b. Water connection points and disposal of waste water,
c. Access lighting
d. Site hoist, cranage and dogmen in accordance with the programme dates,
e. Temporary amenities: Lunch room, Ablutions, First Aid Facilities
f. Traffic control for the safe control of material deliveries to site,
g. Supply of waste bins and disposal of waste materials.
h. Erection and dismantle of Scaffold  to all sides of the perimeter of the building in accordance with Annexure Part A of the Subcontract Conditions
i. Supply, installation, maintenance and removal of temporary hoarding to the site.

[bookmark: _Toc505596895]Site Preliminaries
1. The Subcontractor shall allow for the work hours in accordance with Development Application Approval, planning permits, Council requirements, Council Operation Works Permits, and the Main Contractor’s site specific Construction Management Plan.
1. The Subcontractor shall include for all applicable travel allowances for the project.
1. The Subcontractor is not permitted to place signage (other than safety signage) on any part of the building, formwork, screen system or attachments to the building.
1. It is the Subcontractor’s responsibility to carry out all necessary set out and survey for works relative to the Subcontract scope. The Main Contractor shall provide datum points and main grid lines only for each portion of the works and at each main level. The Subcontractor is to protect set out points provided by the Main Contractor.  Any re-establishment of these points due to removal by the Subcontractor is to be provided by the Subcontractor or at the Subcontractor’s expense.
1. The Subcontractor is to have at all times, until the completion of Subcontract Works, an onsite experienced supervisor, who has the relevant experience, qualifications, and authority to execute the Subcontract Works, and is capable of taking direction from the Main Contractor and carrying out such direction. This appointed supervisor shall attend all site coordination meetings, control all daily work activities, and ensure compliance with all the Main Contractor’s Management Plans. 
1. The Subcontractor is required to provide all necessary labour and equipment to progressively clean up all debris, rubble, and construction waste generated whilst undertaking the Subcontract Works. Remove construction waste from associated work areas and dispose into the waste bins provided by the Main Contractor.  All work areas must be kept clean, tidy and safe to the satisfaction of the Main Contractor.  
1. All waste materials that can be recycled must be sorted by the Subcontractor and placed in the recycling bins provided by the Main Contractor.
1. The Subcontractor shall allow for all costs in regard to access to and egress from the Site, including but not limited to those costs associated with the location and nature of the Site and all necessary access restrictions arising from organised public events and festivals.
1. The Subcontractor shall allow for the following plant install and removal dates as relevant to the construction program-
	
	Install
	Removal

	scaffold
	27/06/2022
	N/A

	
	
	

	
	
	

	
	
	


Note: The above dates are indicative only. No costs will be borne by the Main Contractor as a result of providing these dates.
11. The Subcontractor shall provide task lighting and portable air extractor fans as required to ensure the Subcontractor meets the project’s safety, environmental and quality requirements. Task lighting must conform to the following minimum standards. 
a. All lights to be guarded.
b. Lights must be permanently fixed to fit for purpose stands. 
c. Lights to be tested and tagged by qualified electrician.
12. The Subcontractor shall supply a sufficient number of two way radios or the like for their Site Foreman representative as required.
13. Any necessary documentation to satisfy the requirements indicated in the specifications shall be submitted progressively as the works proceed. (For example: Inspection and Test Plan's, Safe Work / Environmental Method Statements)
14. If the Subcontract elsewhere requires further quality assurance, the Subcontractor shall prepare and maintain a conforming quality system, specific for the project. The conforming quality system shall be approved by the Main Contractor and any relevant consultants prior to commencement of work.
15. The Subcontractor is to provide a certification that it has obtained, read, understands and will comply in full with the Main Contractor’s documents entitled “Work Health & Safety Management Plan”. 
1. The project is a 5-day per week site. The Subcontractor may be required to work outside normal working hours if deemed necessary by the Main Contractor to achieve the Main Contractor’s program.
2. Subcontractors wishing or requiring to work extended hours beyond the Site Working Hours will be responsible for all costs associated with opening and maintaining the site.
3. The Subcontractor is to submit written confirmation and documentation confirming orders for overseas and long lead time materials have been placed within one week of contract award.
4. The Subcontractor is to ensure that all staging of works comply with the Main Contractor’s program requirements (including all necessary return visits).
[bookmark: _Toc505596897]Co-ordination
1. The Subcontractor is responsible to co-ordinate their work with that of the Main Contractor, other trades and the project works as a whole.  The Main Contractor will not consider additional costs for any co-ordination issues that occur throughout the duration of the works. 
2. The Subcontractor is to co-ordinate with services and the structure.  Service and structure documents are available for viewing upon request. 
3. In addition to an appointed supervisor, a Subcontractor Representative will attend all site co-ordination meetings with the Main Contractor representatives and other subcontract trade representatives.
4. The Subcontractor is to allow for all co-ordination associated with hold points in its Works (or the works of other associated trades).
5. Allowance is to be made for any staging and / or return visits to allow the works to be completed in accordance with the Main Contractor’s requirements.
[bookmark: _Toc505596898]Quality Management System Requirements
1. If the Subcontract elsewhere requires further quality assurance, the Subcontractor is required to provide Inspection Test Plans (ITP); detailing a description of each process activity and inspection requirements
2. Each activity description shall reference the appropriate controlling documents including but not limited to Australian Standard, Specification, Plan, Procedures, and manufacturer’s instructions. 
3. All Inspection Test Plans (ITP) and Field Inspection Checklists (FIC) including supporting documentation are to be submitted to the Main Contractor with the necessary Hold, Witness and or Surveillance Points. 
4. All ITPs and FICs are to be approved by the Main Contractor prior to any works commencing.
5. The Subcontractor is to notify the Main Contractor Quality Assurance Officer or Foreman 48 hours prior to a Hold or Witness point.  
6. Field Inspection Checklists (FIC) are to support all Inspection Test Plans (ITP) and to be completed progressively or as tasks are completed. 
7. Certification of Equipment requiring Calibration- All calibration certificates for specified equipment are to be issued to the Main Contractor Quality Assurance officer for registering prior to the equipment being used
8. The Subcontractor shall maintain a Communication Register, recording all the Company contacts inclusive of Quality and Health and Safety Representatives.

[bookmark: _Toc505596899]Finalisation of Works
a. The Subcontractor is to provide : 
b. The supply of all materials required
c. All equipment required
d. All labour required

[bookmark: _Toc505596900]Subcontract Sum Breakdown – See Attached Quotation.

	
	ITEM
	QTY
	UNIT
	AMOUNT

	1
	Materials
	
	
	

	1.01
	Bricks
	7335
	$1.80
	$13203

	1.02
	sand
	5m3
	$200
	$1000

	1.03
	Cement
	44 bags
	$9
	$396

	 
	 SUBTOTAL
	
	
	$14599

	
	
	
	
	

	2
	TRADE
	
	
	

	2.01
	Brickies Mate mortar retardant
	5
	$22
	$110

	2.02
	labour
	4 men
	$450 per day
	$18000

	2.03
	Equipment hires
	1
	$1500
	$1500

	2.04
	
	
	Item
	$0

	2.05
	
	
	No
	$0

	2.06
	
	
	Item
	$0

	2.07
	
	
	Item
	$0

	2.08
	
	
	Item
	$0

	2.09
	
	
	m2
	$0

	2.10
	
	
	No
	$0

	
	SUBTOTAL
	
	
	$19610

	
	
	
	
	

	
	SUBCONTRACT TOTAL (EXCL GST)
	
	
	$34209




[bookmark: _Toc505596902]Schedule of Rates
1. All rates nominated in this Schedule of Rates are fixed for the duration of the contract.
2. This Schedule of Rates shall be used for payment in respect of additions and/or deletions to the Scope of Works.
3. All rates shall be inclusive of costs for management, administration, supervision, overheads, profits, Workers Compensation and all other insurances. Payroll tax and other taxes, customs duty, escalation of prices and wages to contract completion, safety measures and costs complying with all obligations under the contract.
4. All rates including labour component shall be inclusive of the costs of supervision and associated costs, wages paid, all award payments, other industrial agreement payments and the like.
5. All rates including supply component shall be inclusive of all costs for materials, equipment, plant, labour, procurement, payment of fees, transportation, handling (on and off site), delivery, storage, wastage, and complying with the specification and testing as necessary.
6. All rates including an installation component shall be inclusive of all costs for materials, equipment, plant, labour, supervision, procurement, transportation, handling (on and off site), delivery, payment of fees, set out, storage, wastage, environmental controls, safety, cleaning, protection (including removal), complying with the specification and testing as necessary, commissioning, and certification.
7. All rates involving plant or equipment shall be inclusive of the costs of depreciation, fuel, electricity, consumables, registration, transportation, and delivery to and removal from site.
8. All rates are exclusive of GST.
	
	Item
	Unit Rate

	1
	labour
	$56.25 / Hour

	2
	{Rates per elements / items as per  project requirements}
	$0.00 / Hour

	3
	{Rates per elements / items as per  project requirements}
	$0.00 / Hour
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