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	Record number
	Date of entry
	Hazard
	Location
	People exposed
	Possible injuries/ damage
	Control measures
	Risk assessment

	1
	14/12/2019
	LP Steam leak
	D-9 Deaerator
	N/A
	Burns
	Hard barricade area
	(4D) Low

	2
	14/12/2019
	Slippery surface
	E-1 condenser
	N/A
	Injury from slip
	Hosed down area
	(4E) Low

	3
	14/12/2019
	Heat exhaustion
	Site
	All
	Heat stroke / dehydration
	Hydration, frequent breaks, task rotation
	(5D) Low

	4
	15/12/2019
	High Temperature surfaces
	CD-1 Extraction Valve
	N/A
	Burns
	Barricaded area recorded in shift log.
	(5C) Low

	5
	15/12/2019
	Oil on lube oil skid
	CD-5 lube oil skid
	N/A
	Slip injury or Loss of containment to environment
	Spill kit used to contain and remove oil to regulated waste. 
	(4C) Medium


RISK REGISTER

RISK MATRIX
	Matrix
	A:
Death or permanent disability
	B:
Serious injury
	C:
Lost time injury
	D:
Casualty Treatment
	E:
First Aid

	1: Very Likely
	E
	E
	H
	H
	M

	2: Likely
	E
	H
	H
	M
	M

	3: Possible
	H
	H
	M
	M
	L

	4: Unlikely
	H
	M
	M
	L
	L

	5: Very Unlikely
	M
	M
	L
	L
	L



	E: Extreme
	H: High
	M: Medium
	L: Low
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