Scaffold Inspection Checklist
Checklist to be completed as per below guidelines:
* Prior to initial use
** On the first working day of each calendar month
*** After any repairs are completed
**** After any incidents that may affect the structural integrity

	Location:
	
	Date:
	

	Inspector Name:
	
	Time:
	

	Inspector Signature:
	

	
	
	
	

	
	
	COMMENTS
	SPEC REF

	SCAFFOLD VACINITY

	Has public protection been provided?
	YES / NO
	
	

	Have sufficient safeguards against electric powerlines been provided?
	YES / NO
	
	

	Is there sufficient control over vehicle movement?
	YES / NO
	
	

	Is there sufficient control over crane operation?
	YES / NO
	
	

	Are there sufficient controls for the storage, handling and use of hazardous chemicals?
	YES / NO
	
	

	Are scaffolds erected a safe distance away from trenches or excavations?
	YES / NO
	
	

	SUPPORTING STRUCTURE

	Is the supporting structure in good condition?
	YES / NO
	
	

	Does the supporting structure have adequate strength?
	YES / NO
	
	

	Are there sufficient controls to prevent deterioration of the supporting structure?
	YES / NO
	
	

	Are all measures to strengthen the supporting structure adequate?
	YES / NO
	
	

	Is the risk of the supporting structure being overloaded from other sources adequately controlled?
	YES / NO
	
	

	Is the scaffold built on solid ground? If built on soft ground, are soleboards used to properly distribute the load?
	YES / NO
	
	

	SOLEBOARDS AND BASEPLATES

	Are there sufficient soleboards?
	YES / NO
	
	

	Are the soleboards of suitable material and in a serviceable condition?
	YES / NO
	
	

	Are the soleboards secure?
	YES / NO
	
	

	Are there sufficient baseplates?
	YES / NO
	
	

	Are the baseplates of the appropriate type?
	YES / NO
	
	

	Are the baseplates serviceable and of suitable dimensions?
	YES / NO
	
	

	Are the baseplates secure?
	YES / NO
	
	

	SCAFFOLD STRUCTURE

	Are the standards bearing firmly?
	YES / NO
	
	

	Are the standards plumb (or as designed)?
	YES / NO
	
	

	Are the longitudinal standard spacings correct?
	YES / NO
	
	

	Are the transverse standard spacings correct?
	YES / NO
	
	

	Are the joints in standards correctly positioned?
	YES / NO
	
	

	Are the joints in standards correctly secured (special duty or hung scaffold)?
	YES / NO
	
	

	Are the ledgers level (or as designed)?
	YES / NO
	
	

	Are the ledgers continuous (or as designed)?
	YES / NO
	
	

	Are the lift heights correct?
	YES / NO
	
	

	Are the horizontal ledger spacings correct?
	YES / NO
	
	

	Are the ledgers correctly secured?
	YES / NO
	
	

	Are ledger joints correctly positioned (tube and coupler scaffold)?
	YES / NO
	
	

	Are the joints in ledgers correctly secured (tube and coupler scaffold)?
	YES / NO
	
	

	Are there sufficient transoms/putlogs?
	YES / NO
	
	

	Are the transoms/putlogs correctly positioned and secured?
	YES / NO
	
	

	Is the bracing adequate?
	YES / NO
	
	

	Is the scaffold sufficiently stable?
	YES / NO
	
	

	Are the ties correctly positioned and correctly fixed?
	YES / NO
	
	

	PLATFORMS

	Does the scaffold have the required number of working platforms?
	YES / NO
	
	

	Are the working platforms at the required locations?
	YES / NO
	
	

	Are catch platforms correctly positioned?
	YES / NO
	
	

	Are the platforms and supporting scaffold constructed for the appropriate duty live loads?
	YES / NO
	
	

	Are the platform dimensions suitable for the intended work?
	YES / NO
	
	

	Is there adequate edge protection?
	YES / NO
	
	

	Are the platforms correctly constructed?
	YES / NO
	
	

	Are planks secured against wind?
	YES / NO
	
	

	ACCESS AND EGRESS

	Is there safe access and egress to every scaffold platform?
	YES / NO
	
	

	Are temporary stairways correctly installed?
	YES / NO
	
	

	Are portable ladders of an industrial grade, serviceable and correctly installed?
	YES / NO
	
	

	Are access ways and access platforms correctly installed
	YES / NO
	
	

	CONTAINMENT SHEETING

	Has the scaffold been designed for wind loading on any containment sheeting?
	YES / NO
	
	

	Are the fixing ties secure?
	YES / NO
	
	

	Are there any rips or tears?
	YES / NO
	
	

	Are the overlap joints satisfactory?
	YES / NO
	
	

	GENERAL FITNESS FOR PURPOSE

	Is there adequate provision for material handling?
	YES / NO
	
	

	Are the clearances between the scaffold and adjacent structures correct?
	YES / NO
	
	

	Is there adequate protection from falling debris?
	YES / NO
	
	

	Has the scaffold been adequately designed to support all attachments?
	YES / NO
	
	

	Are all approaches and platforms effectively lit?
	YES / NO
	
	

	

	Scaffolder Name:
	
	Site Manager Name:
	

	Scaffolder Signature:
	
	Site Manager Signature:
	



