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Cost Estimation Sheet

	Participant name
	Jeremy Tydd

	Date
	01.12.2024



Details of Building and Construction Project
	Name of project
	6 x 6 Shed

	Type of project
	 Residential building
 Commercial building

	State/Territory
	Qld

	Plans accessed for material estimates
	Lysart




Identify internal linings, external cladding and roof materials from plans and specification
	Item
	Description 

	Internal linings
	Wall frame assembly

	External cladding
	Colorbond sheeting, tophat, screws

	Roofing materials
	Colorbond sheeting,screws, tophat, guttering, downpipes




Opinion of costs - for one (1) room identify costs of three (3) materials needed.
	Item
	Description (including size, thickness)
	Cost per Unit
	Quantity
	Total cost
	Construction method

	1
	Roof Colorbond sheets 6mts x  0.48mm
	98.50
	8
	788.00
	Installation

	2
	Wall Colorbond sheets 3mts x 0.48
	49.00
	32
	1568.00
	Installation

	3
	Screws
	.30
	1000
	300.00
	Installation




Identify two (2) Prime Cost (PC) items and two Provisional Sum items
	Prime Cost items
	Provisional Sum items

	Screws
	Down Pipes

	Colorbond sheets
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