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Documentation of design and construction (suitability or evidence of suitability)
	Project Name: Everton Park Hotel Motel

	Project address: 101 Flockton St, Everton Park
	Site Plan attached: Yes

	Prepared by: Michael Trott

	Date: 17/01/25

	Description of project:
Accommodation refurbishment 


	Site Classification/s:
Mostly rock or very stable soil with little or no ground movement due to moisture changes.

	Documentation of design and construction (suitability or evidence of suitability)

	Site preparation

	Site preparation
	NCC / Australian Standards requirements
	Compliant Performance solution

	Earthworks
	AS 3798: Guidelines on Earthworks for Commercial Sites
	Compaction techniques adjusted to specific site conditions to achieve compliance.

	Site preparation

	Site preparation
	NCC / Australian Standards requirements
	Compliant Performance solution

	Earth retaining structures
	AS 4678: Earth-retaining Structures
	Use of modular block walls with geogrid reinforcement for flexibility.

	Drainage
	AS 3500.3: Stormwater Drainage
	Installation of custom subsurface drainage system to suit high water table areas.

	Site preparation
	NCC / Australian Standards requirements
	Compliant Performance solution

	Termite risk management
	AS 3660.1: Termite Management
	Use of physical barriers integrated with structural elements for added protection.

	Materials
	Materials to meet AS/NZS 1170
	Selection of eco-friendly materials with equivalent structural performance.

	Footings and slabs

	Site classification

	Footings and slabs
	NCC / Australian Standards requirements
	Compliant Performance solution

	Footings and slabs
	AS 3600: Concrete Structures
	Use of high-strength, fibre-reinforced concrete to minimise cracking.

	Footings and slabs
	NCC / Australian Standards requirements
	Compliant Performance solution

	Moisture Barrier
	AS 2870: Waterproofing
	Customised moisture barrier with dual-layer system for enhanced protection.

	Materials
	Compliant with relevant NCC & AS
	High-performance materials meeting equivalent durability standards.

	Concrete and reinforcement

	Concrete and reinforcement
	NCC / Australian Standards requirements
	Compliant Performance solution

	Concrete and reinforcement
	AS 3600: Concrete Structures
AS/NZS 4671: Steel Reinforcing Materials
	Use of geopolymer concrete as a sustainable alternative to Portland cement.
High-ductility steel reinforcement adapted for seismic areas.

	Materials
	Compliant with AS/NZS Standards
	Innovative lightweight reinforcement for ease of installation.

	Masonry

	Masonry
	NCC / Australian Standards requirements
	Compliant Performance solution

	Masonry
	AS 3700: Masonry Structures
	Customised masonry blocks with integrated insulation for energy efficiency.

	Moisture Barrier
	AS 3700: Masonry Waterproofing
	Multi-layered waterproofing membrane tailored for high rainfall areas.

	Materials
	Compliant with relevant NCC & AS
	Alternative masonry materials with comparable strength and durability.

	Framing/Structure

	Framing/Structure
	NCC / Australian Standards requirements
	Compliant Performance solution

	Framing
	AS 1684: Residential Timber Framed Construction
	Engineered timber systems designed for greater load capacity.

	Materials
	Compliant with AS/NZS Standards
	Laminated timber products for enhanced structural integrity.

	Roof and Wall Cladding

	Roof and wall cladding
	NCC / Australian Standards requirements
	Compliant Performance solution

	Roof and wall cladding
	AS 1562.1: Design and Installation of Sheet Roofs
	Innovative cladding system incorporating solar panel integration.

	Materials
	Compliant with relevant NCC & AS
	Lightweight composite cladding with superior thermal performance.

	Glazing

	Glazing
	NCC / Australian Standards requirements
	Compliant Performance solution

	Glazing
	AS 1288: Glass in Buildings
	High-performance glazing with double glazing for acoustic and thermal control.

	Materials
	Compliant with relevant NCC & AS
	Advanced glazing films for enhanced energy efficiency.

	Fire Safety

	Fire Safety
	NCC / Australian Standards requirements
	Compliant Performance solution

	Fire Safety
	NCC Part C: Fire Resistance
	Use of fire-rated cladding and passive fire protection systems.

	
	
	

	
	
	

	Access/Stairs/Lifts/Ramps

	Access/Stairs/Lifts/Ramps
	NCC / Australian Standards requirements
	Compliant Performance solution

	Access
	AS 1428: Design for Access and Mobility
	Modular ramp systems for flexibility in different site conditions.

	
	
	

	Materials
	Compliant with AS/NZS Standards
	Non-slip materials with extended durability in high-traffic areas.

	Ancillary Provisions

	Ancillary Provisions
	NCC / Australian Standards requirements
	Compliant Performance solution

	Waste Management
	NCC Volume 2: Site Waste Management
	On-site waste separation and recycling stations for sustainable waste management.

	Acoustic Performance
	NCC Volume 1 Part F5: Sound Insulation
	Installation of advanced acoustic panels and soundproofing materials.

	
	
	

	Energy Efficiency

	Energy Efficiency
	NCC / Australian Standards requirements
	Compliant Performance solution

	
	NCC Part J: Energy Efficiency
	Integration of smart energy systems and building automation for efficiency.

	
	
	

	
	
	

	Health and Safety

	Site-Specific Requirements:Implementation of site-specific safety plans, including hazard identification, risk assessments, and control measures. Safety equipment (PPE) and training provided to all workers.

Risk Mitigation:Measures include fall prevention systems, fire evacuation plans, and compliance with AS 4801: Occupational Health and Safety Management.

Emergency Preparedness:Clearly marked emergency exits, on-site first aid kits, and regular safety drills conducted to ensure preparedness.

Worker Well-being:Provision of amenities such as clean drinking water, sanitary facilities, and shaded rest areas to maintain worker health and comfort.



	Consultation

	

	Policies

	

	Procedures

	

	Issues to be addressed and consultation

	Issue
	Who to consult
	Improvements for consideration
	Feedback following consideration
	Supporting Resources
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