Construction Plan Details Verification Checklist 

INSTRUCTIONS TO THE ASSESSOR: 
The specifications below are not specific to any building and construction project. Before the actual assessment, access and review the specifications for the building and construction project the candidate is undertaking as part  of this assessment. Update/adapt/revise the checklist below to ensure they reflect these specifications. 

	Completed by
	[bookmark: _GoBack]  DaweI Yang   

	Date completed
	   31/10/2022  



	Plans
	Version No.
	Date Published

	Architectural plans 
	     version1.2010     
	 2010   

	Structural Plans 
	    version1.2010      
	  2010   

	Mechanical Plans 
	    version1.2010      
	   2010  

	Electrical Plans
	    version1.2010      
	   2010  

	Plumbing and Drainage Plans
	      version1.2010    
	  2010   





	Specifications
	Complied?
	Reasons for non-compliance of critical points indicated

	Category 1: Roofer 

	1. Main Roof Covering: Colorbond sheet metal roofing @ 30° pitch 
	☒YES    ☐ NO
	     

	2. Roof Insulation: Sarking to underside of roof sheeting with ceiling insulation to energy assessors requirements. 
	☒YES    ☐ NO
	     

	 3. (celling height .) 
	☒YES    ☐ NO
	     

	Category 2: Roof Plumber 

	1. Gutters: Colorbond fascia & gutters 
	☒YES    ☐ NO
	     

	2. Exposed Downpipes: Standard 90x45 Colorbond downpipes connect to soakwells where shown on plans and match wall colours 
	☒YES    ☐ NO
	     

	 3. concealed downpipes) 
	☐YES    ☒ NO
	   N/A  

	Category 3: Sanitary Plumber 

	1. Drainage and Water Service: Connect to main sewer 
	☒YES    ☐ NO
	     

	Drainage: All soak wells to heights and details shown on site plan including connection to RWP. 
	☒YES    ☐ NO
	     

	Water Service: One 20 mm copper cold water service to all points shown on plan and connect to water meter at the front boundary.
	☒YES    ☐ NO
	     

	2. Fixtures & Fittings 
	☒YES    ☐ NO
	     

	Toilet Suites: Coroma Profile No. 4 vitreous china toilet suite in white 
	☒YES    ☐ NO
	     

	Cisterns: Coroma Profile No. 4 Dual Flush in white
	☒YES    ☐ NO
	     

	 3. (instantaneous gas hot water system connected to all points as required) 
	☒YES    ☐ NO
	     

	Category 4: (Assessor to add more categories as needed.) 

	1. Item 1 external wall: painted rendered finish
	☒YES    ☐ NO
	     

	2. Item 2 internal wall: plaster smooth and float set
	☒YES    ☐ NO
	     

	3.shower screen: clear pivot doors and fixed panels  
	☒YES    ☐ NO
	     



Note to Assessor: The categories above and items under each category are based on a fictitious company’s project specifications. The assessor must update/adapt/revise the above to ensure they reflect the actual specifications for the building project. 
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