Methodology Statement for JDL Construction Group PL

Site Address: 		58 Blackmore Street, Windsor
Date: 			13th November 2020
Time:			0600
Project:			Installation of Connected Extension
	
Installation of relocatable building by Brett’s Timber, at the back of existing house and deck area.
Building to be craned onto the site by East Coast Crane Hire and attached to steel stumps and PFC beams already in place.
Traffic conditions have been assessed by Action Traffic Control, traffic control to be used for the duration of this activity.
All necessary permits have been obtained, East Coast Cranes have assessed the site and selected the appropriately sized crane for this activity.
East coast Crane Hire to supply personnel, to manage the activity.

Methodology:
Traffic control to setup by Action Traffic Control, and manage all traffic from Albion Road, Vine Street and Blackmore Street.
Crane position to be established by East Coast Cranes for the lift, crane set up to take place.
All personnel to wear hard hats and hi-viz PPE, while on site.
East Coast Cranes will have control of the site during the crane usage and all personnel to take directives from the Dogman on site.
Crane to lift PFC channels into place, and to be bolted by JDL Construction.
Crane to lift the portable building into to position, ready for bolting by JDL Construction.
During the bolting stage, all personnel must not go under the building to perform this task.
Bolting to be done working from the outside of the building line, and only when instructed by the Dogman.
Building to be securely bolted, and sub floor bracing installed.
Crane to be folded, all lifting gear to be removed from site.
Traffic control to be removed.
