CONTRACT TITLE:  
LOCATION:  CEP

DRAWING NUMBERS:

SITE SPECIFIC DOCUMENT NUMBER:   CC-HY-CEP-CL-014-0001  A

NO.
ITEM
INSPECTION
STANDARD
INSPECT BY
Y / N
NA
COMMENTS
1
Check set out of penetrations
Drawing/Spec
A




2
Check location and set out and design of pipe work and council approved plans
Drawing/Spec
A




3
Coordinate with other trades

Drawing/Spec
A


4
Check type material –pipe clips, jointing method 
Drawing/Spec 
AS3500.1, AS2845.1,
AS3500.4
A



5
Visual inspection prior to welding, glue or final connection
CC
A


6
Check fire rating any penetrations

ITP/ CC /F.R.
A/W


7
Test pipe work
Water AS3500.1, AS3500.4
A/W



8
Pipe ID / Tape
Spec AS3500.1, AS3500.4
A/W



9
Pipe insulation (Hot Water)
Spec AS3500, AS3500.4
A/W


10
Inspection- Council- other statutory authority

H


11
Photos attached





KEY  A= CC INSPECTION  W= CLIENT WITNESS POINT H= HOLD POINT G=GCCC
Supervisors Confirmation of Satisfactory Inspection
Checklist completed by:
Name: 
Signature:

Date: ___/___/___

