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CPCCBC4012 
Read and interpret plans and specifications 

ASSESSMENT SUMMARY

The assessment activities for CPCCBC4012 Read and interpret plans and specifications cover all aspects of the unit of competency. For Apprentices/Trainees, this includes supervisor completion of the Apprentice/Trainee Record (ATR). 

Participants must read all the information given before starting any assessment task. The assessment tasks are intended to be fair, flexible, valid and reliable. If a Participant has any questions or requires alternative arrangements to be made such requests should be directed to their Trainer/Assessor, who should note such arrangements in the ‘Assessor Comments’ on the affected assessment. If a Participant feels they are not yet ready to be assessed, they should discuss their options with their Trainer/Assessor. 

To satisfactorily complete the assessment, the Participant is required to answer all questions correctly and demonstrate their skills to industry standards. If a Participant does not answer all questions or perform all tasks, they will be deemed ‘Not Satisfactory’ for the task and ‘Not Yet Competent’ for the unit of competency. 

The Trainer/Assessor can provide the Participant with additional information on interpreting the assessment outcomes and guide the Participant’s options. If a Participant is still deemed ‘Not Satisfactory’ they will have the opportunity to undertake a supplementary assessment or appeal the result as per the process in the Student Handbook. 

By signing below, the Participant acknowledges:
· They understand the assessment instructions and requirements, and consent to being assessed. 
· The work submitted is to be their own work – with the work of/with others needing to be clearly acknowledged and documented. 
· They consent to any photo/video recording of their work that occurs during assessment. 

	Participant name
	Michael Trott

	Participant signature
	


	Pre-requisite unit(s) to be achieved and authenticated prior to undertaking assessment

	 Not applicable 



	Task
	Date completed
	Assessment Results 

	Theory Exam
	3/11/2023
	 Satisfactory 
	 Not Satisfactory

	Workbook 
	5/11/2023
	 Satisfactory 
	 Not Satisfactory

	Practical Assessment
	6/11/2023
	 Satisfactory 
	 Not Satisfactory

	Outcome for CPCCBC4012
	Select Date.
	 Competent
	 Not Yet Competent



	Evidence requirements checklist (ticked by assessor and evidence supplied to RTO)

	 Theory Exam
 Workbook
 Hand out 3 - Slab Plan for Activity 3
	 Practical Assessment
 Cost estimation sheet (HO5 template available)



	Assessor name
	

	Assessor signature
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THEORY EXAM


	Participant name
	Michael Trott




	FOR THE PARTICIPANT

	Instructions

	· You will complete written questions as outlined on the following pages. You must attempt all questions and provide enough detail in your responses to demonstrate your knowledge.
· It is anticipated that you should complete this assessment within two (2) hours, but additional time may be allowed upon negotiation with the Assessor.
· You must complete all questions unassisted by the Assessor or other personnel but may refer to reference material as needed. All questions must be answered correctly for a ‘Satisfactory’ assessment outcome to be awarded. 
· An oral examination may be allowed under certain circumstances, whereby your answers will be documented by another party. 
· Any written questions that are incomplete, or not answered satisfactorily will need to be completed again after further training support.
· If you answer a question incorrectly but modify your response, put your initials next to the written change (or the Assessor must initial a verbal change).

	Resources required

	Pen




	FOR THE ASSESSOR

	Instructions

	· Where oral examination has occurred, ensure that this is acknowledged in writing (e.g. FT001 and Assessor Comments)
· All questions must be satisfactorily demonstrated by the Participant for a Satisfactory determination (indicated by an Assessor tick to the right of the question).
· Assessors are to complete marking in pen of a different colour to the Participant.
· If the Participant verbally modifies their response, write in the modified response verbatim and put your initials next to the written change. 


[bookmark: _Ref396827952]

	[bookmark: _Hlk82780839]ASSESSOR COMMENTS

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	




[bookmark: _Ref130817641]What is the significance of concept drawing/sketches?

	[bookmark: _Hlk85785851]Answer
	The significance of concept drawings are they can be used for the purpose of presenting preliminary ideas regarding the building project quickly and although the drawings are simple they can also be used to further explore more ideas and quickly incorporate these ideas into the drawing.
 
	




[bookmark: _Ref130817651]Discuss when you may come across concept drawings/sketches.

	Answer
	You would come across concept drawings at presenting stage of a project
	




[bookmark: _Ref130818166]Explain what is meant by architectural plans.

	Answer
	.Architectural plans are drawings that can be used to understand details about the architectural aspects of a building and how architectural elements are integrated into the building
	




[bookmark: _Ref130818168]Provide four (4) plans that are considered part of the architectural plans.

	Answer
1.

2.

3.

4.
	
Site plans

Elevations

Sections

Detailed views
	



[bookmark: _Ref130818385]Describe what structural plans are.

	Answer
	Structural plans are drawings that provide information on the structural aspects of the building
	




[bookmark: _Ref130818387]How is a structural plan different from an architectural plan?

	Answer
	 Architectural plans are concerned with information regarding the aesthetic, function, and general feel of the building, structural plans are concerned with what makes the building strong and stable against expected external forces.

	




[bookmark: _Ref130819696]Explain what a civil plan is.

	Answer
	 These drawings show an overview of all construction site elements and how these are integrated into each other during the construction phase.

	




[bookmark: _Ref130819697]Discuss how civil plans may be similar to other plans.

	Answer
	They generally contain details that can be found on both architectural and structural plans and like architectural civil plans contain the contours of the landscape
	




[bookmark: _Ref130820127]What is the purpose for mechanical plans?

	Answer
	The purpose of mechanical plans is to show specifications related to the mechanical equipment and processes. Mechanical plans will also show you where different mechanical equipment is placed in a building and the layout of necessary ducting 
	




[bookmark: _Ref130820129]Discuss three (3) details you may find in mechanical plans.

	Answer
1.



2.



3.
	
HVAC layout



Size type and layout of ducting



Thermostat type and location
	




[bookmark: _Ref130822249]When would electrical plans be used?

	Answer
	Electrical plans would be used to quatify the amount of lights in an area and where they will be situated.
It can also give you information about electrical systems  or circuits such as power, lighting and communication and where they are situated in the building 
	




[bookmark: _Ref130822251]Provide three (3) examples of details contained in electrical plans.

	Answer
1.

2.

3.
	
Wiring layout for power

Wiring layout for lighting

Location of panels and switches
	



[bookmark: _Ref130822998]What are plumbing and drainage plans used for?

	Answer
	Plumbing plans can be used for a guide for the installation of water supply and drainage components with examples being pipes, fixtures, valves 
	




[bookmark: _Ref130822999]Discuss what may be needed when plans display council pipework.

	Answer
	You will need to determine whether council approval or permits are required
	




[bookmark: _Ref130881039]Why is it important to check and ensure that the plans you are using are the current version?

	Answer
	This is highly important because these plans contain all the up to date amendments of the building
	




[bookmark: _Ref130881993]What can occur if an outdated version of the plans is used?

	Answer
	If outdated plans are used mistakes can be made in developing cost estimates, purchases of non-compliant material can be made and faulty installation of construction elements could occur. All this could incur extra  costs for addressing and rectifying faults caused by using outdated plans.
	




[bookmark: _Ref77849989][bookmark: _Ref130883061]Discuss what site plans are drawn to reflect.

	Answer
	Site plans are drawn to reflect the entire scope of the project and gives you an overview of the entire property and location which in turn gives you state/territory requirements the building must follow.
	




[bookmark: _Ref130883068]Discuss the purpose of reading the floor plan.

	Answer
	The purpose of reading a floor plan is to show you the layout of the building and where the walls, column’s, doors and windows are and defines the space of the building. You can also use them to gain dimensions.
	



[bookmark: _Ref130883412]Discuss two (2) key differences between elevation view and section view.

	Answer
1.











2.
	
Elevation drawings show the vertical view of the building as it can be seen from the outside (façade) whereas section drawings show how the structure looks with respect to an imaginary line that cuts it








With sections views you can look at the building interior and gain internal dimensions whereas on the elevation drawings you can gain the roof height
	




[bookmark: _Ref130884038]Discuss the purpose of reading detail drawings.

	Answer
	The purpose of reading detailed drawings is get more clarification on detailed jobs as it gives you more intricate details of difficult configurations.
Detailed drawings give you better guidance on how a certain job can be done
	




[bookmark: _Ref130884676]Why is it important to measure from a datum point?

	Answer
	It is important to measure from the datum because this is the point of reference for all vertical measurements made in the construction project.
	




[bookmark: _Ref130885229]Discuss what reduced levels (RL) are and how these are established in construction drawings.

	Answer
	Reduced levels are vertical measurements and these can be established in construction drawings by setting the datum at the lowest part of the building (e.g. basement), which will be considered as 0.0 metres elevation. This means that all other elements, excluding foundations, will have a ‘positive’ elevation
	




[bookmark: _Ref130886686]Describe the purpose of the title block and what it contains.

	Answer
	Title blocks provide general information about the drawings and specific information about the particular drawing sheet
	




[bookmark: _Ref130886688]Where is the title block usually located on the plans?

	Answer
	It is lusually located at the bottom portion or at the right hand side of the drawing sheet
	




[bookmark: _Ref130887510]Describe the purpose of using scale drawings in construction.

	Answer
	The purpose of a scale drawing is to be able measure and determine the actual size of building components with the use of a scale rule
	




[bookmark: _Ref130552834]Describe each ratio of standard scale ranges below.

	Answer
	Ratio
	Description
	

	
	1:100
	The real size of the object, the drawing is a 100 times smaller
	

	
	1:2
	Given the real size of the object, the drawing is 2 times smaller
	

	
	1:50
	Given the real size of the object, the drawing is 50 times smaller
	



[bookmark: _Ref130888097]Describe why examining detail drawings is important.

	Answer
	Examining detail drawings are important when analysing intricate details and any complex configuration since this allows you to determine the specifications of building components such as sizes and thickness, as well as the corresponding methods of construction or installation processes.

	




[bookmark: _Ref130888441]What is the difference between utilities plans and specifications and services plans and specifications in the context of building construction?

	Answer
	The difference between the two is the utilities plan is concerned with providing information regarding the supply for electricity and water, lifts, gas supply, sewage and other items for the construction phase. Whereas the services plan is concerned with systems necessary for the smooth flow of construction operations, which include lighting, security alarm and fire safety detection and protection. .

	




[bookmark: _Ref130889173]Describe what is meant by each of the following drawing descriptions.

	Answer
	Drawing description
	Meaning
	

	
	Isometric drawings
	These are 3d drawings on a 2d surface where the same scale is used for all axes
	

	
	Oblique drawings
	These are the 2d projection of 3d drawings that represent an object accurately by showing the true shape and form of the object based on the point of view of the observer
	

	
	Perspective drawings
	These are 3d drawings which show an approximate representation of an object as perceived by the eye
	

	
	Orthographic drawings
	These drawings are 3d images presented in 2d in which three views are generally produced
	



[bookmark: _Ref130889385]What are CAD drawings? Explain how CAD is used in building and construction?

	Answer
	CAD drawings are drawings created and modified with the use of computer software.These drawings can be 2d or 3d illustrations or models created and used by engineers, architects, and construction managers to create precise drawings of the building and its components. They allow you to examine parts of the building conveniently and accurately in different views and at different angles and they can be easily modified.
	




[bookmark: _Ref130889897]Provide a brief description of the given classes of buildings according to the National Construction Code.

	Answer
	Building Class
	Description
	

	
	Class 1a building
	One or more buildings forming a single dwelling 
	

	
	Class 2 building
	A building containing two or more sole-occupancy units, each being a separate dwelling
	

	
	Class 4 building
	Is  the only dwelling or residence within any class 5,6,7,8 or 9 buildings
	

	
	Class 5 building
	An office building used for professional or commercial purposes, except for buildings of class 6,7,8 or 9
	

	
	Class 7b building
	Buildings used to display or produce wholesale goods
	

	
	Class 10a building
	A private garage, carport, shed or the like
	




[bookmark: _Ref130975341]What is building information modelling (BIM)?

	Answer
	This is a 3D model based process that uses tools and technology that enable the creation and management of digital representations of physical and functional characteristics of structures, buildings and places
	




[bookmark: _Ref130890045]Explain how the NCC is relevant to construction drawings.

	Answer
	The NCC is relevant as it must be reflected in the construction drawings during the planning stage as it sets out the technical provisions for design, construction and performance of buildings and plumbing and drainage systems
	




[bookmark: _Ref130890248]Discuss the importance of complying with standards during a building and construction project.

	Answer
	The importance of complying with standards during a building and construction project is the upmost of importance as these standards are going to be used to assess the completed building, so referring to them during the construction phase means greater chance of passing these assessments.
	




[bookmark: _Ref130910187]Discuss how you would identify wind bracing and tie-down requirements from construction plans.

	Answer
	Wind bracing and tie down requirements can be identified in the roof plan and also in the detailed drawings. Detail drawings provide large scale views of wind bracings and tie downs which means that you can look further into the set up, sizes and materials used in the makeup of wind bracing and tie downs.
	




[bookmark: _Ref130969649]Discuss why you would access AS 1684.2 Residential timber-framed construction Non-cyclonic areas, when reading plans and specifications.

	Answer
	You would access As 1684.2 to check accuracy of wind bracing materials and tie down methods from your plans against the wind bracing table shown in AS 1684.2. This makes sure the details in the plans are accurate and to pick out any discrepancies between the details in the plans and the wind bracing table.
	




[bookmark: _Ref130970244]Reasonable allowances are made by builders for the different construction items in a building project. Discuss what Prime Cost (PC) items are.

	Answer
	PC items are items that are not yet selected or whose prices cannot be determined at the time the contract is entered. It requires a builder to make reasonable allowances for the supply and installation of these items
	




[bookmark: _Ref130970247]Explain what Provisional Sum (PS) items are.

	Answer
	PS items are particular works or services whose cost of carrying out the works are not yet defined into detail for builders to establish accurately .
	




[bookmark: _Ref130971979]Explain how to locate installation points of the services to the building from the plans.

	Answer
	To locate the installation points of building services, you can refer to floor plans. The point of installation of services is the connection between a fixture and the medium or material used for supply
	




[bookmark: _Ref130971981]Explain how to locate connection points of services to the building from the plans.

	Answer
	To locate connection points of building services, you can refer to the site plan. The point of connection of services can be located by referring to the labels and legend or schedule.
	




[bookmark: _Ref130972216]Explain how to locate fixtures from the plans.

	Answer
	You can locate fixtures from the plans by referring to the construction plans and then study the labels and legends
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WORKBOOK


	Participant name
	Michael Trott




	FOR THE PARTICIPANT

	Instructions

	· You will complete written activities as outlined on the following pages. You must attempt all questions and provide enough detail in your responses to demonstrate your knowledge.
· The timeframe for these tasks will be established by your Assessor or Training Plan, but additional time may be allowed upon negotiation with the Assessor.
· You must complete all questions unassisted by the Assessor or other personnel but may refer to reference material as needed. All questions must be answered correctly for a ‘Satisfactory’ assessment outcome to be awarded. 
· An oral examination may be allowed under certain circumstances, whereby your answers will be documented by another party. 
· Any written questions that are incomplete, or not answered satisfactorily will need to be completed again after further training support.
· If you answer a question incorrectly but modify your response, put your initials next to the written change (or the Assessor must initial a verbal change).

	Resources required

	Pen




	FOR THE ASSESSOR

	Instructions

	· Where oral examination has occurred, ensure that this is acknowledged in writing (e.g. FT001 and Assessor Comments)
· All questions must be satisfactorily demonstrated by the Participant for a Satisfactory determination (indicated by an Assessor tick to the right of the question).
· Assessors are to complete marking in pen of a different colour to the Participant.
· If the Participant verbally modifies their response, write in the modified response verbatim and put your initials next to the written change. 




	ASSESSOR COMMENTS

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	




NOTE

At times, you will be provided with a specific business context to which you must respond, otherwise it is anticipated that you will use a workplace of your choosing (your own, or hypothetical) to provide the context to the task.

At all times, the responses in your assessment must reference Australian (Queensland or Federal) documentation, including legislation, regulations, codes of practice, standards and guidance publications.

For the following activities, name the State/Territory you will base your research on. 

	State/ Territory
	Queensland




	ACTIVITY 1  [bookmark: _Ref35349341]

	Research and document your findings regarding legislation and codes that apply in your state/territory relevant to the following three (3) items. Summarise the requirements relevant to building drawings and sketches you identified and provide the URL where you sourced your responses.
a) Smoke alarms in a new building
b) Pool fences
c) Protection of waterways



a) Smoke alarms
	Name of Legislation (Commonwealth or State) 

	AS3786-2014

	Summary of relevant excerpt/requirement 

	Must be photoelectric
Not also contain an ionisation sensor
Be less than 10 years old
Operate when tested
Be inter connected with every smoke alarm in the dwelling so all activate together
They must be installed in each bedroom, in hallways, between bedrooms and other parts of the storey
Smoke alarms must be powered by either hardwired or powered by non removable 10 year battery or a combination of both

	Source (URL or web source)

	Qfes.qld.gov.au



b) Pool fence installation
	Name of Legislation (Commonwealth or State) 

	AS 1926.1-2012

	Summary of relevant excerpt/requirement 

	Not less than 1.2m high
Shield or remove climbable objects within 900mm
Remove climbable objects from the pool barrier and surround
Trim back bushes or branches that can be used to climb on

	Source (URL or web source)

	www.qld.gov.au




c) Protection of waterways
	Name of Legislation (Commonwealth or State)

	Environmental protection(water and wetland biodiversity) policy 2019

	Summary of relevant excerpt/requirement

	Companies need to gain a license before they are allowed to discharge waste water to waterways 

	Source (URL or web source)

	Environment.des.qld.gov.au



	Satisfactory Outcome
	
	




	ACTIVITY 2  [bookmark: _Ref35349352]

	Access Handout 1 (HO1- Floor Plan with dimensions) and respond to the following:
a) What is used for the internal wall lining?
b) What is used for the external cladding?
c) What roofing cladding is required?
d) How do you identify the smoke alarm installation points?



	a) What is used for the internal wall lining?

	Gyprock 

	b) What is used for the external cladding?

	Painted render finish

	c) What roof cladding is required?

	Colorbond custom orb sheeting

	d) How do you identify the smoke alarm installation points?

	By locating the legend which signifies the smoke alarms with an s in a circle




	Satisfactory Outcome
	
	





	ACTIVITY 3  [bookmark: _Ref130909754]

	Access Handout 2 (HO2- Footing Plan) and Handout 3 (HO3- Slab Plan) and respond to the following:
a) Specify the size and type of reinforcing to be used for BP.1 in Handout 2 (HO2-footing plan)
b) How do you determine where each BP.1 footing pier should be placed?
c) Mark each of the load bearing points in Hand out 3 (HO3- Slab Plan)



	a) Specify the size and type of reinforcing to be used for BP.1

	450mm diameter 
Vertical – 5.n12
Ligs R6 helix – 200mm pitch

	b) How do you determine where each BP.1 footing pier should be placed?

	By referring to the footing plan in the left hand top corner

	c) Mark each of the load bearing points in Hand out 3 (HO3- Slab Plan)

	[image: Diagram, engineering drawing

Description automatically generated]




	Satisfactory Outcome
	
	




	ACTIVITY 4  [bookmark: _Ref130974558]

	Access Handout 4 (HO4- Residential Floor Plan) and respond to the following:
a) Which drawings are shown in these plans?
b) Which Australian Standard must be referenced when installing termite protection?
c) Make a list of the finishes noted on the document.




	a) Which drawings are shown in these plans?

	Floor plans and elevations

	b) Which Australian Standard must be referenced when installing termite protection?

	AS 3660 SE

	c) Make a list of the finishes noted on the document.

	Roof – custom orb deep ocean colorbond
Gutter/fascia – deep ocean colorbond
Walls – Dulux cargo river
Corbells – Dulux calf skin
Window frame – Powdercoat  anotech grey
Paving – Lifestyle paving liquid limestone




	Satisfactory Outcome
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PRACTICAL ASSESSMENT


	Participant name
	Michael Trott




	FOR THE PARTICIPANT

	Instructions

	· The tasks outlined on the following pages will require performance of normal workplace activities, as a result of a structured activity set by an Observer in the workplace or a simulated activity set by your Assessor/Observer. 
· The timeframe for these tasks will be established by your Assessor/Observer, in consideration of location conditions and industry requirements.
· You must complete all tasks unassisted by the Assessor or other personnel, unless the steps note this assistance. 
· You must attempt all tasks (and itemised steps) for a ‘Satisfactory’ assessment outcome to be awarded.
· For any observation conducted that is incomplete, or without satisfactory performance, the observation will need to be completed again after further training support.




	FOR THE ASSESSOR/OBSERVER

	Instructions

	· The following observation record should be used to judge and record your observations of the Participant as they complete the task(s) set. You must record your observations of the Participant’s performance. 
· For each occasion, indicate the task performed and whether it was a simulation or workplace-based task. 
· Any simulated assessment must ensure the Participant still performs under workplace conditions which reflect industry standards.
· In the comments, provide clear detail regarding the task that the Participant was required to do (e.g. PPE used, materials handled, attachments connected, plant types).
· All steps must be satisfactorily demonstrated by the Participant for a ‘Satisfactory’ determination (indicated by an Assessor tick to the right of each itemised step, or an Observer tick to the right of each itemised step, and confirmation by an Assessor in the Assessor Comments).
· Where you have determined that one or more task steps have not been satisfactorily demonstrated, provide the Participant with additional support and outline details of such assistance in the Assessor/Observer Comments. Allow the Participant two (2) further opportunities to demonstrate the task again to allow an opportunity for a ‘Satisfactory’ assessment outcome to be achieved. 
· If after three (3) attempts the Assessor determines that the Participant cannot demonstrate the required steps, a ‘Not Satisfactory’ outcome is to be determined.





	TASK OUTCOME

	Task
	Date
	Task Type (Tick)
	Location
	Task outcome (Tick)

	
	
	
	
	Satisfactory
	Not Satisfactory

	Task 1
	6/11/2023
	 Workplace
 Simulation
	Office
	
	



	ASSESSOR COMMENTS: GENERAL

	As necessary, outline:
· Details on reattempts, alternative arrangements or reasonable adjustments made.
· Where a Participant is deemed ‘Not Satisfactory’, provide recommendations for future training.

	




	ASSESSOR COMMENTS: PRACTICAL TASK 1: OCCASION 1

	 Individual student (as named on cover page)
 Multiple students [ All from Attendance Report,  Specific students involved – identify students]

	Task
	Provide detail 

	1.1A. 1.1B. 
	Specify type of plan and NCC class determined: 
Michael determined it was a class 6 building being that of a building which sells goods or supplies and service to the public

	1.1A. 1.1C. 
	Specify how currency of documents was confirmed:
Michael referred to the title block

	1.1D. 
	Specify environmental controls determined from plans/specifications.
Michael  determined the building was in Queensland therefore all works are guided within the environmental protection act 1994

	1.2B. 1.2C. 
	Specify how building layout, material requirements spaces and dimensions were determined from plans and specifications.
Michael confirmed the layout of concrete footings pillars by identifying them using the footing plans
Michael determined the size and dimensions of the deck by using a scale rule at 1:100.
Michael noted the deck would be a timber deck (merbau) and the surrounding screening would be black powder coated aluminium 65mm wide

	1.2G. 
	Specify services identified on site:
Michael identified the underground stormwater, underground electrical cables from the sub floor plans

	1.2H. 
	Specify site features located to be removed/ retained:
Michael identified the tiled surface that is to be removed in preparation for new flooring/deck

	1.2J. 
	Specify variations found:
Michael located the adding of a shade sail over the deck as a variation

	1.3A. 
	Specify concrete footing and slab information identified:
Michael identified that the footing would be 4500 bored piers with minimum 40mpa compressive strength concrete from the footings plan

	1.3B. 
	Specify how load bearing points were recognised:
Michael located the load bearing points with the help of the footing plan

	1.3C. 
	Specify how wind bracing and tie down requirements were confirmed:
These were confirmed in the footing section plans in a typical cross bracing detail (BR1)g

	1.4B. 1.4C. 
	Specify how installation points and fixtures were determined:
Michael determined these from studying the utilities and services plans

	1.4B. 
	Specify how connection points were determined:
Michael determined these from the site plans

	1.4C. 
	Specify where finishing details were located:
Michael located these in finishes legend on the finishes plan
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	Practical Task 1 

	Description of task:
The participant must demonstrate skills and knowledge to identify and interpret building and construction information from plans and specifications in a workplace (or a similar environment) in the context of a construction project including:
· Identify types of plans.
· Check and confirm that the current version of plans, specifications and amendments is being used.
· Use the appropriate plans and aspects of drawings for relevant purposes.
· Confirm that the details on plans comply with the specifications.
· Identify environmental controls from plans/specifications.
· Read and interpret the plans.
· Read and confirm standards of work and tolerances from job specifications.
· Determine building layout, spaces and dimensions from floor plan.
· Determine material sizes, thickness and construction methods from detail drawings for estimates. (Template available for use HO5_ Cost Estimation)
· Recognise and confirm job specifications located in drawings, notes, and descriptions.
· Determine internal linings, external cladding and roof materials needed for estimates from plans and specifications. .(Template available for use HO5_ Cost Estimation)
· Apply information from plans to estimation, planning and supervisory tasks.(Template available for use HO5_ Cost Estimation)
· Gain access to the site, achieve orientation and identify services, datum and reduced levels.
· Locate site features to be removed or retained.
· Determine the building location from the site plans to actual.
· Verify plans recognising variations between the plans and the actual site, reporting findings as required.
· Appropriately communicate with others to be understood.
· Adhere to site safety requirements, including requirements relating to hazard identification.
· Identify structural details.
· Identify concrete footing and slab sizes and position and type of reinforcing required.
· Identify structural load bearing points of the building and compare information from specification.
· Identify wind bracing and tie-down requirements checking for accuracy against the wind bracing table.
· Identify non-structural details.
· Identify provisional sum (PS) and prime cost (PC) items when estimating costs.(Template available for use HO5_ Cost Estimation)
· Locate installation and connection points of services to the building.
· Identify location of fixtures from plans and details of finishes from specifications.

These tasks may be simulated or real. The Participant is to gather evidence of how they have completed each component of the Practical Task, which is to be submitted with this Practical Assessment sheet. The Observer is to provide detailed comments on the tasks completed by the Participant (on the Observer Comments, overleaf). The Assessor is to verify the Observer’s comments, noting their findings in the Assessor Comments (on the back of the Practical Assessment cover page) and provide the assessment outcome.

	Resources required: 
Work site; plans and specifications, quality documentation; access to the internet/access legislation, current building and construction codes and standards and the NCC. PC applications and software to access CAD. Templates for estimating.

	Observer details

	Name of observer:
	Bruce Davie

	Role of observer 
(Confirm suitability to sign)
	General Manager

	Email address of observer
	bdavie@core4service.com

	Signature of observer:
	
	Date:
	6/11/2023



	When completing the task, did the Participant:
	Tick if satisfactorily completed. 
Provide comments if left unticked.

	1 Identify types of plans

	[bookmark: _Ref130979481]Check and confirm that the current version of plans, specifications and amendments is being used.
	
	[bookmark: _Ref130979484]Use the appropriate plans and aspects of drawings for relevant purposes.
	
	[bookmark: _Ref130979803]Confirm that the details on plans comply with the specifications.
	
	[bookmark: _Ref130979521]Identify environmental controls from plans/specifications.
	
	2 Read and interpret the plan

	[bookmark: _Ref130984040]Read and confirm standards of work and tolerances from job specifications.
	
	[bookmark: _Ref130980146]Determine building layout, spaces and dimensions from floor plan.
	
	[bookmark: _Ref130980150][bookmark: _Ref130984245]Determine material sizes, thickness and construction methods from detail drawings.(Template available for use HO5_ Cost Estimation)
	
	[bookmark: _Ref130980260]Recognise and confirm job specifications located in drawings, notes, and descriptions.
	
	[bookmark: _Ref130984259]Determine internal linings, external cladding and roof materials from plans and specifications. (Template available for use HO5_ Cost Estimation)
	
	[bookmark: _Ref130984400]Apply information from plans to estimation, planning and supervisory tasks.(Template available for use HO5_ Cost Estimation)
	
	[bookmark: _Ref130982305]Gain access to the site, achieve orientation and identify services, datum and reduced levels.
	
	[bookmark: _Ref130982340]Locate site features to be removed or retained.
	
	[bookmark: _Ref130982465]Determine the building location from the site plans to actual.
	
	[bookmark: _Ref130982550]Verify plans recognising variations between the plans and the actual site, reporting findings as required.
	
	[bookmark: _Ref130984197]Appropriately communicate with others to be understood.
	
	[bookmark: _Ref130984226]Adhere to site safety requirements, including requirements relating to hazard identification.
	
	3 Identify structural details

	[bookmark: _Ref130983367]Identify concrete footing and slab sizes and position and type of reinforcing required.
	
	[bookmark: _Ref130983503]Identify structural load bearing points of the building and compare information from specification.
	
	[bookmark: _Ref130983514]Identify wind bracing and tie-down requirements checking for accuracy against the wind bracing table.
	
	4 Identify non-structural details

	[bookmark: _Ref130984299]Identify provisional sum (PS) and prime cost (PC) items when estimating costs.
	
	[bookmark: _Ref130983670]Locate installation and connection points of services to the building.
	
	[bookmark: _Ref130983805]Identify location of fixtures from plans and details of finishes from specifications.
	




	Observer comments:

	Michael demonstrated a proficient ability to identify and interpret building and construction information from plans and specifications in a workplace setting. Michael’s skill in reading and interpreting various types of plans, including structural and non-structural details, was notable. He exhibited a strong grasp of the key components essential for accurate estimation in the context of a construction project.

1.4A Not applicable to job as was a fixed contract
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