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	Project Name
	QTMP Torbanlea

	[bookmark: _gjdgxs]Scope of Work
	Site Establishment Works

	Site Address
	Ritchie Rd Torbanlea

	Date of Inspection
	07/07/2024
	Inspected By
	Mick Franz

	Site Contact/s
	Mick Franz

	Inspection Summary
	
Excavation - Trenching



	Corrective Action Reference



	Barricading left down Around Open Trench








	Ref
	Criteria
	Observations

	
	
	
Yes
	
No
	
N/A
	
Comments

	1
	All workers carrying out work have received the general construction induction training. (Blue/White Card)

Work Health and Safety Regulation 2011 s316
	YES
	
	
	

	2
	PPE is:
· suitable for the relevant hazards
· of suitable size and fit
· maintained such that it is clean and hygienic and in good working order.
· 
Work Health and Safety Regulation 2011 s.44
	YES
	
	
	PPE Stored and Maintained Correctly
Gloves worn at all times as per JHG Instruction

	3
	A safe work method statement (SWMS) has been prepared for each high-risk construction work activity that is underway or about to commence and is Current Revision.

Work Health and Safety Regulation 2011 s.299(1)
	YES
	
	
	SWMS AVAILABLE IN SITE OFFICE 
SWMS CAPTURED ON START CARDS FOR RELEVANT TASKS

	4
	The work environment has been maintained such that it is clean and in a safe condition.

Managing the Work Environment and Facilities Code of Practice, 1.3 Maintaining the work environment and facilities.
	YES
	


	
	ACCESS AND EGRESS CLEARLY SIGNED AND KEPT CLEAR
SUFFICIENT BINS PROVIDED TO MAINTAIN HOUSEKEEPING


	5
	Work areas are clearly identified and separated as necessary so that work can be undertaken safely.

Work Health and Safety Regulation 2011 s.40
	Yes
	
	
	CROWD BARRIERS AND SIGNAGE USED TO DELINEATE WORK AREAS
SPOTTERS USED WELL IN CONTROLLING WORK AREAS

OPEN TRENCHES TO HAVE BARRICADING INSTALL AT ALL TIMES WITH SIGNAGE 

	6
	Lighting at the workplace is sufficient to allow:
· each worker to carry out work without risk to health and safety
· people to move within the workplace without risk to health and safety
· safe evacuation in an emergency.

Work Health and Safety Regulation 2011 s.40
Managing the Work Environment and Facilities Code of Practice, 2.6 Lighting
	YES
	
	
	SUFFICIENT LUX LEVELS PROVIDED THROUGHOUT SITE

	7
	Adequate facilities have been provided for workers, including toilets, drinking water, washing facilities, and eating facilities.

Work Health and Safety Regulation 2011 s.41
	YES
	
	
	FACILITIES MAINTAINED WELL

	8
	Facilities provided for workers are in good working order and are clean, safe, and accessible.

Work Health and Safety Regulation 2011 s.41
	YES
	
	
	ALL SITE FACILITIES CLEANED REGULARLY

	9
	First aid equipment has been provided for the workplace and is accessible to each worker.

Work Health and Safety Regulation 2011 s.42
	YES
	
	
	FULLY STOCKED FIRST AID ROOM 

	10
	Electrical leads are arranged to avoid damage.

Electrical Safety Regulation 2013 s.102
	YES
	
	
	LEAD STANDS USED WELL
COMMUNICATION WITH ALL TRADES TO UTILISE TIE RAILS WHEN CONNECTING LEADS TO TEMP BOARD POWER SUPPLIES
NOTED ON OCCASIONS SUMO LEADS HAVE BEEN MOVED BY OTHERS AFTER INSTALLATION COMPLETED BY SITE ELECTRICIANS 

	11
	Electrical equipment has been inspected, testing, and tagged in accordance with AS/NZS 3012 Electrical installations – Construction and demolition sites.
	YES
	
	
	3 MONTHLY TEST AND TAG DUE 1/10/2024

	12
	The risks to health and safety associated with any hazardous manual tasks have been identified and managed.

Work Health and Safety Regulation 2011 s.60
	YES
	
	
	CRANE AND FORKLIFT AVAILABLE FOR LOADING AND UNLOADING 

	13
	A safety data sheet (SDS) exists and is available for inspection for each hazardous chemical used, handled, or stored at the workplace.

Work Health and Safety Regulation 2011 s.344
	YES
	
	
	SDS AVAILABLE IN FIRST AID OFFICE
SDS RECORDS UPDATED
HAZARDOUS CHEMICALS STORED IN CORRECT CONTAINERS 

	Environmental 

	14
	Are controls for air pollution adequate?
	YES
	
	
	ONGOING MONITORING CONDUCTED DAILY

	15
	Are controls for water pollution adequate? 
	YES
	
	
	

	16
	Are controls for noise control adequate?
	YES
	
	
	ONGOING MONITORING CONDUCTED DAILY

	17
	Are controls for waste management adequate?
	YES
	
	
	BINS EMPTIED DAILY 

	18
	Are controls for the protection of Flora, Fauna and Historical Heritage adequate?
	YES
	
	
	

	Legal

	19
	Have there been any HSEQ breaches, incidents or near misses?
	
	NO
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