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	Record number
	Date of entry
	Hazard
	Location
	People exposed
	Possible injuries/ damage
	Control measures
	Risk assessment

	1
	16/12/20
	Faulty electronic equipment causing a fire in the workplace
	Can occur in any section of the manufacturing shed
	All workers in the affected area
	Burns, smoke inhalation, death, fire damage to workplace 
	All equipment and machine to tagged and tested, training regarding checking cords before use and warning signs 
	High

	2
	16/12/20
	Spraying mentholated spirits onto glass to break laminate layer near hot lamp that is also used to break laminate barrier
	Cutting table in the right corner at the back of the shed
	Workers operating machine and other staff walking past area
	Burns from chemical if ignited by hot lamp inside machine
	Stopping use of metho when the lamp is in use and the bottle containing metho has a new lid so it can be used just at the source
	High

	3
	16/12/20
	Flammable chemical storage cabinet mixed with an ignition source 
	Next LISEC glass cutting machine 
	Workers operating LISEC cutting machine and affected workers traveling to staff room
	Burns, smoke inhalation, death, fire damage to workplace and poisonous fumes
	Store all chemicals in a class 3 dangerous chemicals cabinet and move cabinet further away from the glass cutting machine and walking traffics in the workplace
	High

	4
	16/12/20
	Grinding metal glass storage frames, causing sparks which can cause a fire in the workplace
	Left side of the manufacturing 
	The one worker disassembling the glass storage frames 
	Burns, smoke inhalation, death and fire damage to workplace
	Create a designated idea out doors for the grinding to take place away from any sources of ignition.
	High

	5
	16/12/20
	[bookmark: _GoBack]Cigarette buts being thrown into the large bin
	The large dumpster type bin outside in front of the manufacturing shed 
	Workers, customers and visitors arriving and leaving the workplace
	Burns, smoke inhalation, death and fire damage to workplace
	Create signs to warn against throwing buts into bin, training given to worker regarding the issues and ensure designated smoking areas with ashtrays are labelled.
	High


RISK REGISTER

RISK MATRIX
	Matrix
	A:
Death or permanent disability
	B:
Serious injury
	C:
Lost time injury
	D:
Casualty Treatment
	E:
First Aid

	1: Very Likely
	E
	E
	H
	H
	M

	2: Likely
	E
	H
	H
	M
	M

	3: Possible
	H
	H
	M
	M
	L

	4: Unlikely
	H
	M
	M
	L
	L

	5: Very Unlikely
	M
	M
	L
	L
	L



	E: Extreme
	H: High
	M: Medium
	L: Low
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